


                                     +
                                   + + +
                                   + + +
                                   + + +
                             +     + + +     +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                     +     + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                     +       +     + + +     +       +
                                   + + +
                                   + + +
                                   + + +
 ASPENTECH                         + + +
                                   + + +
 FLOWSHEET SIMULATION              + + +
 FOR THE PROCESS INDUSTRIES        + + +
                                     +


                                                                        TM
 AAAAA   SSSSS   PPPPP   EEEEE   NN    N   PPPPP   L       U   U   SSSSS
 A   A   S       P   P   E       N N   N   P   P   L       U   U   S    
 AAAAA   SSSSS   PPPPP   EEEEE   N   N N   PPPPP   L       U   U   SSSSS
 A   A       S   P       E       N    NN   P       L       U   U       S
 A   A   SSSSS   P       EEEEE   N     N   P       LLLLL   UUUUU   SSSSS

 ASPEN PLUS IS A TRADEMARK OF           HOTLINE:
 ASPEN TECHNOLOGY, INC.                 U.S.A. 888/996-7001
 TEN CANAL PARK                         EUROPE (32) 2/724-0100
 CAMBRIDGE, MASSACHUSETTS 02141                             
 617/949-1000

 PLATFORM: WIN32                                         OCTOBER 6, 2016     
 VERSION: 11.1   Build 192                               THURSDAY    
 INSTALLATION: TEAM_EAT                                  7:51:55 A.M.        

 THIS COPY OF ASPEN PLUS LICENSED TO                                 


      ASPEN PLUS (R) IS A PROPRIETARY PRODUCT OF ASPEN TECHNOLOGY, INC.
      (ASPENTECH), AND MAY BE USED ONLY UNDER AGREEMENT WITH ASPENTECH.
      RESTRICTED RIGHTS LEGEND:  USE, REPRODUCTION, OR DISCLOSURE BY THE
      U.S. GOVERNMENT IS SUBJECT TO RESTRICTIONS SET FORTH IN 
      (i) FAR 52.227-14, Alt. III, (ii) FAR 52.227-19, (iii) DFARS 
      252.227-7013(c)(1)(ii), or (iv) THE ACCOMPANYING LICENSE AGREEMENT,
      AS APPLICABLE. FOR PURPOSES OF THE FAR, THIS SOFTWARE SHALL BE DEEMED
      TO BE "UNPUBLISHED" AND LICENSED WITH DISCLOSURE PROHIBITIONS.
      CONTRACTOR/SUBCONTRACTOR: ASPEN TECHNOLOGY, INC. TEN CANAL PARK,
      CAMBRIDGE, MA 02141.
 *** INPUT SUMMARY ***

 >>CURRENT RUN

   ORIGINAL RUN                           OCTOBER 6, 2016     
   7:51:55 A.M.                           THURSDAY    
   INPUT FILE: _4535fpg.inm                                                                    
   RUN ID : _4535fpg
     1    ;
     2    ;Input file created by Aspen Plus Rel. 11.1 at 07:51:55 Thu Oct 6, 2016
     3    ;Directory C:\Program Files (x86)\AspenTech\Working Folders\Aspen Plus 11.1  Runid _UNNAMED
     4    ;
     5
     6
     7
     8    TITLE 'Tutorial'
     9
    10    IN-UNITS ENG
    11
    12    DEF-STREAMS CONVEN ALL
    13
    14    ACCOUNT-INFO ACCOUNT=1 PROJECT-ID=1  &
    15            PROJECT-NAME="HOS3124@GMAIL.COM"  &
    16            USER-NAME="HOSSEIN KHAKPOUR"
    17
    18    DESCRIPTION "
    19        General Simulation with English Units :
    20        F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr.
    21
    22        Property Method: None
    23
    24        Flow basis for input: Mole
    25
    26        Stream report composition: Mole flow
    27        "
    28
    29    DATABANKS PURE11  / AQUEOUS  / SOLIDS  / INORGANIC  /  &
    30            NOASPENPCD
    31
    32    PROP-SOURCES PURE11  / AQUEOUS  / SOLIDS  / INORGANIC
    33
    34    COMPONENTS
    35        WATER H2O /
    36        ACETONE C3H6O-1 /
    37        MIBK C6H12O-2
    38
    39    FLOWSHEET
    40        BLOCK MIXER IN=FEED MIBK OUT=PRUDUCT
    41
    42    PROPERTIES IDEAL
    43
    44    STREAM FEED
    45        SUBSTREAM MIXED TEMP=75. PRES=50. MASS-FLOW=100.
    46        MASS-FRAC WATER 0.5 / ACETONE 0.5
    47
    48    STREAM MIBK
    49        SUBSTREAM MIXED TEMP=75. PRES=50. MASS-FLOW=100.
    50        MOLE-FLOW MIBK 1.
    51
    52    BLOCK MIXER MIXER
    53        PARAM NPHASE=1 PHASE=L
    54        BLOCK-OPTION FREE-WATER=NO
    55
    56    EO-CONV-OPTI
    57    ;
    58    ;
    59    ;
    60    ;
    61    ;
 *** INPUT TRANSLATOR MESSAGES ***


  *   WARNING IN THE "STREAM" PARAGRAPH WHICH BEGINS ON LINE 48                 
      STREAM NAME: MIBK                                        (STSTRM.28)      
      COMPONENT MOLE FLOWS OF SUBSTREAM: "MIXED"                                
      ARE NORMALIZED TO THE TOTAL MOLE FLOW VALUE.                              
 
 

 PDF updated                                                                      TIME =      0.15

 *** CALCULATION TRACE ***

 TUTORIAL                                                        

 *** FLOWSHEET ANALYSIS MESSAGES ***

 FLOWSHEET CONNECTIVITY BY STREAMS       

   STREAM     SOURCE     DEST           STREAM     SOURCE     DEST
   MIBK       ----       MIXER          FEED       ----       MIXER   
   PRUDUCT    MIXER      ----                                         

 FLOWSHEET CONNECTIVITY BY BLOCKS        

   BLOCK        INLETS                         OUTLETS
   MIXER        FEED MIBK                      PRUDUCT                     

      COMPUTATION ORDER FOR THE FLOWSHEET IS:
      MIXER 

Calculations begin                                                              time      0.04


 SIMULATION CALCULATIONS BEGIN                                                    TIME =      0.04

      ENTHALPY CALCULATION FOR INLET STREAM FEED OF BLOCK MIXER                   TIME =      0.04
      KODE = 2  NTRIAL =   1  T =   297.04  P =  0.3447E+06  V =  0.0000E+00  Q =  0.0000E+00

      ENTHALPY CALCULATION FOR INLET STREAM MIBK OF BLOCK MIXER                   TIME =      0.05
      KODE = 2  NTRIAL =   1  T =   297.04  P =  0.3447E+06  V =  0.0000E+00  Q =  0.0000E+00

      UOS BLOCK MIXER    MODEL: MIXER                                             TIME =      0.05
      KODE = 1   NO. TEMP ITER =    4     TEMP =   297.04    
      KPHASE =    2 KODE =    1 T =   297.04     P =  0.34474E+06 Q =  0.00000E+00

 Report Writer entered                                                            Time =     57.03

 Results generated                                                                Time =     57.04

 Report Writer entered                                                            Time =     57.08

 Results generated                                                                Time =     57.09

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED

 *** CALCULATION TRACE ***

 TUTORIAL                                                        



*** INPUT SPECIFICATION MESSAGES ***

 STREAM-REPOR IS  NEW 12/08/2016   10:25:45:10 
 STREAM-REPOR MOLEFLOW MASSFRAC

 PDF updated                                                                      TIME =    992.92
 THIS COPY OF ASPEN PLUS LICENSED TO                                 
 
 

Calculations begin                                                              time    994.95


 Report Writer entered                                                            Time =   1092.74

 Results generated                                                                Time =   1092.75

 Report Writer entered                                                            Time =   1092.76

 Results generated                                                                Time =   1092.77

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED
