MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Thu Dec 08 13:13:34 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
RGIBBS
RGibbs
Built-In
RGIBBS
? SETUP MAIN ? \ TITLE TITLE = "GIBBS" \ \ SIMULATE INTERACTIVE = NO MOLEFRAC
 = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? SETUP GLOBAL ? \ "IN-UNITS" 
INSET = MET \ \ "STREAM-CLASS" SCLASS = CONVEN \ ? SETUP DIAGNOSTICS ? ? 
SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" METCBAR ? \ 
DESCRIPTION DESCRIPTION = "Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ 
MMLOCAL \ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 
4 3 3 3 3 1 3 3 3 4 3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 
3 3 3 4 3 3 3 3 3 3 3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ 
DESCRIPTION DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" 
\ \ MMLOCAL \ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 
8 3 4 3 3 3 3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 
3 3 3 3 3 4 3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? 
\ DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" 
\ \ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 
5 1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "SYS-OPTIONS" ? ? SETUP 
"ACCOUNT-INFO" ? \ ACCOUNT USER-NAME = "GIBBS" \ ? SETUP "RUN-CONTROL" ? ? 
SETUP DESCRIPTION ? \ DESCRIP DESCRIP = ( 
"General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = CO ANAME = CO OUTNAME = CO TYPE = CONV 
DBNAME1 = "CARBON-MONOXIDE" ANAME1 = "CO" /  CID = CO2 ANAME = CO2 OUTNAME = 
CO2 TYPE = CONV DBNAME1 = "CARBON-DIOXIDE" ANAME1 = "CO2" /  CID = H2 ANAME
 = H2 OUTNAME = H2 TYPE = CONV DBNAME1 = "HYDROGEN" ANAME1 = "H2" /  CID = 
H2O ANAME = H2O OUTNAME = H2O TYPE = CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  
CID = CH4 ANAME = CH4 OUTNAME = CH4 TYPE = CONV DBNAME1 = "METHANE" ANAME1 = 
"CH4" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET GLOBAL ? \ 
BLOCK BLKID = RGIBBS BLKTYPE = RGIBBS IN = ( FEED M0-1 ) OUT = ( PRODUCT M0-1 
) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? PROPERTIES MAIN ? \ GPROPERTIES 
GBASEOPSET = NRTL GOPSETNAME = NRTL PARCON = -1 \ ? PROPERTIES "OPTION-SETS" 
NRTL ? \ PARAM BASE = NRTL \ ? PROPERTIES "MOLEC-STRUCT" CH4 ? ? PROPERTIES 
"MOLEC-STRUCT" CO ? ? PROPERTIES "MOLEC-STRUCT" CO2 ? ? PROPERTIES 
"MOLEC-STRUCT" H2 ? ? PROPERTIES "MOLEC-STRUCT" H2O ? ? PROPERTIES PARAMETERS 
BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = RKTKIJ 
SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDKIJ-1" 
? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ SETNO = 1 UNITROW = 0 
TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDMIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL = psi TUNITROW = 22 
TUNITLABEL = F BDBANK = ( BINARY HENRY ) NEL = 6 \ ? PROPERTIES PARAMETERS 
BINARY "T-DEPENDENT" "NRTL-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = NRTL 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F BDBANK = ( "VLE-IG" 
"LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; 
\ P1 ID = MASSVFRA \ \ P1 ID = MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX 
UNITS = ( "J/kg" ) \ \ P1 ID = RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX 
UNITS = ( "J/kg-K" ) \ \ P1 ID = PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX 
UNITS = ( "N-sec/sqm" ) \ \ P1 ID = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = 
SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID = MWMX \ \ P2 PHASE = ( T V L ) \ \ 
DESCRIPTION DESCRIPTION = "Thermal and Transport, for heat exchanger design" 
\ ? "PROP-SET" MAIN THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" 
) \ \ P1 ID = CPMX UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = 
MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 300. <22> <1> 
PRES = 470. <20> <3> BASIS = "MOLE-FRAC" TOTFLOW = 1000. <-89> <3> TOTAL = 1. 
<-89> <0> JUNK = 5 \ \ MOLE-FLOW SSID1 = MIXED CID = CO FLOW = 0.2368 <-4> 
<0> /  SSID1 = MIXED CID = CO2 FLOW = 0.0361 <-4> <0> /  SSID1 = MIXED CID = 
H2 FLOW = 0.7172 <-4> <0> /  SSID1 = MIXED CID = H2O FLOW = 0.0001 <-4> <0> 
/  SSID1 = MIXED CID = CH4 FLOW = 0.0098 <-4> <0> \ ? BLOCK RGIBBS RGIBBS ? ; 
"MET_MOLE" ; ; ICON2 ; \ PARAM TEMP = 300. <22> <1> PRES = 470. <20> <3> \ ? 
"EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = SIMULATION 
\ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE = 
RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L = 
DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFRAC = MOLEFRAC \ ? REPORT 
"FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT "ADA-REPORT" ? ? REPORT 
"BATCH-OPERAT" ? ; "ENG_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6375
browserwidth 10335
browsertreewidth 3525
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 4
SIZE -4.07647 1.98597 -0.978402 1.4
BLOCK
ID: RGIBBS
Version: 1
ICON: "ICON2"
Flag 0
Section GLOBAL
At -0.895928 0.104525
Label At -0.057662 0.717763
Scale 1.804878 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
TYPE 0 TERMINAL 1
At -4.001810 0.701810
Label At 1.276809 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -4.001810 0.701810
x x -2.725000 0.701810
y y -2.725000 0.645703
x x -1.635922 0.645703
t l -1.435922 0.645703
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: PRODUCT
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At 1.911312 0.701810
Label At -1.136312 0.000000
ROUTE 0 0
r l 1.911312 0.701810
x y 0.775000 0.701810
y x 0.775000 0.645703
x 0 -0.157072 0.645703
t r -0.357072 0.645703
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.85249 -3.2 -3.1 -3.3448
Size: 0.0149321
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -9.392307 9.392307 3.300000 -3.300000
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.014932

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "FaraDars" "FARADARS_PC"
 )                                                                              
 DSET RUN-STATUS IT @IT ( "DECEMBER 8, 2016    1:10:47 P.M." "_4753yxm.inm" 0)  
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (CO CO2 H2 H2O CH4)                                  
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_4753yxm")                                      
 DSET RUN-STATUS RUNID @RUNID ("_4753yxm")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "DECEMBER 8, 2016 1:10:47 P.M." )                     
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "GIBBS" )                                       
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (* * * "GIBBS" )                              
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (2.80104000D+01 4.40098000D+01 2.01588000D+00 1.80152800D+01    
 1.60427600D+01)                                                                
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (5.35578000D+01 <3> 5.35578000D+01 <3> 5.35578000D+01 <3>    
 1.80500000D+01 <3> 5.35578000D+01 <3> )                                        
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (8.17000000D+01 <1> 1.94700000D+02 <1> 2.03900000D+01 <1>       
 3.73150000D+02 <1> 1.11660000D+02 <1> )                                        
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (2.36800000D+02 <3> 1.69991905D+00 <3> 7.17199676D+02 <3>  
 -2.40199838D+02 <3> -2.38499919D+02 <3> 1.00000000D+00 4.70891705D-02          
 9.99999549D-01 -9.99583853D-01 -9.60531602D-01 4.76999838D+02 <3>              
 -5.68434189D-17 -8.54925020D-11 <3> -8.70026397D-15 3.25308551D+06 <3>         
 5.44110055D-01)                                                                
 DSET ALIAS @ALIAS ( "CO" "CO2" "H2" "H2O" "CH4" )                              
 IDSET ID_21 (NPOINT) (#5)                                                      
 IDSET ID_22 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)               
 LSET L_6 (%ID_22 & %ID_21)                                                     
 DSET COMPONENTS MAIN COMPS @L_6 ("CO" C "CO" "CO" "CO" "CO2" C "CO2" "CO2"     
 "CO2" "H2" C "H2" "H2" "H2" "H2O" C "H2O" "H2O" "H2O" "CH4" C "CH4" "CH4" "CH4"
 )                                                                              
 IDSET ID_23 (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 145 *1 137 *1   
 1052 *2 <13> )                                                                 
 LSET L_7 (%ID_RXBAL %ID_23)                                                    
 DSET BLOCK RGIBBS RGIBBS BLKSTAT @BLKSTAT (0 0)                                
 DSET BLOCK RGIBBS RGIBBS COMPSTAT @L1 (0)                                      
 DSET BLOCK RGIBBS RGIBBS BLKIN @BLKIN (1 FEED)                                 
 DSET BLOCK RGIBBS RGIBBS TYPIN @TYPIN (1 MATERIAL)                             
 DSET BLOCK RGIBBS RGIBBS BLKOUT @BLKOUT (1 PRODUCT)                            
 DSET BLOCK RGIBBS RGIBBS TYPOUT @TYPOUT (1 MATERIAL)                           
 DSET BLOCK RGIBBS RGIBBS RES_Q @L_7 (1.00000000D+03 <3> 5.23000162D+02 <3>     
 -4.76999838D+02 <3> -1.70530257D-16 9.82642621D+03 <3> 9.82642621D+03 <3> * <3>
 -9.07048797D-15 * <3> * <3> * <3> * 1.00000000D+03 <3> 5.23000162D+02 <3>      
 -4.76999838D+02 <3> -1.70530257D-16 9.82642621D+03 <3> 9.82642621D+03 <3> * <3>
 -9.07048797D-15 -2.72564156D+06 <3> -5.97872707D+06 <3> * <3> 5.44110055D-01   
 -3.25308551D+06 <3> 3.00000000D+02 <1> 4.70000000D+02 <3> 1.00000000D+00 1 0   
 -3.25308551D+06 <3> )                                                          
 IDSET ID_24 (ATOM_NUM) (H C O)                                                 
 IDSET ID_25 (COMPONENTS) (CO CO2 H2 H2O CH4)                                   
 IDSET ID_26 (PROPERTIES) (147 *2)                                              
 LSET L_8 (( %ID_26 & %ID_24) & %ID_25)                                         
 DSET BLOCK RGIBBS RGIBBS RGIB_ATM @L_8 ( 0.D0 1.00000000D+00 1.00000000D+00    
 0.D0 1.00000000D+00 2.00000000D+00 2.00000000D+00 0.D0 0.D0 2.00000000D+00     
 0.D0 1.00000000D+00 4.00000000D+00 1.00000000D+00 0.D0 )                       
 IDSET ID_27 (PHASE) (VAPOR)                                                    
 IDSET ID_28 (PROPERTIES) (133 *5)                                              
 IDSET ID_29 (PROPERTIES) (139 *2)                                              
 IDSET ID_30 (PROPERTIES) (140 *5)                                              
 IDSET ID_31 (COMPONENTS) (CO H2 CH4 H2O CO2)                                   
 IDSET ID_32 (PROPERTIES) (8002 *2)                                             
 IDSET ID_33 (PROPERTIES) (8001 *2 <11> )                                       
 LSET L_9 (( %ID_28 %ID_29 %ID_30 ( %ID_31 & %ID_32) %ID_33 ) & %ID_27)         
 DSET BLOCK RGIBBS RGIBBS RGIB_TAB @L_9 ( VAPOR 1.00000000D+00 PRODUCT          
 9.46661522D-13 6.19093975D-07 4.74760693D-01 4.59464175D-01 6.57745130D-02     
 5.23000162D+02 <3> )                                                           
 IDSET ID_34 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )     
 LSET L_10 ( %ID_34 )                                                           
 IDSET ID_35 (PROPERTIES) (253 *2)                                              
 IDSET ID_36 (PROPERTIES) (253 *2 <11> )                                        
 IDSET ID_37 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_38 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_39 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_40 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_41 (PROPERTIES) (8101 *2 <11> 8002 *2 )                               
 IDSET ID_42 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_11 ( %ISODES (( %ID_NCC & %ID_41 %ID_42) & %IDS_1) )                    
 DSET STREAM MATERIAL FEED STR_MAIN @L_11 (* RGIBBS MIXED 2.36800000D+02 <3>    
 3.61000000D+01 <3> 7.17200000D+02 <3> 1.00000000D-01 <3> 9.80000000D+00 <3>    
 2.36800000D-01 3.61000000D-02 7.17200000D-01 1.00000000D-04 9.80000000D-03     
 1.00000000D+03 <3> 9.82642621D+03 <3> 8.72900004D+02 <3> 3.00000000D+02 <1>    
 4.70000000D+02 <3> 9.99903959D-01 9.60407040D-05 0.D0 -9.81230953D+03 <3>      
 -9.98563396D+02 <3> -2.72564156D+06 <3> -5.81143549D+00 <3> -5.91408857D-01 <3>
 1.90934430D-02 <3> 1.87620309D-01 <3> 9.82642621D+00 8.92570810D+02 <3> )      
 DSET STREAM MATERIAL FEED RES_STR @L_10 (3.00000000D+02 <1> 4.70000000D+02 <3> 
 9.82642621D+03 <3> 8.72900004D+02 <3> 1.00000000D+03 <3> 9.99903959D-01 )      
 DSET STREAM MATERIAL PRODUCT STR_MAIN @L_11 (RGIBBS * VAPOR 4.95104129D-10 <3> 
 3.44000809D+01 <3> 3.23786249D-04 <3> 2.40299838D+02 <3> 2.48299919D+02 <3>    
 9.46661522D-13 6.57745130D-02 6.19093975D-07 4.59464175D-01 4.74760693D-01     
 5.23000162D+02 <3> 9.82642621D+03 <3> 4.56546071D+02 <3> 3.00000000D+02 <1>    
 4.70000000D+02 <3> 1.00000000D+00 0.D0 0.D0 -4.11537488D+04 <3>                
 -2.19036065D+03 <3> -5.97872707D+06 <3> -2.43608357D+01 <3> -1.29657729D+00 <3>
 1.90926389D-02 <3> 3.58723420D-01 <3> 1.87885720D+01 3.24636987D+02 <3> )      
 DSET STREAM MATERIAL PRODUCT RES_STR @L_10 (3.00000000D+02 <1> 4.70000000D+02  
 <3> 9.82642621D+03 <3> 4.56546071D+02 <3> 5.23000162D+02 <3> 1.00000000D+00 )  
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
