MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Thu Dec 08 10:08:38 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
HEATEX
HeatX
Built-In
HEATX
? SETUP MAIN ? \ TITLE TITLE = "heat exchanger" \ \ SIMULATE INTERACTIVE = NO 
MOLEFRAC = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? SETUP GLOBAL ? \ 
"IN-UNITS" INSET = MET \ \ "STREAM-CLASS" SCLASS = CONVEN \ ? SETUP 
DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" 
METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT USER-NAME = "HEX" \ ? SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ 
DESCRIP DESCRIP = ( "General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = WT ANAME = H2O OUTNAME = WT TYPE = 
CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  CID = BZ ANAME = C6H6 OUTNAME = BZ 
TYPE = CONV DBNAME1 = "BENZENE" ANAME1 = "C6H6" /  CID = ST ANAME = C8H8 
OUTNAME = ST TYPE = CONV DBNAME1 = "STYRENE" ANAME1 = "C8H8" /  CID = EB 
ANAME = C8H10-4 OUTNAME = EB TYPE = CONV DBNAME1 = "ETHYLBENZENE" ANAME1 = 
"C8H10-4" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET GLOBAL ? 
\ BLOCK BLKID = HEATEX BLKTYPE = HEATX IN = ( "COLD-IN" M1-2 "HOT-IN" M0-1 ) 
OUT = ( "COLD-OUT" M1-2 "HOT-OUT" M0-1 ) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? 
PROPERTIES MAIN ? \ GPROPERTIES GBASEOPSET = NRTL GOPSETNAME = NRTL PARCON = 
-1 \ ? PROPERTIES "OPTION-SETS" NRTL ? \ PARAM BASE = NRTL \ ? PROPERTIES 
"MOLEC-STRUCT" BZ ? ? PROPERTIES "MOLEC-STRUCT" EB ? ? PROPERTIES 
"MOLEC-STRUCT" ST ? ? PROPERTIES "MOLEC-STRUCT" WT ? ? PROPERTIES PARAMETERS 
BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = RKTKIJ 
SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDKIJ-1" 
? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ SETNO = 1 UNITROW = 0 
TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDMIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL = psi TUNITROW = 22 
TUNITLABEL = F BDBANK = ( BINARY HENRY ) NEL = 6 \ ? PROPERTIES PARAMETERS 
BINARY "T-DEPENDENT" "NRTL-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = NRTL 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F BDBANK = ( "VLE-IG" 
"LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL PARAMNAME2 = NRTL CID1 = WT CID2
 = BZ UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = LLE-ASPEN VAL2 = 
LLE-ASPEN VAL3 = LLE-ASPEN VAL4 = LLE-ASPEN VAL5 = LLE-ASPEN VAL6 = LLE-ASPEN 
VAL7 = LLE-ASPEN VAL8 = LLE-ASPEN VAL9 = LLE-ASPEN VAL10 = LLE-ASPEN VAL11 = 
LLE-ASPEN VAL12 = LLE-ASPEN /  PARAMNAME2 = NRTL CID1 = WT CID2 = ST UNITROW2
 = 0 TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = LLE-ASPEN VAL2 = LLE-ASPEN VAL3 = 
LLE-ASPEN VAL4 = LLE-ASPEN VAL5 = LLE-ASPEN VAL6 = LLE-ASPEN VAL7 = LLE-ASPEN 
VAL8 = LLE-ASPEN VAL9 = LLE-ASPEN VAL10 = LLE-ASPEN VAL11 = LLE-ASPEN VAL12 = 
LLE-ASPEN /  PARAMNAME2 = NRTL CID1 = WT CID2 = EB UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = F VAL1 = LLE-ASPEN VAL2 = LLE-ASPEN VAL3 = LLE-ASPEN VAL4 = 
LLE-ASPEN VAL5 = LLE-ASPEN VAL6 = LLE-ASPEN VAL7 = LLE-ASPEN VAL8 = LLE-ASPEN 
VAL9 = LLE-ASPEN VAL10 = LLE-ASPEN VAL11 = LLE-ASPEN VAL12 = LLE-ASPEN /  
PARAMNAME2 = NRTL CID1 = BZ CID2 = ST UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2
 = F VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG 
VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 
= VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = BZ CID2 = EB UNITROW2 = 0 
TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 
= VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = 
VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1
 = ST CID2 = EB UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = VLE-IG 
VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = 
VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = 
VLE-IG \ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 
ID = MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 
ID = RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 
ID = PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 
ID = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 
ID = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL "COLD-IN" ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 20. <22> 
<4> PRES = 10. <20> <5> BASIS = "MASS-FRAC" FLOWBASE = MASS TOTFLOW = 6000. 
<-80> <3> TOTAL = 1. <-89> <0> JUNK = 4 \ \ MOLE-FLOW SSID1 = MIXED CID = WT 
FLOW = 1. <-3> <0> /  SSID1 = MIXED CID = BZ FLOW = 0. <-3> <0> /  SSID1 = 
MIXED CID = ST FLOW = 0. <-3> <0> /  SSID1 = MIXED CID = EB FLOW = 0. <-3> 
<0> \ ? STREAM MATERIAL "HOT-IN" ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED 
TEMP = 200. <22> <4> PRES = 4. <20> <5> BASIS = "MASS-FRAC" FLOWBASE = MASS 
TOTFLOW = 10000. <-80> <3> TOTAL = 1. <-89> <0> JUNK = 4 \ \ MOLE-FLOW SSID1
 = MIXED CID = WT FLOW = 0.1 <-3> <0> /  SSID1 = MIXED CID = BZ FLOW = 0.5 
<-3> <0> /  SSID1 = MIXED CID = ST FLOW = 0.2 <-3> <0> /  SSID1 = MIXED CID
 = EB FLOW = 0.2 <-3> <0> \ ? BLOCK HEATX HEATEX ? ; "MET_MOLE" ; ; "GEN-HS" 
; \ PARAM SPEC = "VFRAC-HOT" VALUE = 0. <0> <0> \ \ FEEDS FHOT = "HOT-IN" 
FCOLD = "COLD-IN" \ \ PRODUCTS PHOT = "HOT-OUT" PCOLD = "COLD-OUT" \ ? 
"EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = SIMULATION 
\ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE = 
RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L = 
DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFRAC = MOLEFRAC \ ? REPORT 
"FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT "ADA-REPORT" ? ? REPORT 
"BATCH-OPERAT" ? ; "MET_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6420
browserwidth 10335
browsertreewidth 2445
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 6
SIZE -4.6 7.64534 -3.85342 2.58261
BLOCK
ID: HEATEX
Version: 1
ICON: "GEN-HS"
Flag 0
Section GLOBAL
At 4.300000 -0.400000
Label At -0.027185 0.350166
Scale 3.450000 Modifier 0
STREAM
ID: COLD-IN
Version: 1
Flag 0
TYPE 0 TERMINAL 1
At 0.307453 -0.491925
Label At 1.303106 0.090298
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r 0.307453 -0.491925
x x 1.610559 -0.491925
y y 1.610559 -0.401627
x x 2.721529 -0.401627
t l 2.921529 -0.401627
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: COLD-OUT
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At 7.563353 -0.409938
Label At -0.973226 0.008310
ROUTE 0 0
r l 7.563353 -0.409938
x y 6.610559 -0.409938
y x 6.610559 -0.401627
x 0 5.875022 -0.401627
t r 5.675022 -0.401627
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: HOT-IN
Version: 1
Flag 0
TYPE 0 TERMINAL 1
At 5.001241 -3.771428
Label At 0.000000 0.622283
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r u 5.001241 -3.771428
y y 5.001241 -2.526863
x x 5.030586 -2.526863
y y 5.030586 -1.465753
t d 5.030586 -1.265753
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: HOT-OUT
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At 5.308694 1.598758
Label At -0.869192 0.000000
ROUTE 0 0
r l 5.308694 1.598758
x y 3.565964 1.598758
y 0 3.565964 0.662500
t u 3.565964 0.462500
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.70994 -3.2 -3.09503 -3.3205
Size: 0.0204969
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -7.809317 17.975775 3.300000 -5.759627
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.020497

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "FaraDars" "FARADARS_PC"
 )                                                                              
 DSET RUN-STATUS IT @IT ( "DECEMBER 8, 2016    10:04:57 A.M." "_3208jqc.inm" 0) 
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (WT BZ ST EB)                                        
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_3208jqc")                                      
 DSET RUN-STATUS RUNID @RUNID ("_3208jqc")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "DECEMBER 8, 2016 10:04:57 A.M." )                    
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "HEAT EXCHANGER" )                              
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (* * * "HEX" )                                
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (1.80152800D+01 7.81136400D+01 1.04151520D+02 1.06167400D+02)   
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (1.80500000D+01 <3> 8.85091000D+01 <3> 1.14573000D+02 <3>    
 1.22062000D+02 <3> )                                                           
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (3.73150000D+02 <1> 3.53240000D+02 <1> 4.18310000D+02 <1>       
 4.09350000D+02 <1> )                                                           
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 0.D0 0.D0 0.D0   
 0.D0 <3> 0.D0 0.D0 <3> 0.D0 0.D0 <3> 0.D0)                                     
 DSET ALIAS @ALIAS ( "H2O" "C6H6" "C8H8" "C8H10-4" )                            
 IDSET ID_64 (NPOINT) (#4)                                                      
 IDSET ID_65 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)               
 LSET L_33 (%ID_65 & %ID_64)                                                    
 DSET COMPONENTS MAIN COMPS @L_33 ("WT" C "H2O" "H2O" "WT" "BZ" C "C6H6" "C6H6" 
 "BZ" "ST" C "C8H8" "C8H8" "ST" "EB" C "C8H10-4" "C8H10-4" "EB" )               
 IDSET ID_66 (PROPERTIES) (944 *2 <13> 945 *2 <1> 950 *2 <16> 955 *2 <31> 45 *2 
 <22> 46 *2 <20> 47 *2 48 *2 49 *2 <22> 50 *2 <20> 51 *2 52 *2 70 *1 71 *1 164  
 *2 <22> 165 *2 <20> 166 *2 169 *2 <22> 170 *2 <20> 171 *2 938 *1 1170 *2 <31>  
 1171 *2 <75> 1172 *2 <31> 1173 *2 <31> 1174 *2 <75> 1175 *2 <31> 1069 *6 30201 
 *2 <31> )                                                                      
 LSET L_34 (%ID_RXBAL %ID_66)                                                   
 DSET BLOCK HEATX HEATEX BLKSTAT @BLKSTAT (2 0)                                 
 DSET BLOCK HEATX HEATEX COMPSTAT @L1 (2)                                       
 DSET BLOCK HEATX HEATEX BLKMSG @BLKMSG (                                       
 "INTERNAL TEMPERATURE CROSS DETECTED AT ZONE BOUNDARY" )                       
 DSET BLOCK HEATX HEATEX BLKIN @BLKIN (2 HOT-IN COLD-IN)                        
 DSET BLOCK HEATX HEATEX TYPIN @TYPIN (2 MATERIAL MATERIAL)                     
 DSET BLOCK HEATX HEATEX BLKOUT @BLKOUT (2 HOT-OUT COLD-OUT)                    
 DSET BLOCK HEATX HEATEX TYPOUT @TYPOUT (2 MATERIAL MATERIAL)                   
 DSET BLOCK HEATX HEATEX HTX_RES @L_34 (4.90609320D+02 <3> 4.90609320D+02 <3>   
 0.D0 <3> 0.D0 1.60000000D+04 <3> 1.60000000D+04 <3> * <3> 0.D0 * <3> * <3> *   
 <3> * 4.90609320D+02 <3> 4.90609320D+02 <3> 0.D0 <3> 0.D0 1.60000000D+04 <3>   
 1.60000000D+04 <3> * <3> 0.D0 -6.46049505D+06 <3> -6.46049505D+06 <3> * <3>    
 0.D0 4.31496304D+05 <3> 1.53594665D+04 <1> 2.03019012D-02 <3> 1.38377105D-01   
 <1> 3.76349479D+02 <1> 3.94769307D+00 <3> 0.D0 * 4.53126473D+02 <1>            
 9.86923267D+00 <3> 1.75649539D-01 * 9 9 4.73150000D+02 <1> 3.94769307D+00 <3>  
 1.00000000D+00 2.93150000D+02 <1> 9.86923267D+00 <3> 0.D0 0 8.31994789D+01 <1> 
 0.D0 <3> 9.68005211D+01 <1> 2.00235266D+01 <1> 0.D0 <3> 1.59976473D+02 <1>     
 COUNTERCURRENT -7.67769944D+01 <1> )                                           
 IDSET ID_67 (PROPERTIES) (162 *5 163 *5 167 *5 168 *5)                         
 LSET L_35 ( %ID_67)                                                            
 DSET BLOCK HEATX HEATEX HTX_STRM @L_35 (HOT-IN HOT-OUT COLD-IN COLD-OUT)       
 IDSET ID_68 (STRSEQ) ( #2)                                                     
 LSET L_36 (%PORT_NO & %ID_68)                                                  
 LSET L_37 (%PORT_NO & %ID_68)                                                  
 DSET BLOCK HEATX HEATEX IN_PORT @L_36 (0 * * 1 * *)                            
 DSET BLOCK HEATX HEATEX OUT_PORT @L_37 (0 * * 1 * *)                           
 IDSET ID_69 (PROPERTIES) (944 *2 <13> 945 *2 <1> 946 *2 <1> 947 *2 950 *2 <16> 
 951 *2 <16> 953 *2 952 *2 942 *2 954 *2 955 *2 <31> )                          
 LSET L_38 (%ID_69)                                                             
 DSET BLOCK HEATX HEATEX DET-RES1 @L_38 ( 4.31496304D+05 <3> 1.53594665D+04 <1> 
 1.53594665D+04 <1> 0.D0 2.03019012D-02 <3> * <3> * * 1.00000000D+00            
 1.00000000D+00 1.38377105D-01 <1> )                                            
 IDSET ID_70 (PROPERTIES) (957 *2 <25> 958 *2 959 *2 <25> 960 *2 963 *2 <25>    
 964 *2 966 *2 <75> 967 *2 <75> 968 *2 <75> 969 *2 <75> 970 *2 <75> 971 *2 <75> 
 1063 *2 1064 *2 1065 *2 <16> 1066 *2 1067 *2 1068 *2 )                         
 LSET L_39 (%ID_70)                                                             
 DSET BLOCK HEATX HEATEX DET-RES2 @L_39 ( * <1> * * <1> * * <1> * * <3> * <3>   
 0.D0 <3> * <3> * <3> 0.D0 <3> 0.D0 0.D0 2.03019012D-02 <3> 1.00000000D+00      
 6.00000000D-01 8.00000000D-01 )                                                
 IDSET ID_71 (ZONES) ( #3 )                                                     
 IDSET ID_72 (PROPERTIES) (956 *2 <22> 962 *2 <22> 954 *2 <31> 950 *2 <16> 944  
 *2 <13> 945 *2 <1> )                                                           
 LSET L_40 (%ID_72 & %ID_71)                                                    
 DSET BLOCK HEATX HEATEX HTX_ZON @L_40 ( 4.26525846D+02 <1> 4.53126473D+02 <1>  
 3.14764808D+00 <1> 2.03019012D-02 <3> 5.26628443D+04 <3> 8.24102879D+01 <1>    
 4.12343471D+02 <1> 4.53126473D+02 <1> 2.87811034D-02 <1> 2.03019012D-02 <3>    
 8.84438549D+04 <3> 1.51364320D+04 <1> 3.76349479D+02 <1> 4.53126450D+02 <1>    
 1.01714841D+01 <1> 2.03019012D-02 <3> 2.90389605D+05 <3> 1.40624189D+02 <1> )  
 IDSET ID_73 (NPOINTS) ( #7)                                                    
 IDSET ID_74 (PROPERTIES) (747 *6)                                              
 LSET L_41 (%ID_74 & %ID_73)                                                    
 DSET BLOCK HEATX HEATEX ERRTXT @L_41 (                                         
 "*  WARNING"                                                                   
 "   INTERNAL TEMPERATURE CROSS DETECTED AT BOUNDARY OF ZONE 1"                 
 "   HOT STREAM TEMP =   426.5258, COLD STREAM TEMP =   453.1265"               
 ""                                                                             
 "*  WARNING"                                                                   
 "   INTERNAL TEMPERATURE CROSS DETECTED AT BOUNDARY OF ZONE 2"                 
 "   HOT STREAM TEMP =   412.3435, COLD STREAM TEMP =   453.1265"               
 )                                                                              
 IDSET ID_75 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )     
 LSET L_42 ( %ID_75 )                                                           
 IDSET ID_76 (PROPERTIES) (253 *2)                                              
 IDSET ID_77 (PROPERTIES) (253 *2 <11> )                                        
 IDSET ID_78 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_79 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_80 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_81 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_82 (PROPERTIES) (8101 *2 <11> 8002 *2 )                               
 IDSET ID_83 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_43 ( %ISODES (( %ID_NCC & %ID_82 %ID_83) & %IDS_1) )                    
 DSET STREAM MATERIAL COLD-IN STR_MAIN @L_43 (* HEATEX LIQUID 3.33050610D+02 <3>
 0.D0 <3> 0.D0 <3> 0.D0 <3> 1.00000000D+00 0.D0 0.D0 0.D0 3.33050610D+02 <3>    
 6.00000000D+03 <3> 1.00168069D+02 <3> 2.93150000D+02 <1> 9.86923267D+00 <3>    
 0.D0 1.00000000D+00 0.D0 -6.83169330D+04 <3> -3.79216604D+03 <3>               
 -6.32027678D+06 <3> -3.91336088D+01 <3> -2.17224538D+00 <3> 5.54152987D-02 <3> 
 9.98322122D-01 <3> 1.80152800D+01 1.00192724D+02 <3> )                         
 DSET STREAM MATERIAL COLD-IN RES_STR @L_42 (2.93150000D+02 <1> 9.86923267D+00  
 <3> 6.00000000D+03 <3> 1.00168069D+02 <3> 3.33050610D+02 <3> 0.D0 )            
 DSET STREAM MATERIAL COLD-OUT STR_MAIN @L_43 (HEATEX * MIXED 3.33050610D+02 <3>
 0.D0 <3> 0.D0 <3> 0.D0 <3> 1.00000000D+00 0.D0 0.D0 0.D0 3.33050610D+02 <3>    
 6.00000000D+03 <3> 3.77290911D+03 <3> 4.53126473D+02 <1> 9.86923267D+00 <3>    
 1.75649539D-01 8.24350461D-01 0.D0 -6.36528170D+04 <3> -3.53326826D+03 <3>     
 -5.88878048D+06 <3> -2.75338610D+01 <3> -1.52836154D+00 <3> 1.47123699D-03 <3> 
 2.65047463D-02 <3> 1.80152800D+01 1.00192724D+02 <3> )                         
 DSET STREAM MATERIAL COLD-OUT RES_STR @L_42 (4.53126473D+02 <1> 9.86923267D+00 
 <3> 6.00000000D+03 <3> 3.77290911D+03 <3> 3.33050610D+02 <3> 1.75649539D-01 )  
 DSET STREAM MATERIAL HOT-IN STR_MAIN @L_43 (* HEATEX VAPOR 5.55084351D+01 <3>  
 6.40093075D+01 <3> 1.92027922D+01 <3> 1.88381744D+01 <3> 3.52303185D-01        
 4.06256866D-01 1.21877060D-01 1.19562889D-01 1.57558709D+02 <3> 1.00000000D+04 
 <3> 2.58260073D+04 <3> 4.73150000D+02 <1> 3.94769307D+00 <3> 1.00000000D+00    
 0.D0 0.D0 -3.20379470D+03 <3> -5.04785758D+01 <3> -1.40218267D+05 <3>          
 -2.50594546D+01 <3> -3.94833532D-01 <3> 1.01679614D-04 <3> 6.45344295D-03 <3>  
 6.34684052D+01 1.86114668D+02 <3> )                                            
 DSET STREAM MATERIAL HOT-IN RES_STR @L_42 (4.73150000D+02 <1> 3.94769307D+00   
 <3> 1.00000000D+04 <3> 2.58260073D+04 <3> 1.57558709D+02 <3> 1.00000000D+00 )  
 DSET STREAM MATERIAL HOT-OUT STR_MAIN @L_43 (HEATEX * LIQUID 5.55084351D+01 <3>
 6.40093075D+01 <3> 1.92027922D+01 <3> 1.88381744D+01 <3> 3.52303185D-01        
 4.06256866D-01 1.21877060D-01 1.19562889D-01 1.57558709D+02 <3> 1.00000000D+04 
 <3> 2.01392079D+02 <3> 3.76349479D+02 <1> 3.94769307D+00 <3> 0.D0              
 1.00000000D+00 0.D0 -1.30628923D+04 <3> -2.05817244D+02 <3> -5.71714572D+05 <3>
 -4.96846750D+01 <3> -7.82825326D-01 <3> 1.30391348D-02 <3> 8.27573089D-01 <3>  
 6.34684052D+01 1.86114668D+02 <3> )                                            
 DSET STREAM MATERIAL HOT-OUT RES_STR @L_42 (3.76349479D+02 <1> 3.94769307D+00  
 <3> 1.00000000D+04 <3> 2.01392079D+02 <3> 1.57558709D+02 <3> 0.D0 )            
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 1 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 10 * * * * * )                                
 DSET RUN-STATUS COMPSTAT @L_1 (2)                                              
 IDSET ID_84 (NPOINT) ( #4)                                                     
 IDSET ID_85 (PROPERTIES) (747 *6)                                              
 LSET L_44 ( %ID_84 & %ID_85)                                                   
 DSET RUN-STATUS ERRTXT @L_44 (                                                 
 "The following Unit Operation blocks were"                                     
 "completed with warnings:"                                                     
 " HEATEX "                                                                     
 ""                                                                             
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (2)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
