


                                     +
                                   + + +
                                   + + +
                                   + + +
                             +     + + +     +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                     +     + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                     +       +     + + +     +       +
                                   + + +
                                   + + +
                                   + + +
 ASPENTECH                         + + +
                                   + + +
 FLOWSHEET SIMULATION              + + +
 FOR THE PROCESS INDUSTRIES        + + +
                                     +


                                                                        TM
 AAAAA   SSSSS   PPPPP   EEEEE   NN    N   PPPPP   L       U   U   SSSSS
 A   A   S       P   P   E       N N   N   P   P   L       U   U   S    
 AAAAA   SSSSS   PPPPP   EEEEE   N   N N   PPPPP   L       U   U   SSSSS
 A   A       S   P       E       N    NN   P       L       U   U       S
 A   A   SSSSS   P       EEEEE   N     N   P       LLLLL   UUUUU   SSSSS

 ASPEN PLUS IS A TRADEMARK OF           HOTLINE:
 ASPEN TECHNOLOGY, INC.                 U.S.A. 888/996-7001
 TEN CANAL PARK                         EUROPE (32) 2/724-0100
 CAMBRIDGE, MASSACHUSETTS 02141                             
 617/949-1000

 PLATFORM: WIN32                                         NOVEMBER 17, 2016   
 VERSION: 11.1   Build 192                               THURSDAY    
 INSTALLATION: TEAM_EAT                                  11:06:06 P.M.       

 THIS COPY OF ASPEN PLUS LICENSED TO                                 


      ASPEN PLUS (R) IS A PROPRIETARY PRODUCT OF ASPEN TECHNOLOGY, INC.
      (ASPENTECH), AND MAY BE USED ONLY UNDER AGREEMENT WITH ASPENTECH.
      RESTRICTED RIGHTS LEGEND:  USE, REPRODUCTION, OR DISCLOSURE BY THE
      U.S. GOVERNMENT IS SUBJECT TO RESTRICTIONS SET FORTH IN 
      (i) FAR 52.227-14, Alt. III, (ii) FAR 52.227-19, (iii) DFARS 
      252.227-7013(c)(1)(ii), or (iv) THE ACCOMPANYING LICENSE AGREEMENT,
      AS APPLICABLE. FOR PURPOSES OF THE FAR, THIS SOFTWARE SHALL BE DEEMED
      TO BE "UNPUBLISHED" AND LICENSED WITH DISCLOSURE PROHIBITIONS.
      CONTRACTOR/SUBCONTRACTOR: ASPEN TECHNOLOGY, INC. TEN CANAL PARK,
      CAMBRIDGE, MA 02141.
 *** INPUT SUMMARY ***

 >>CURRENT RUN

   ORIGINAL RUN                           NOVEMBER 17, 2016   
   11:06:06 P.M.                          THURSDAY    
   INPUT FILE: _4154vii.inm                                                                    
   RUN ID : _4154vii
     1    ;
     2    ;Input file created by Aspen Plus Rel. 11.1 at 23:06:00 Thu Nov 17, 2016
     3    ;Directory C:\Program Files (x86)\AspenTech\Working Folders\Aspen Plus 11.1  Runid _UNNAMED
     4    ;
     5
     6
     7
     8    TITLE 'DIST2'
     9
    10    IN-UNITS ENG
    11
    12    DEF-STREAMS CONVEN ALL
    13
    14    ACCOUNT-INFO ACCOUNT=D PROJECT-ID=D PROJECT-NAME="D"  &
    15            USER-NAME="D"
    16
    17    DESCRIPTION "
    18        General Simulation with English Units :
    19        F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr.
    20
    21        Property Method: None
    22
    23        Flow basis for input: Mole
    24
    25        Stream report composition: Mole flow
    26        "
    27
    28    DATABANKS PURE11  / AQUEOUS  / SOLIDS  / INORGANIC  /  &
    29            NOASPENPCD
    30
    31    PROP-SOURCES PURE11  / AQUEOUS  / SOLIDS  / INORGANIC
    32
    33    COMPONENTS
    34        BZ C6H6 /
    35        TL C7H8
    36
    37    FLOWSHEET
    38        BLOCK B1 IN=FEED2 OUT=DIST2 BOT2
    39
    40    PROPERTIES NRTL
    41
    42    PROP-DATA NRTL-1
    43        IN-UNITS ENG
    44        PROP-LIST NRTL
    45        BPVAL BZ TL -2.885200000 2023.110164 .3000000000 0.0 0.0  &
    46            0.0 104.0000032 231.3500021
    47        BPVAL TL BZ 2.191100000 -1554.715428 .3000000000 0.0 0.0  &
    48            0.0 104.0000032 231.3500021
    49
    50    STREAM FEED2
    51        SUBSTREAM MIXED PRES=100. <kPa> VFRAC=0.  &
    52            MOLE-FLOW=100. <kmol/hr>
    53        MOLE-FLOW BZ 0.4 / TL 0.6
    54
    55    BLOCK B1 RADFRAC
    56        PARAM NSTAGE=7 P-UPDATE=YES
    57        COL-CONFIG CONDENSER=TOTAL
    58        FEEDS FEED2 4
    59        PRODUCTS DIST2 1 L / BOT2 7 L
    60        P-SPEC 1 100. <kPa>
    61        COL-SPECS MOLE-D=37.5 <kmol/hr> MOLE-RR=3.
    62        TRAY-SIZE 1 2 6 CAPS TRAY-SPACE=2.
    63        TRAY-RATE 1 2 6 CAPS DIAM=1. <meter> P-UPDATE=YES
    64
    65    EO-CONV-OPTI
    66    ;
    67    ;
    68    ;
    69    ;
    70    ;
 *** INPUT TRANSLATOR MESSAGES ***


  *   WARNING IN THE "STREAM" PARAGRAPH WHICH BEGINS ON LINE 50                 
      STREAM NAME: FEED2                                       (STSTRM.29)      
      COMPONENT MOLE FLOWS OF SUBSTREAM: "MIXED"                                
      ARE NORMALIZED TO THE TOTAL MOLE FLOW VALUE.                              
 
 

 PDF updated                                                                      TIME =      8.57

 *** CALCULATION TRACE ***

 DIST2                                                           

 *** FLOWSHEET ANALYSIS MESSAGES ***

 FLOWSHEET CONNECTIVITY BY STREAMS       

   STREAM     SOURCE     DEST           STREAM     SOURCE     DEST
   FEED2      ----       B1             DIST2      B1         ----    
   BOT2       B1         ----                                         

 FLOWSHEET CONNECTIVITY BY BLOCKS        

   BLOCK        INLETS                         OUTLETS
   B1           FEED2                          DIST2 BOT2                  

      COMPUTATION ORDER FOR THE FLOWSHEET IS:
      B1 

Calculations begin                                                              time      0.23


 SIMULATION CALCULATIONS BEGIN                                                    TIME =      0.23

      ENTHALPY CALCULATION FOR INLET STREAM FEED2 OF BLOCK B1                     TIME =      0.26
      KODE = 3  NTRIAL =   3  T =   367.83  P =  0.1000E+06  V =  0.0000E+00  Q =  0.0000E+00

      UOS BLOCK B1       MODEL: RADFRAC                                           TIME =      0.70

       Convergence iterations:
         OL   ML   IL     Err/Tol
          1    1    2      111.38    
          2    1    2      10.390    
          3    1    2      5.6631    
          4    1    3     0.22266    

 Report Writer entered                                                            Time =    126.43

 Results generated                                                                Time =    126.52

 Report Writer entered                                                            Time =    126.60

 Results generated                                                                Time =    126.65

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED


*** INPUT SPECIFICATION MESSAGES ***

 STREAM-REPOR IS  NEW 11/17/2016   23:09:09:71 
 STREAM-REPOR MOLEFLOW MOLEFRAC

 PDF updated                                                                      TIME =    179.56
 THIS COPY OF ASPEN PLUS LICENSED TO                                 
 
 


Calculations begin                                                              time    181.72


 Report Writer entered                                                            Time =    652.49

 Results generated                                                                Time =    652.52

 Report Writer entered                                                            Time =    652.58

 Results generated                                                                Time =    652.61

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED

 *** CALCULATION TRACE ***

 DIST2                                                           


 Report Writer entered                                                            Time =    598.16

 Results generated                                                                Time =    598.18

 Report Writer entered                                                            Time =    598.21

 Results generated                                                                Time =    598.23

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED

 *** CALCULATION TRACE ***

 DIST2                                                           



*** INPUT SPECIFICATION MESSAGES ***

 CHANGES WERE MADE TO STREAM       FEED2    12/11/2016   13:30:02:85 
 ;
 ;Input file created by Aspen Plus Rel. 11.1 at 13:30:00 Sun Dec 11, 2016
 ;Directory ÑèÞKd  Runid simu
 ;
 
 
 
 STREAM FEED2
     SUBSTREAM MIXED PRES=100. <kPa> VFRAC=0.  &
         MOLE-FLOW=100. <kmol/hr>
     MOLE-FRAC BZ 0.4 / TL 0.6

 PDF updated                                                                      TIME =     28.14
 THIS COPY OF ASPEN PLUS LICENSED TO                                 
 
 

Calculations begin                                                              time     30.19


 SIMULATION CALCULATIONS BEGIN                                                    TIME =     30.19

      ENTHALPY CALCULATION FOR INLET STREAM FEED2 OF BLOCK B1                     TIME =     30.19
      KODE = 3  NTRIAL =   3  T =   367.83  P =  0.1000E+06  V =  0.0000E+00  Q =  0.0000E+00

      UOS BLOCK B1       MODEL: RADFRAC                                           TIME =     30.19

       Convergence iterations:
         OL   ML   IL     Err/Tol
          1    1    4      111.96    
          2    1    2      10.231    
          3    1    2      3.9133    
          4    1    2     0.18266    

 Report Writer entered                                                            Time =     62.66

 Results generated                                                                Time =     62.67

 Report Writer entered                                                            Time =     62.71

 Results generated                                                                Time =     62.74

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED
