


                                     +
                                   + + +
                                   + + +
                                   + + +
                             +     + + +     +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                     +     + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                     +       +     + + +     +       +
                                   + + +
                                   + + +
                                   + + +
 ASPENTECH                         + + +
                                   + + +
 FLOWSHEET SIMULATION              + + +
 FOR THE PROCESS INDUSTRIES        + + +
                                     +


                                                                        TM
 AAAAA   SSSSS   PPPPP   EEEEE   NN    N   PPPPP   L       U   U   SSSSS
 A   A   S       P   P   E       N N   N   P   P   L       U   U   S    
 AAAAA   SSSSS   PPPPP   EEEEE   N   N N   PPPPP   L       U   U   SSSSS
 A   A       S   P       E       N    NN   P       L       U   U       S
 A   A   SSSSS   P       EEEEE   N     N   P       LLLLL   UUUUU   SSSSS

 ASPEN PLUS IS A TRADEMARK OF           HOTLINE:
 ASPEN TECHNOLOGY, INC.                 U.S.A. 888/996-7001
 TEN CANAL PARK                         EUROPE (32) 2/724-0100
 CAMBRIDGE, MASSACHUSETTS 02141                             
 617/949-1000

 PLATFORM: WIN32                                         DECEMBER 8, 2016    
 VERSION: 11.1   Build 192                               THURSDAY    
 INSTALLATION: TEAM_EAT                                  10:59:06 A.M.       

 THIS COPY OF ASPEN PLUS LICENSED TO                                 


      ASPEN PLUS (R) IS A PROPRIETARY PRODUCT OF ASPEN TECHNOLOGY, INC.
      (ASPENTECH), AND MAY BE USED ONLY UNDER AGREEMENT WITH ASPENTECH.
      RESTRICTED RIGHTS LEGEND:  USE, REPRODUCTION, OR DISCLOSURE BY THE
      U.S. GOVERNMENT IS SUBJECT TO RESTRICTIONS SET FORTH IN 
      (i) FAR 52.227-14, Alt. III, (ii) FAR 52.227-19, (iii) DFARS 
      252.227-7013(c)(1)(ii), or (iv) THE ACCOMPANYING LICENSE AGREEMENT,
      AS APPLICABLE. FOR PURPOSES OF THE FAR, THIS SOFTWARE SHALL BE DEEMED
      TO BE "UNPUBLISHED" AND LICENSED WITH DISCLOSURE PROHIBITIONS.
      CONTRACTOR/SUBCONTRACTOR: ASPEN TECHNOLOGY, INC. TEN CANAL PARK,
      CAMBRIDGE, MA 02141.
 *** INPUT SUMMARY ***

 >>CURRENT RUN

   ORIGINAL RUN                           DECEMBER 8, 2016    
   10:59:06 A.M.                          THURSDAY    
   INPUT FILE: _5835wiv.inm                                                                    
   RUN ID : _5835wiv
     1    ;
     2    ;Input file created by Aspen Plus Rel. 11.1 at 10:59:06 Thu Dec 8, 2016
     3    ;Directory D:\FaraDars.Org\T1173\FVCHE9506\FVCHE9506-S3\Files And Codes\T2-flash  Runid t1
     4    ;
     5
     6
     7
     8    TITLE 'Tutorial'
     9
    10    IN-UNITS ENG
    11
    12    OUT-UNITS ENG
    13
    14    DEF-STREAMS CONVEN ALL
    15
    16    ACCOUNT-INFO ACCOUNT=1 PROJECT-ID=1  &
    17            PROJECT-NAME="HOS3124@GMAIL.COM"  &
    18            USER-NAME="HOSSEIN KHAKPOUR"
    19
    20    DESCRIPTION "
    21        General Simulation with English Units :
    22        F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr.
    23
    24        Property Method: None
    25
    26        Flow basis for input: Mole
    27
    28        Stream report composition: Mole flow
    29        "
    30
    31    DATABANKS PURE11  / AQUEOUS  / SOLIDS  / INORGANIC  /  &
    32            NOASPENPCD
    33
    34    PROP-SOURCES PURE11  / AQUEOUS  / SOLIDS  / INORGANIC
    35
    36    COMPONENTS
    37        WATER H2O /
    38        ACETONE C3H6O-1 /
    39        MIBK C6H12O-2
    40
    41    FLOWSHEET
    42        BLOCK MIXER IN=FEED MIBK OUT=PRUDUCT
    43        BLOCK FLASH1 IN=PRUDUCT OUT=VAPOR1 WA1 MA1
    44
    45    PROPERTIES NRTL FREE-WATER=STEAMNBS
    46        PROPERTIES IDEAL / PENG-ROB / SRK / UNIFAC
    47
    48    PROP-DATA NRTL-1
    49        IN-UNITS ENG
    50        PROP-LIST NRTL
    51        BPVAL WATER ACETONE .0544000000 755.9488740 .3000000000 0.0  &
    52            0.0 0.0 68.00000346 203.1800024
    53        BPVAL ACETONE WATER 6.398100000 -3256.183774 .3000000000  &
    54            0.0 0.0 0.0 68.00000346 203.1800024
    55        BPVAL WATER MIBK 9.162943000 -2247.739182 .2000000000 0.0  &
    56            0.0 0.0 32.00000374 240.8000021
    57        BPVAL MIBK WATER -3.230481000 2175.978583 .2000000000 0.0  &
    58            0.0 0.0 32.00000374 240.8000021
    59        BPVAL ACETONE MIBK -5.445200000 3300.340834 .3000000000 0.0  &
    60            0.0 0.0 77.00000338 230.2340022
    61        BPVAL MIBK ACETONE 5.301300000 -3124.634735 .3000000000 0.0  &
    62            0.0 0.0 77.00000338 230.2340022
    63
    64    STREAM FEED
    65        SUBSTREAM MIXED TEMP=75. PRES=50. MASS-FLOW=100.
    66        MASS-FRAC WATER 0.5 / ACETONE 0.5
    67
    68    STREAM MIBK
    69        SUBSTREAM MIXED TEMP=75. PRES=50. MASS-FLOW=100.
    70        MOLE-FLOW MIBK 1.
    71
    72    BLOCK MIXER MIXER
    73        PARAM NPHASE=1 PHASE=L
    74        BLOCK-OPTION FREE-WATER=NO
    75
    76    BLOCK FLASH1 FLASH3
    77        PARAM TEMP=75. PRES=50.
    78
    79    EO-CONV-OPTI
    80
    81    STREAM-REPOR MOLEFLOW MASSFRAC
    82    ;
    83    ;
    84    ;
    85    ;
    86    ;
 *** INPUT TRANSLATOR MESSAGES ***


      INFORMATION                                              (ESBPLD.1)       
      BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD                    
      ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD                       

  *   WARNING IN THE "STREAM" PARAGRAPH WHICH BEGINS ON LINE 68                 
      STREAM NAME: MIBK                                        (STSTRM.28)      
      COMPONENT MOLE FLOWS OF SUBSTREAM: "MIXED"                                
      ARE NORMALIZED TO THE TOTAL MOLE FLOW VALUE.                              
 
 

 PDF updated                                                                      TIME =      0.08

 *** CALCULATION TRACE ***

 TUTORIAL                                                        

 *** FLOWSHEET ANALYSIS MESSAGES ***

 FLOWSHEET CONNECTIVITY BY STREAMS       

   STREAM     SOURCE     DEST           STREAM     SOURCE     DEST
   MIBK       ----       MIXER          FEED       ----       MIXER   
   PRUDUCT    MIXER      FLASH1         VAPOR1     FLASH1     ----    
   WA1        FLASH1     ----           MA1        FLASH1     ----    

 FLOWSHEET CONNECTIVITY BY BLOCKS        

   BLOCK        INLETS                         OUTLETS
   MIXER        FEED MIBK                      PRUDUCT                     
   FLASH1       PRUDUCT                        VAPOR1 WA1 MA1              

      COMPUTATION ORDER FOR THE FLOWSHEET IS:
      MIXER FLASH1 

Calculations begin                                                              time      0.09


 SIMULATION CALCULATIONS BEGIN                                                    TIME =      0.09

      ENTHALPY CALCULATION FOR INLET STREAM FEED OF BLOCK MIXER                   TIME =      0.09
      KODE = 2  NTRIAL =   2  T =   297.04  P =  0.3447E+06  V =  0.0000E+00  Q =  0.0000E+00

      ENTHALPY CALCULATION FOR INLET STREAM MIBK OF BLOCK MIXER                   TIME =      0.09
      KODE = 2  NTRIAL =   1  T =   297.04  P =  0.3447E+06  V =  0.0000E+00  Q =  0.0000E+00

      UOS BLOCK MIXER    MODEL: MIXER                                             TIME =      0.09
      KODE = 1   NO. TEMP ITER =    5     TEMP =   291.65    
      KPHASE =    2 KODE =    1 T =   291.65     P =  0.34474E+06 Q =  0.00000E+00

      UOS BLOCK FLASH1   MODEL: FLASH3                                            TIME =      0.09
      KODE = 2  NTRIAL =   9  T =   297.04  P =  0.3447E+06  V =  0.0000E+00  BETA =  0.5818      Q =   412.3    

 Report Writer entered                                                            Time =      0.19

 Results generated                                                                Time =      0.20

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED
