MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Thu Dec 08 14:03:57 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
PLUG
RPlug
Built-In
RPLUG
? SETUP MAIN ? \ TITLE TITLE = "bz plz" \ \ SIMULATE INTERACTIVE = NO 
MOLEFLOW = NOMOLEFLOW MOLEFRAC = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? 
SETUP GLOBAL ? \ "IN-UNITS" INSET = MET \ \ "STREAM-CLASS" SCLASS = CONVEN \ 
? SETUP DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP 
"UNITS-SET" METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = 1 PROJECT-ID = 1 PROJECT-NAME = "1" USER-NAME = "1" \ ? 
SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ DESCRIP DESCRIP = ( 
"General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = C6H6 ANAME = C6H6 OUTNAME = C6H6 TYPE
 = CONV DBNAME1 = "BENZENE" ANAME1 = "C6H6" /  CID = C12H10 ANAME = C12H10 
OUTNAME = C12H10 TYPE = CONV DBNAME1 = "DIPHENYL" ANAME1 = "C12H10" /  CID = 
H2 ANAME = H2 OUTNAME = H2 TYPE = CONV DBNAME1 = "HYDROGEN" ANAME1 = "H2" /  
CID = C18H14 ANAME = C18H14-2 OUTNAME = C18H14 TYPE = CONV DBNAME1 = 
"M-TERPHENYL" ANAME1 = "C18H14-2" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE 
? ? FLOWSHEET GLOBAL ? \ BLOCK BLKID = PLUG BLKTYPE = RPLUG IN = ( FEED M0-1 
) OUT = ( PRODUCT M0-1 ) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? PROPERTIES MAIN 
? \ GPROPERTIES GBASEOPSET = SYSOP0 GOPSETNAME = SYSOP0 PARCON = -1 \ ? 
PROPERTIES "MOLEC-STRUCT" C6H6 ? ? PROPERTIES "MOLEC-STRUCT" C12H10 ? ? 
PROPERTIES "MOLEC-STRUCT" C18H14 ? ? PROPERTIES "MOLEC-STRUCT" H2 ? ? 
PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 
\ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 ID = 
MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 ID = 
RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 ID = 
PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 ID
 = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID
 = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 1400. <22> <2> 
PRES = 14.69595 <20> <2> BASIS = "MOLE-FRAC" TOTFLOW = 0.0682 <-89> <2> TOTAL
 = 1. <-89> <0> JUNK = 4 \ \ MOLE-FLOW SSID1 = MIXED CID = C6H6 FLOW = 1. 
<-4> <0> /  SSID1 = MIXED CID = C12H10 FLOW = 0. <-4> <0> /  SSID1 = MIXED 
CID = H2 FLOW = 0. <-4> <0> /  SSID1 = MIXED CID = C18H14 FLOW = 0. <-4> <0> 
\ ? "STREAM-SUM" ? ? BLOCK RPLUG PLUG ? ; "ENG_MOLE" ; ; ICON2 ; \ PARAM TYPE
 = "T-SPEC" LENGTH = 37.5 <17> <5> DIAM = 0.5 <17> <5> \ \ REACTIONS RXN-ID
 = ( "R-1" ) \ ? "EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS 
MODE = SIMULATION \ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS 
MODE = RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS 
MODE-L = DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L
 = "PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFLOW = NOMOLEFLOW MOLEFRAC = 
MOLEFRAC \ ? REPORT "FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT 
"ADA-REPORT" ? ? REPORT "BATCH-OPERAT" ? ; "ENG_MOLE" ; ? REACTIONS POWERLAW 
"R-1" ? ; "ENG_MOLE" ; \ REAC-DATA R-D-REACNO = 1 PHASE = V R-D-CBASIS = 
MOLARITY PRE-EXP = 3.235E-006 <0> <0> ACT-ENERGY = 30190. <39> <3> \ \ 
REAC-DATA R-D-REACNO = 2 PHASE = V PRE-EXP = 1.0205E-006 <0> <0> ACT-ENERGY
 = 301090. <39> <3> \ \ REAC-DATA R-D-REACNO = 3 PHASE = V PRE-EXP = 
3.7545E-006 <0> <0> ACT-ENERGY = 30190. <39> <3> \ \ REAC-DATA R-D-REACNO = 4 
PHASE = V PRE-EXP = 7.9544E-006 <0> <0> ACT-ENERGY = 30190. <39> <3> \ \ 
STOIC REACNO = 1 STOIC-CID = C6H6 STOIC-SUBS = MIXED COEF = -1. <0> <0> 
EXPONENT = 2. <0> <0> /  REACNO = 2 STOIC-CID = C12H10 STOIC-SUBS = MIXED 
COEF = -0.5 <0> <0> EXPONENT = 1. <0> <0> /  REACNO = 2 STOIC-CID = H2 
STOIC-SUBS = MIXED COEF = -0.5 <0> <0> EXPONENT = 1. <0> <0> /  REACNO = 3 
STOIC-CID = C6H6 STOIC-SUBS = MIXED COEF = -1. <0> <0> /  REACNO = 3 
STOIC-CID = C12H10 STOIC-SUBS = MIXED COEF = -1. <0> <0> /  REACNO = 4 
STOIC-CID = C18H14 STOIC-SUBS = MIXED COEF = -1. <0> <0> /  REACNO = 4 
STOIC-CID = H2 STOIC-SUBS = MIXED COEF = -1. <0> <0> \ \ STOIC1 REACNO1 = 1 
STOIC-CID1 = C12H10 STOIC-SUBS1 = MIXED COEF1 = 0.5 <0> <0> /  REACNO1 = 1 
STOIC-CID1 = H2 STOIC-SUBS1 = MIXED COEF1 = 0.5 <0> <0> /  REACNO1 = 2 
STOIC-CID1 = C6H6 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 3 
STOIC-CID1 = C18H14 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 3 
STOIC-CID1 = H2 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 4 
STOIC-CID1 = C6H6 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 4 
STOIC-CID1 = C12H10 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> \ \ FORCONTROL 
FCVAR1 = C12H10 \ 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6375
browserwidth 11970
browsertreewidth 5250
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 5
SIZE -0.55 8.8864 -11.7314 -1.31
BLOCK
ID: PLUG
Version: 1
ICON: "ICON2"
Flag 0
Section GLOBAL
At 4.850000 -2.200000
Label At 0.000000 0.300000
Annotation At -0.600000 -0.300000
Scale 2.966666 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
Port 1 PLUG i1
TYPE 0 TERMINAL 1
At 0.796904 -2.209628
Label At 1.123839 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r 0.796904 -2.209628
x x 1.920743 -2.209628
y y 1.920743 -2.201527
x x 2.867731 -2.201527
t l 3.067731 -2.201527
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: PRODUCT
Version: 1
Flag 0
Port 0 PLUG o1
TYPE 0 TERMINAL 2
At 8.806811 -2.291362
Label At -1.078251 0.000000
ROUTE 0 0
r l 8.806811 -2.291362
x y 7.728560 -2.291362
y x 7.728560 -2.201527
x 0 6.837621 -2.201527
t r 6.637621 -2.201527
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -0.55 -11.3 0.897931 -11.7314
Size: 0.0089758
Font: 1 0 =Times New Roman
TABLE
Version: 2
CanUpdate: 1
Dim: 3.3 -3.2 6.22058 -6.22023
Size: 1 0.0089758
Font: 1 0 =Times New Roman
Tag
Tag
12 2
2 0
5
1
0
0
0
0
0
0
0
0
Stream ID
To
From
Phase
Stream ID
To
From
Phase
bz plz

FEED
PRODUCT
PLUG


PLUG
VAPOR
VAPOR
Temperature
Pressure
Vapor Frac
Mole Flow
Mass Flow
Volume Flow
Enthalpy
Mole Frac
  C6H6
  C12H10
  H2
  C18H14
K
atm

kmol/hr
kg/hr
l/min
MMBtu/hr





    1033.2
    1033.2
      1.00
      1.00
     1.000
     1.000
     0.031
     0.031
     2.416
     2.416
    43.709
    43.709
     0.006
     0.006
 
 
     1.000
     1.000
          
     trace
          
          
          
          
# of PFS Objects = 0
VIEWPORT -2.432092 8.859468 -1.606667 -5.573972
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.008976

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "Hossein Khakpour"      
 "FARADARS_PC" )                                                                
 DSET RUN-STATUS IT @IT ( "DECEMBER 8, 2016    2:03:05 P.M." "" 0)              
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (C6H6 C12H10 H2 C18H14)                              
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_0304orw")                                      
 DSET RUN-STATUS RUNID @RUNID ("_0304orw")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "DECEMBER 8, 2016 2:03:05 P.M." )                     
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "BZ PLZ" )                                      
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (1 1 "1" "1" )                                
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (7.81136400D+01 1.54211400D+02 2.01588000D+00 2.30309160D+02)   
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (8.85091000D+01 <3> 1.55639000D+02 <3> 5.35578000D+01 <3>    
 2.21275000D+02 <3> )                                                           
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (3.53240000D+02 <1> 5.28150000D+02 <1> 2.03900000D+01 <1>       
 6.48150000D+02 <1> )                                                           
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (-7.42156336D-13 <3> -7.42276021D-13 <3> 0.D0 <3> 0.D0 <3> 
 -2.39908309D-11 -1.00000000D+00 0.D0 0.D0 -1.48443410D-12 <3> -8.81688735D-17  
 -1.72439396D-10 <3> -7.13607667D-11 -3.02937337D-08 <3> -7.26720777D-11)       
 DSET ALIAS @ALIAS ( "C6H6" "C12H10" "H2" "C18H14-2" )                          
 IDSET ID_231 (NPOINT) (#4)                                                     
 IDSET ID_232 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)              
 LSET L_109 (%ID_232 & %ID_231)                                                 
 DSET COMPONENTS MAIN COMPS @L_109 ("C6H6" C "C6H6" "C6H6" "C6H6" "C12H10" C    
 "C12H10" "C12H10" "C12H10" "H2" C "H2" "H2" "H2" "C18H14" C "C18H14-2"         
 "C18H14-2" "C18H14" )                                                          
 IDSET ID_233 (PROPERTIES) (1 *2 <13> 33 *2 <22> 34 *2 <22> 148 *2 <24> 183 *2  
 <20> 170 *2 <20> )                                                             
 LSET L_110 (%ID_RXBAL %ID_233)                                                 
 DSET BLOCK RPLUG PLUG BLKSTAT @BLKSTAT (0 0)                                   
 DSET BLOCK RPLUG PLUG COMPSTAT @L1 (0)                                         
 DSET BLOCK RPLUG PLUG BLKIN @BLKIN (1 FEED)                                    
 DSET BLOCK RPLUG PLUG TYPIN @TYPIN (1 MATERIAL)                                
 DSET BLOCK RPLUG PLUG BLKOUT @BLKOUT (1 PRODUCT)                               
 DSET BLOCK RPLUG PLUG TYPOUT @TYPOUT (1 MATERIAL)                              
 DSET BLOCK RPLUG PLUG RES_Q @L_110 (3.09349993D-02 <3> 3.09349993D-02 <3>      
 1.48443138D-12 <3> -8.81688735D-17 2.41644539D+00 <3> 2.41644539D+00 <3> * <3> 
 -7.13609505D-11 * <3> * <3> * <3> * 3.09349993D-02 <3> 3.09349993D-02 <3>      
 1.48443138D-12 <3> -8.81688735D-17 2.41644539D+00 <3> 2.41644539D+00 <3> * <3> 
 -7.13609505D-11 4.16855204D+02 <3> 4.16855204D+02 <3> * <3> -7.26720777D-11    
 3.02937353D-08 <3> 1.03315000D+03 <1> 1.03315000D+03 <1> 4.60084748D-05 <2>    
 1.00000008D+00 <3> 0.D0 <3> )                                                  
 IDSET ID_234 (NPOINT) (#11)                                                    
 IDSET ID_235 (PROPERTIES) (72 *2 <17> )                                        
 LSET L_111 (%ID_235 & %ID_234 & %IDS_1)                                        
 DSET BLOCK RPLUG PLUG PLPR_1 @L_111 (0.D0 <1> 9.52500000D-02 <1>               
 1.90500000D-01 <1> 2.85750000D-01 <1> 3.81000000D-01 <1> 4.76250000D-01 <1>    
 5.71500000D-01 <1> 6.66750000D-01 <1> 7.62000000D-01 <1> 8.57250000D-01 <1>    
 9.52500000D-01 <1> )                                                           
 IDSET ID_236 (PROPERTIES) (32 *2 <20> )                                        
 LSET L_112 (%ID_236 & %ID_234 & %IDS_1)                                        
 DSET BLOCK RPLUG PLUG PLPR_1 @L_112 (1.00000008D+00 <3> 1.00000008D+00 <3>     
 1.00000008D+00 <3> 1.00000008D+00 <3> 1.00000008D+00 <3> 1.00000008D+00 <3>    
 1.00000008D+00 <3> 1.00000008D+00 <3> 1.00000008D+00 <3> 1.00000008D+00 <3>    
 1.00000008D+00 <3> )                                                           
 IDSET ID_237 (PROPERTIES) (31 *2 <22> )                                        
 LSET L_113 (%ID_237 & %ID_234 & %IDS_1)                                        
 DSET BLOCK RPLUG PLUG PLPR_1 @L_113 (1.03315000D+03 <1> 1.03315000D+03 <1>     
 1.03315000D+03 <1> 1.03315000D+03 <1> 1.03315000D+03 <1> 1.03315000D+03 <1>    
 1.03315000D+03 <1> 1.03315000D+03 <1> 1.03315000D+03 <1> 1.03315000D+03 <1>    
 1.03315000D+03 <1> )                                                           
 IDSET ID_238 (PROPERTIES) (2 *2)                                               
 LSET L_114 (%ID_238 & %ID_234 & %IDS_1)                                        
 DSET BLOCK RPLUG PLUG PLPR_1 @L_114 (1.00000000D+00 1.00000000D+00             
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00     
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 )                  
 IDSET ID_239 (PROPERTIES) (138 *2 <24> )                                       
 LSET L_115 (%ID_239 & %ID_234 & %IDS_1)                                        
 DSET BLOCK RPLUG PLUG PLPR_1 @L_115 (0.D0 <2> 4.60084748D-06 <2>               
 9.20169497D-06 <2> 1.38025425D-05 <2> 1.84033899D-05 <2> 2.30042374D-05 <2>    
 2.76050849D-05 <2> 3.22059324D-05 <2> 3.68067799D-05 <2> 4.14076274D-05 <2>    
 4.60084748D-05 <2> )                                                           
 IDSET ID_240 (PROPERTIES) (67 *2)                                              
 LSET L_116 (%ID_235 & %ID_234 & %IDS_1 )                                       
 DSET BLOCK RPLUG PLUG PZL_1 @L_116 (0.D0 <1> 9.52500000D-02 <1> 1.90500000D-01 
 <1> 2.85750000D-01 <1> 3.81000000D-01 <1> 4.76250000D-01 <1> 5.71500000D-01 <1>
 6.66750000D-01 <1> 7.62000000D-01 <1> 8.57250000D-01 <1> 9.52500000D-01 <1> )  
 IDSET ID_241 (COMPONENTS) (C6H6)                                               
 LSET L_117 ( %ID_240 & %ID_241 & %ID_234 & %IDS_1 )                            
 DSET BLOCK RPLUG PLUG PLZ_1 @L_117 (1.00000000D+00 1.00000000D+00              
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00     
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 )                  
 IDSET ID_242 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )    
 LSET L_118 ( %ID_242 )                                                         
 IDSET ID_243 (PROPERTIES) (253 *2)                                             
 IDSET ID_244 (PROPERTIES) (253 *2 <11> )                                       
 IDSET ID_245 (PROPERTIES) (253 *2 <12> )                                       
 IDSET ID_246 (PROPERTIES) (253 *2 <17> )                                       
 IDSET ID_247 (PROPERTIES) (253 *2 <27> )                                       
 IDSET ID_248 (PROPERTIES) (253 *2 <59> )                                       
 IDSET ID_249 (PROPERTIES) (8002 *2 )                                           
 IDSET ID_250 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22> 
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_119 ( %ISODES (( %ID_NCC & %ID_249 %ID_250) & %IDS_1) )                 
 DSET STREAM MATERIAL FEED STR_MAIN @L_119 (* PLUG VAPOR 1.00000000D+00 0.D0    
 0.D0 0.D0 3.09349993D-02 <3> 2.41644539D+00 <3> 4.37091987D+01 <3>             
 1.03315000D+03 <1> 1.00000008D+00 <3> 1.00000000D+00 0.D0 0.D0 4.85107082D+04  
 <3> 6.21027367D+02 <3> 4.16855204D+02 <3> 7.06646059D+00 <3> 9.04638498D-02 <3>
 1.17957622D-05 <3> 9.21409924D-04 <3> 7.81136400D+01 4.56338152D-02 <3> )      
 DSET STREAM MATERIAL FEED RES_STR @L_118 (1.03315000D+03 <1> 1.00000008D+00 <3>
 2.41644539D+00 <3> 4.37091987D+01 <3> 3.09349993D-02 <3> 1.00000000D+00 )      
 DSET STREAM MATERIAL PRODUCT STR_MAIN @L_119 (PLUG * VAPOR 1.00000000D+00      
 2.39946998D-11 0.D0 0.D0 3.09349993D-02 <3> 2.41644539D+00 <3> 4.37091987D+01  
 <3> 1.03315000D+03 <1> 1.00000008D+00 <3> 1.00000000D+00 0.D0 0.D0             
 4.85107082D+04 <3> 6.21027367D+02 <3> 4.16855204D+02 <3> 7.06646059D+00 <3>    
 9.04638498D-02 <3> 1.17957622D-05 <3> 9.21409924D-04 <3> 7.81136400D+01        
 4.56338152D-02 <3> )                                                           
 DSET STREAM MATERIAL PRODUCT RES_STR @L_118 (1.03315000D+03 <1> 1.00000008D+00 
 <3> 2.41644539D+00 <3> 4.37091987D+01 <3> 3.09349993D-02 <3> 1.00000000D+00 )  
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
