MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Sun Nov 13 11:49:25 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
PLUG
RPlug
Built-In
RPLUG
? SETUP MAIN ? \ TITLE TITLE = "bz plz" \ \ SIMULATE INTERACTIVE = NO 
MOLEFLOW = NOMOLEFLOW MOLEFRAC = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? 
SETUP GLOBAL ? \ "IN-UNITS" INSET = ENG \ \ "STREAM-CLASS" SCLASS = CONVEN \ 
? SETUP DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP 
"UNITS-SET" METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = 1 PROJECT-ID = 1 PROJECT-NAME = "1" USER-NAME = "1" \ ? 
SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ DESCRIP DESCRIP = ( 
"General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = C6H6 ANAME = C6H6 OUTNAME = C6H6 TYPE
 = CONV DBNAME1 = "BENZENE" ANAME1 = "C6H6" /  CID = C12H10 ANAME = C12H10 
OUTNAME = C12H10 TYPE = CONV DBNAME1 = "DIPHENYL" ANAME1 = "C12H10" /  CID = 
H2 ANAME = H2 OUTNAME = H2 TYPE = CONV DBNAME1 = "HYDROGEN" ANAME1 = "H2" /  
CID = C18H14 ANAME = C18H14-2 OUTNAME = C18H14 TYPE = CONV DBNAME1 = 
"M-TERPHENYL" ANAME1 = "C18H14-2" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE 
? ? FLOWSHEET GLOBAL ? \ BLOCK BLKID = PLUG BLKTYPE = RPLUG IN = ( FEED M0-1 
) OUT = ( PRODUCT M0-1 ) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? PROPERTIES MAIN 
? \ GPROPERTIES GBASEOPSET = SYSOP0 GOPSETNAME = SYSOP0 PARCON = -1 \ ? 
PROPERTIES "MOLEC-STRUCT" C6H6 ? ? PROPERTIES "MOLEC-STRUCT" C12H10 ? ? 
PROPERTIES "MOLEC-STRUCT" C18H14 ? ? PROPERTIES "MOLEC-STRUCT" H2 ? ? 
PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 
\ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 ID = 
MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 ID = 
RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 ID = 
PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 ID
 = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID
 = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 1400. <22> <2> 
PRES = 14.69595 <20> <2> BASIS = "MOLE-FRAC" TOTFLOW = 0.0682 <-89> <2> TOTAL
 = 1. <-89> <0> JUNK = 4 \ \ MOLE-FLOW SSID1 = MIXED CID = C6H6 FLOW = 1. 
<-4> <0> /  SSID1 = MIXED CID = C12H10 FLOW = 0. <-4> <0> /  SSID1 = MIXED 
CID = H2 FLOW = 0. <-4> <0> /  SSID1 = MIXED CID = C18H14 FLOW = 0. <-4> <0> 
\ ? BLOCK RPLUG PLUG ? ; "ENG_MOLE" ; ; ICON2 ; \ PARAM TYPE = "T-SPEC" 
LENGTH = 37.5 <17> <5> DIAM = 0.5 <17> <5> \ \ REACTIONS RXN-ID = ( "R-1" ) \ 
? "EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = 
SIMULATION \ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE
 = RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L
 = DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFLOW = NOMOLEFLOW MOLEFRAC = 
MOLEFRAC \ ? REPORT "FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT 
"ADA-REPORT" ? ? REPORT "BATCH-OPERAT" ? ; "ENG_MOLE" ; ? REACTIONS POWERLAW 
"R-1" ? ; "ENG_MOLE" ; \ REAC-DATA R-D-REACNO = 1 PHASE = V R-D-CBASIS = 
MOLARITY PRE-EXP = 3.235E-006 <0> <0> ACT-ENERGY = 30190. <39> <3> \ \ 
REAC-DATA R-D-REACNO = 2 PHASE = V PRE-EXP = 1.0205E-006 <0> <0> ACT-ENERGY
 = 301090. <39> <3> \ \ REAC-DATA R-D-REACNO = 3 PHASE = V PRE-EXP = 
3.7545E-006 <0> <0> ACT-ENERGY = 30190. <39> <3> \ \ REAC-DATA R-D-REACNO = 4 
PHASE = V PRE-EXP = 7.9544E-006 <0> <0> ACT-ENERGY = 30190. <39> <3> \ \ 
STOIC REACNO = 1 STOIC-CID = C6H6 STOIC-SUBS = MIXED COEF = -1. <0> <0> 
EXPONENT = 2. <0> <0> /  REACNO = 2 STOIC-CID = C12H10 STOIC-SUBS = MIXED 
COEF = -0.5 <0> <0> EXPONENT = 1. <0> <0> /  REACNO = 2 STOIC-CID = H2 
STOIC-SUBS = MIXED COEF = -0.5 <0> <0> EXPONENT = 1. <0> <0> /  REACNO = 3 
STOIC-CID = C6H6 STOIC-SUBS = MIXED COEF = -1. <0> <0> /  REACNO = 3 
STOIC-CID = C12H10 STOIC-SUBS = MIXED COEF = -1. <0> <0> /  REACNO = 4 
STOIC-CID = C18H14 STOIC-SUBS = MIXED COEF = -1. <0> <0> /  REACNO = 4 
STOIC-CID = H2 STOIC-SUBS = MIXED COEF = -1. <0> <0> \ \ STOIC1 REACNO1 = 1 
STOIC-CID1 = C12H10 STOIC-SUBS1 = MIXED COEF1 = 0.5 <0> <0> /  REACNO1 = 1 
STOIC-CID1 = H2 STOIC-SUBS1 = MIXED COEF1 = 0.5 <0> <0> /  REACNO1 = 2 
STOIC-CID1 = C6H6 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 3 
STOIC-CID1 = C18H14 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 3 
STOIC-CID1 = H2 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 4 
STOIC-CID1 = C6H6 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> /  REACNO1 = 4 
STOIC-CID1 = C12H10 STOIC-SUBS1 = MIXED COEF1 = 1. <0> <0> \ \ FORCONTROL 
FCVAR1 = C12H10 \ 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6465
browserwidth 11970
browsertreewidth 5250
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 4
SIZE -4.63839 4.53622 -0.693333 0.79
BLOCK
ID: PLUG
Version: 1
ICON: "ICON2"
Flag 0
Section GLOBAL
At -0.500000 -0.100000
Label At 0.000000 0.300000
Annotation At -0.600000 -0.300000
Scale 2.966666 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
Port 1 PLUG i1
TYPE 0 TERMINAL 1
At -4.556657 -0.194118
Label At 0.565828 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -4.556657 -0.194118
x x -3.425000 -0.194118
y y -3.425000 -0.101527
x x -2.482269 -0.101527
t l -2.282269 -0.101527
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: PRODUCT
Version: 1
Flag 0
Port 0 PLUG o1
TYPE 0 TERMINAL 2
At 3.453251 -0.194118
Label At -0.539125 0.000000
ROUTE 0 0
r l 3.453251 -0.194118
x y 2.375000 -0.194118
y x 2.375000 -0.101527
x 0 1.487621 -0.101527
t r 1.287621 -0.101527
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.71889 -3.2 -2.41115 -3.5694
Size: 0.0204334
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -7.785140 19.677399 4.808309 -5.224509
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.020433

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "Hossein Khakpour"      
 "HOSSEINKHAKPOUR" )                                                            
 DSET RUN-STATUS IT @IT ( "NOVEMBER 13, 2016   11:39:22 A.M." "_0437fpq.inm" 0) 
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (C6H6 C12H10 H2 C18H14)                              
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_0437fpq")                                      
 DSET RUN-STATUS RUNID @RUNID ("_0437fpq")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "NOVEMBER 13, 2016 11:39:22 A.M." )                   
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "BZ PLZ" )                                      
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (1 1 "1" "1" )                                
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (7.81136400D+01 1.54211400D+02 2.01588000D+00 2.30309160D+02)   
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (1.41777978D+00 <2> 2.49309763D+00 <2> 8.57913662D-01 <2>    
 3.54448550D+00 <2> )                                                           
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (1.76162003D+02 <2> 4.91000000D+02 <2> -4.22967993D+02 <2>      
 7.06999998D+02 <2> )                                                           
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (-1.63617730D-12 <2> -1.63643853D-12 <2> 0.D0 <2> 0.D0 <2> 
 -2.39908696D-11 -1.00000000D+00 0.D0 0.D0 -3.27261829D-12 <2> -1.06377526D-16  
 -3.80163456D-10 <2> -7.13607025D-11 -4.32774868D-07 <2> -7.26720716D-11)       
 DSET ALIAS @ALIAS ( "C6H6" "C12H10" "H2" "C18H14-2" )                          
 IDSET ID_116 (NPOINT) (#4)                                                     
 IDSET ID_117 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)              
 LSET L_49 (%ID_117 & %ID_116)                                                  
 DSET COMPONENTS MAIN COMPS @L_49 ("C6H6" C "C6H6" "C6H6" "C6H6" "C12H10" C     
 "C12H10" "C12H10" "C12H10" "H2" C "H2" "H2" "H2" "C18H14" C "C18H14-2"         
 "C18H14-2" "C18H14" )                                                          
 IDSET ID_118 (PROPERTIES) (1 *2 <13> 33 *2 <22> 34 *2 <22> 148 *2 <24> 183 *2  
 <20> 170 *2 <20> )                                                             
 LSET L_50 (%ID_RXBAL %ID_118)                                                  
 DSET BLOCK RPLUG PLUG BLKSTAT @BLKSTAT (0 0)                                   
 DSET BLOCK RPLUG PLUG COMPSTAT @L1 (0)                                         
 DSET BLOCK RPLUG PLUG BLKIN @BLKIN (1 FEED)                                    
 DSET BLOCK RPLUG PLUG TYPIN @TYPIN (1 MATERIAL)                                
 DSET BLOCK RPLUG PLUG BLKOUT @BLKOUT (1 PRODUCT)                               
 DSET BLOCK RPLUG PLUG TYPOUT @TYPOUT (1 MATERIAL)                              
 DSET BLOCK RPLUG PLUG RES_Q @L_50 (6.82000000D-02 <2> 6.82000000D-02 <2>       
 3.27261103D-12 <2> -1.06377526D-16 5.32735025D+00 <2> 5.32735025D+00 <2> * <2> 
 -7.13608692D-11 * <2> * <2> * <2> * 6.82000000D-02 <2> 6.82000000D-02 <2>      
 3.27261103D-12 <2> -1.06377526D-16 5.32735025D+00 <2> 5.32735025D+00 <2> * <2> 
 -7.13608692D-11 5.95517451D+03 <2> 5.95517451D+03 <2> * <2> -7.26720716D-11    
 4.32774927D-07 <2> 1.40000000D+03 <2> 1.40000000D+03 <2> 4.60084748D-05 <2>    
 1.46959500D+01 <2> 0.D0 <2> )                                                  
 IDSET ID_119 (NPOINT) (#11)                                                    
 IDSET ID_120 (PROPERTIES) (72 *2 <17> )                                        
 LSET L_51 (%ID_120 & %ID_119 & %IDS_1)                                         
 DSET BLOCK RPLUG PLUG PLPR_1 @L_51 (0.D0 <2> 3.12500000D-01 <2> 6.25000000D-01 
 <2> 9.37500000D-01 <2> 1.25000000D+00 <2> 1.56250000D+00 <2> 1.87500000D+00 <2>
 2.18750000D+00 <2> 2.50000000D+00 <2> 2.81250000D+00 <2> 3.12500000D+00 <2> )  
 IDSET ID_121 (PROPERTIES) (32 *2 <20> )                                        
 LSET L_52 (%ID_121 & %ID_119 & %IDS_1)                                         
 DSET BLOCK RPLUG PLUG PLPR_1 @L_52 (1.46959500D+01 <2> 1.46959500D+01 <2>      
 1.46959500D+01 <2> 1.46959500D+01 <2> 1.46959500D+01 <2> 1.46959500D+01 <2>    
 1.46959500D+01 <2> 1.46959500D+01 <2> 1.46959500D+01 <2> 1.46959500D+01 <2>    
 1.46959500D+01 <2> )                                                           
 IDSET ID_122 (PROPERTIES) (31 *2 <22> )                                        
 LSET L_53 (%ID_122 & %ID_119 & %IDS_1)                                         
 DSET BLOCK RPLUG PLUG PLPR_1 @L_53 (1.40000000D+03 <2> 1.40000000D+03 <2>      
 1.40000000D+03 <2> 1.40000000D+03 <2> 1.40000000D+03 <2> 1.40000000D+03 <2>    
 1.40000000D+03 <2> 1.40000000D+03 <2> 1.40000000D+03 <2> 1.40000000D+03 <2>    
 1.40000000D+03 <2> )                                                           
 IDSET ID_123 (PROPERTIES) (2 *2)                                               
 LSET L_54 (%ID_123 & %ID_119 & %IDS_1)                                         
 DSET BLOCK RPLUG PLUG PLPR_1 @L_54 (1.00000000D+00 1.00000000D+00              
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00     
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 )                  
 IDSET ID_124 (PROPERTIES) (138 *2 <24> )                                       
 LSET L_55 (%ID_124 & %ID_119 & %IDS_1)                                         
 DSET BLOCK RPLUG PLUG PLPR_1 @L_55 (0.D0 <2> 4.60084748D-06 <2> 9.20169497D-06 
 <2> 1.38025425D-05 <2> 1.84033899D-05 <2> 2.30042374D-05 <2> 2.76050849D-05 <2>
 3.22059324D-05 <2> 3.68067799D-05 <2> 4.14076274D-05 <2> 4.60084748D-05 <2>    
 )                                                                              
 IDSET ID_125 (PROPERTIES) (67 *2)                                              
 LSET L_56 (%ID_120 & %ID_119 & %IDS_1 )                                        
 DSET BLOCK RPLUG PLUG PZL_1 @L_56 (0.D0 <2> 3.12500000D-01 <2> 6.25000000D-01  
 <2> 9.37500000D-01 <2> 1.25000000D+00 <2> 1.56250000D+00 <2> 1.87500000D+00 <2>
 2.18750000D+00 <2> 2.50000000D+00 <2> 2.81250000D+00 <2> 3.12500000D+00 <2> )  
 IDSET ID_126 (COMPONENTS) (C6H6)                                               
 LSET L_57 ( %ID_125 & %ID_126 & %ID_119 & %IDS_1 )                             
 DSET BLOCK RPLUG PLUG PLZ_1 @L_57 (1.00000000D+00 1.00000000D+00               
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00     
 1.00000000D+00 1.00000000D+00 1.00000000D+00 1.00000000D+00 )                  
 IDSET ID_127 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )    
 LSET L_58 ( %ID_127 )                                                          
 IDSET ID_128 (PROPERTIES) (253 *2)                                             
 IDSET ID_129 (PROPERTIES) (253 *2 <11> )                                       
 IDSET ID_130 (PROPERTIES) (253 *2 <12> )                                       
 IDSET ID_131 (PROPERTIES) (253 *2 <17> )                                       
 IDSET ID_132 (PROPERTIES) (253 *2 <27> )                                       
 IDSET ID_133 (PROPERTIES) (253 *2 <59> )                                       
 IDSET ID_134 (PROPERTIES) (8002 *2 )                                           
 IDSET ID_135 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22> 
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_59 ( %ISODES (( %ID_NCC & %ID_134 %ID_135) & %IDS_1) )                  
 DSET STREAM MATERIAL FEED STR_MAIN @L_59 (* PLUG VAPOR 1.00000000D+00 0.D0     
 0.D0 0.D0 6.82000000D-02 <2> 5.32735025D+00 <2> 9.26145492D+01 <2>             
 1.40000000D+03 <2> 1.46959500D+01 <2> 1.00000000D+00 0.D0 0.D0 8.73192747D+04  
 <2> 1.11784926D+03 <2> 5.95517451D+03 <2> 7.06646059D+00 <2> 9.04638498D-02 <2>
 7.36385396D-04 <2> 5.75217437D-02 <2> 7.81136400D+01 9.66925806D-02 <2> )      
 DSET STREAM MATERIAL FEED RES_STR @L_58 (1.40000000D+03 <2> 1.46959500D+01 <2> 
 5.32735025D+00 <2> 9.26145492D+01 <2> 6.82000000D-02 <2> 1.00000000D+00 )      
 DSET STREAM MATERIAL PRODUCT STR_MAIN @L_59 (PLUG * VAPOR 1.00000000D+00       
 2.39946998D-11 0.D0 0.D0 6.82000000D-02 <2> 5.32735025D+00 <2> 9.26145492D+01  
 <2> 1.40000000D+03 <2> 1.46959500D+01 <2> 1.00000000D+00 0.D0 0.D0             
 8.73192747D+04 <2> 1.11784926D+03 <2> 5.95517451D+03 <2> 7.06646059D+00 <2>    
 9.04638498D-02 <2> 7.36385396D-04 <2> 5.75217437D-02 <2> 7.81136400D+01        
 9.66925806D-02 <2> )                                                           
 DSET STREAM MATERIAL PRODUCT RES_STR @L_58 (1.40000000D+03 <2> 1.46959500D+01  
 <2> 5.32735025D+00 <2> 9.26145492D+01 <2> 6.82000000D-02 <2> 1.00000000D+00 )  
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET ID_136 (NPOINT) ( #7)                                                    
 IDSET ID_137 (PROPERTIES) (747 *6)                                             
 LSET L_60 ( %ID_136 & %ID_137)                                                 
 DSET RUN-STATUS ERRTXT @L_60 (                                                 
 "The following messages were issued during Input Translation:"                 
 ""                                                                             
 "   INFORMATION WHILE CHECKING INPUT SPECIFICATIONS"                           
 "   BLOCK NAME: PLUG    MODEL NAME: RPLUG"                                     
 "   THE REACTOR TYPE IS 'SPECIFIED TEMPERATURE' AND NO TEMPERATURE"            
 "   IS GIVEN WITH A 'T-SPEC' SENTENCE. THE REACTOR TEMPERATURE"                
 "   WILL BE SET TO THE (MIXED) INLET TEMPERATURE."                             
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
