MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Sun Nov 27 16:21:06 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
3
>VERSION 0
MIXER
Mixer
Built-In
MIXER
>VERSION 0
PUMP
Pump
Built-In
PUMP
>VERSION 0
VALVE
Valve
Built-In
VALVE
? SETUP MAIN ? \ TITLE TITLE = "simulation" \ \ SIMULATE INTERACTIVE = NO 
MOLEFLOW = MOLEFLOW MOLEFRAC = MOLEFRAC MASSFRAC = MASSFRAC TFFFILE = "GEN_M" 
VISITED = 1 \ ? SETUP GLOBAL ? \ "IN-UNITS" INSET = MET OUTSET = ENG \ \ 
"STREAM-CLASS" SCLASS = CONVEN \ ? SETUP DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" 
? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = 12 PROJECT-ID = 123 PROJECT-NAME = "ASA-1" USER-NAME = "ASA" 
\ ? SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ DESCRIP DESCRIP = ( 
"General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = WT ANAME = H2O OUTNAME = WT TYPE = 
CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  CID = AC ANAME = C3H6O-1 OUTNAME = 
AC TYPE = CONV DBNAME1 = "ACETONE" ANAME1 = "C3H6O-1" /  CID = MIBK ANAME = 
C6H12O-2 OUTNAME = MIBK DBNAME1 = "METHYL-ISOBUTYL-KETONE" ANAME1 = "C6H12O-2" 
/  CID = BUOH ANAME = C4H10O-1 OUTNAME = BUOH TYPE = CONV DBNAME1 = "N-BUTANOL" 
ANAME1 = "C4H10O-1" /  CID = NBAC ANAME = C6H12O2-1 OUTNAME = NBAC DBNAME1 = 
"N-BUTYL-ACETATE" ANAME1 = "C6H12O2-1" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? 
SOLVE ? ? FLOWSHEET GLOBAL ? \ BLOCK BLKID = MIXER BLKTYPE = MIXER IN = ( 1 
M0-1 2 M0-1 3 M0-1 ) OUT = ( 4 M0-1 ) \ \ BLOCK BLKID = PUMP BLKTYPE = PUMP 
IN = ( 4 M0-1 ) OUT = ( 5 M0-1 ) \ \ BLOCK BLKID = VALVE BLKTYPE = VALVE 
IN = ( 5 M0-1 ) OUT = ( 6 M0-1 ) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? 
PROPERTIES MAIN ? \ GPROPERTIES GBASEOPSET = IDEAL GOPSETNAME = IDEAL PARCON
 = -2 \ ? PROPERTIES "OPTION-SETS" IDEAL ? \ PARAM BASE = IDEAL \ ? 
PROPERTIES "OPTION-SETS" NRTL ? \ PARAM BASE = NRTL \ ? PROPERTIES 
"OPTION-SETS" "NRTL-2" ? \ PARAM BASE = "NRTL-2" \ ? PROPERTIES "OPTION-SETS" 
"PENG-ROB" ? \ PARAM BASE = "PENG-ROB" \ ? PROPERTIES "MOLEC-STRUCT" AC ? ? 
PROPERTIES "MOLEC-STRUCT" BUOH ? ? PROPERTIES "MOLEC-STRUCT" MIBK ? ? 
PROPERTIES "MOLEC-STRUCT" NBAC ? ? PROPERTIES "MOLEC-STRUCT" WT ? ? 
PROPERTIES REGPAR ? \ FRED REGCASE = "DB-PURE11" PARNAME = "API" COMPI = "WT" 
COMPJ = "" VALUE = ( "1.00000000E+01" ) /  REGCASE = "DB-PURE11" PARNAME = 
"API" COMPI = "AC" COMPJ = "" VALUE = ( "4.85000000E+01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "API" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"4.57562000E+01" ) /  REGCASE = "DB-PURE11" PARNAME = "DGFORM" COMPI = "WT" 
COMPJ = "" VALUE = ( "-2.28590000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = 
"DGFORM" COMPI = "AC" COMPJ = "" VALUE = ( "-1.51300000E+08" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DGFORM" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"-1.35100000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = "DHFORM" COMPI = "WT" 
COMPJ = "" VALUE = ( "-2.41814000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = 
"DHFORM" COMPI = "AC" COMPJ = "" VALUE = ( "-2.15700000E+08" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DHFORM" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"-2.86400000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = "DHVLB" COMPI = "WT" 
COMPJ = "" VALUE = ( "4.07992000E+07" ) /  REGCASE = "DB-PURE11" PARNAME = 
"DHVLB" COMPI = "AC" COMPJ = "" VALUE = ( "2.95566000E+07" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DHVLB" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"3.45593000E+07" ) /  REGCASE = "DB-PURE11" PARNAME = "HCOM" COMPI = "WT" 
COMPJ = "" VALUE = ( "0.E0" ) /  REGCASE = "DB-PURE11" PARNAME = "HCOM" COMPI
 = "AC" COMPJ = "" VALUE = ( "-1.65900000E+09" ) /  REGCASE = "DB-PURE11" 
PARNAME = "HCOM" COMPI = "MIBK" COMPJ = "" VALUE = ( "-3.47620000E+09" ) /  
REGCASE = "DB-PURE11" PARNAME = "MUP" COMPI = "WT" COMPJ = "" VALUE = ( 
"5.84934000E-25" ) /  REGCASE = "DB-PURE11" PARNAME = "MUP" COMPI = "AC" 
COMPJ = "" VALUE = ( "9.11056000E-25" ) /  REGCASE = "DB-PURE11" PARNAME = 
"MUP" COMPI = "MIBK" COMPJ = "" VALUE = ( "8.50382000E-25" ) /  REGCASE = 
"DB-PURE11" PARNAME = "MW" COMPI = "WT" COMPJ = "" VALUE = ( "1.80152800E+01" 
) /  REGCASE = "DB-PURE11" PARNAME = "MW" COMPI = "AC" COMPJ = "" VALUE = ( 
"5.80800400E+01" ) /  REGCASE = "DB-PURE11" PARNAME = "MW" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "1.00160680E+02" ) /  REGCASE = "DB-PURE11" PARNAME = 
"OMEGA" COMPI = "WT" COMPJ = "" VALUE = ( "3.44861000E-01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "OMEGA" COMPI = "AC" COMPJ = "" VALUE = ( 
"3.06527000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "OMEGA" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "3.55671000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "PC" 
COMPI = "WT" COMPJ = "" VALUE = ( "2.20550000E+07" ) /  REGCASE = "DB-PURE11" 
PARNAME = "PC" COMPI = "AC" COMPJ = "" VALUE = ( "4.70100000E+06" ) /  
REGCASE = "DB-PURE11" PARNAME = "PC" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"3.27000000E+06" ) /  REGCASE = "DB-PURE11" PARNAME = "RKTZRA" COMPI = "WT" 
COMPJ = "" VALUE = ( "2.43172000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = 
"RKTZRA" COMPI = "AC" COMPJ = "" VALUE = ( "2.45200000E-01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "RKTZRA" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"2.58900000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "SG" COMPI = "WT" COMPJ
 = "" VALUE = ( "1.00000000E+00" ) /  REGCASE = "DB-PURE11" PARNAME = "SG" 
COMPI = "AC" COMPJ = "" VALUE = ( "7.86000000E-01" ) /  REGCASE = "DB-PURE11" 
PARNAME = "SG" COMPI = "MIBK" COMPJ = "" VALUE = ( "7.98280000E-01" ) /  
REGCASE = "DB-PURE11" PARNAME = "TB" COMPI = "WT" COMPJ = "" VALUE = ( 
"3.73150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "TB" COMPI = "AC" COMPJ
 = "" VALUE = ( "3.29440000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "TB" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "3.89150000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "TC" COMPI = "WT" COMPJ = "" VALUE = ( "6.47130000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "TC" COMPI = "AC" COMPJ = "" VALUE = ( 
"5.08200000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "TC" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "5.74600000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "VB" 
COMPI = "WT" COMPJ = "" VALUE = ( "1.88308000E-02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "VB" COMPI = "AC" COMPJ = "" VALUE = ( "7.74659000E-02" ) /  
REGCASE = "DB-PURE11" PARNAME = "VB" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"1.41450000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "VC" COMPI = "WT" COMPJ
 = "" VALUE = ( "5.59478000E-02" ) /  REGCASE = "DB-PURE11" PARNAME = "VC" 
COMPI = "AC" COMPJ = "" VALUE = ( "2.09000000E-01" ) /  REGCASE = "DB-PURE11" 
PARNAME = "VC" COMPI = "MIBK" COMPJ = "" VALUE = ( "3.69000000E-01" ) /  
REGCASE = "DB-PURE11" PARNAME = "VLSTD" COMPI = "WT" COMPJ = "" VALUE = ( 
"1.80500000E-02" ) /  REGCASE = "DB-PURE11" PARNAME = "VLSTD" COMPI = "AC" 
COMPJ = "" VALUE = ( "7.39962000E-02" ) /  REGCASE = "DB-PURE11" PARNAME = 
"VLSTD" COMPI = "MIBK" COMPJ = "" VALUE = ( "1.25788000E-01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "ZC" COMPI = "WT" COMPJ = "" VALUE = ( "2.29000000E-01" 
) /  REGCASE = "DB-PURE11" PARNAME = "ZC" COMPI = "AC" COMPJ = "" VALUE = ( 
"2.33000000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "ZC" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "2.53000000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = 
"ATOMNO" COMPI = "WT" COMPJ = "" VALUE = ( "1.00000000E+00" "8.00000000E+00" 
) /  REGCASE = "DB-PURE11" PARNAME = "ATOMNO" COMPI = "AC" COMPJ = "" VALUE
 = ( "6.00000000E+00" "1.00000000E+00" "8.00000000E+00" ) /  REGCASE = 
"DB-PURE11" PARNAME = "ATOMNO" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"6.00000000E+00" "1.00000000E+00" "8.00000000E+00" ) /  REGCASE = "DB-PURE11" 
PARNAME = "CPIGDP" COMPI = "WT" COMPJ = "" VALUE = ( "3.33630000E+04" 
"2.67900000E+04" "2.61050000E+03" "8.89600000E+03" "1.16900000E+03" 
"1.00000000E+02" "2.27315000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "CPIGDP" 
COMPI = "AC" COMPJ = "" VALUE = ( "5.70400000E+04" "1.63200000E+05" 
"1.60700000E+03" "9.68000000E+04" "7.31500000E+02" "2.00000000E+02" 
"1.50000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "CPIGDP" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "1.22700000E+05" "2.19500000E+05" "8.42000000E+02" 
"1.19100000E+05" "2.46000000E+03" "2.98150000E+02" "1.50015000E+03" ) /  
REGCASE = "DB-PURE11" PARNAME = "CPSDIP" COMPI = "WT" COMPJ = "" VALUE = ( 
"-2.62490000E+02" "1.40520000E+02" "0.E0" "0.E0" "0.E0" "3.15000000E+00" 
"2.73150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "CPSDIP" COMPI = "AC" 
COMPJ = "" VALUE = ( "-1.20000000E+04" "1.27600000E+03" "-6.17000000E+00" 
"1.32000000E-02" "0.E0" "3.00000000E+01" "1.78450000E+02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "CPSDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"1.69000000E+05" "0.E0" "0.E0" "0.E0" "0.E0" "1.89150000E+02" "1.89150000E+02" 
) /  REGCASE = "DB-PURE11" PARNAME = "DHVLDP" COMPI = "WT" COMPJ = "" VALUE
 = ( "5.20530000E+07" "3.19900000E-01" "-2.12000000E-01" "2.57950000E-01" 
"0.E0" "2.73160000E+02" "6.47130000E+02" ) /  REGCASE = "DB-PURE11" PARNAME
 = "DHVLDP" COMPI = "AC" COMPJ = "" VALUE = ( "4.21500000E+07" "3.39700000E-01" 
"0.E0" "0.E0" "0.E0" "1.78450000E+02" "5.08200000E+02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DHVLDP" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"5.46870000E+07" "4.05830000E-01" "0.E0" "0.E0" "0.E0" "1.89150000E+02" 
"5.74600000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNLDIP" COMPI = "WT" 
COMPJ = "" VALUE = ( "1.78630000E+01" "5.86060000E+01" "-9.53960000E+01" 
"2.13890000E+02" "-1.41260000E+02" "2.73160000E+02" "6.47130000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "DNLDIP" COMPI = "AC" COMPJ = "" VALUE = ( 
"1.23320000E+00" "2.58860000E-01" "5.08200000E+02" "2.91300000E-01" "0.E0" 
"1.78450000E+02" "5.08200000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNLDIP" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "7.16870000E-01" "2.64530000E-01" 
"5.74600000E+02" "2.89180000E-01" "0.E0" "1.89150000E+02" "5.74600000E+02" ) 
/  REGCASE = "DB-PURE11" PARNAME = "DNSDIP" COMPI = "WT" COMPJ = "" VALUE = ( 
"5.30300000E+01" "-7.84090000E-03" "0.E0" "0.E0" "0.E0" "2.33150000E+02" 
"2.73150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNSDIP" COMPI = "AC" 
COMPJ = "" VALUE = ( "1.66770000E+01" "0.E0" "0.E0" "0.E0" "0.E0" 
"1.74150000E+02" "1.74150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNSDIP" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "1.04000000E+01" "0.E0" "0.E0" "0.E0" 
"0.E0" "1.89150000E+02" "1.89150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME
 = "KLDIP" COMPI = "WT" COMPJ = "" VALUE = ( "-4.32000000E-01" "5.72550000E-03" 
"-8.07800000E-06" "1.86100000E-09" "0.E0" "2.73160000E+02" "6.33150000E+02" ) 
/  REGCASE = "DB-PURE11" PARNAME = "KLDIP" COMPI = "AC" COMPJ = "" VALUE = ( 
"2.87800000E-01" "-4.27000000E-04" "0.E0" "0.E0" "0.E0" "1.78450000E+02" 
"3.43150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "KLDIP" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "2.30100000E-01" "-2.88990000E-04" "0.E0" "0.E0" "0.E0" 
"1.89150000E+02" "4.51420000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "KVDIP" 
COMPI = "WT" COMPJ = "" VALUE = ( "2.16060000E-03" "7.68390000E-01" 
"3.94050000E+03" "-4.45340000E+05" "0.E0" "2.73160000E+02" "1.07315000E+03" ) 
/  REGCASE = "DB-PURE11" PARNAME = "KVDIP" COMPI = "AC" COMPJ = "" VALUE = ( 
"-2.68000000E+01" "9.09800000E-01" "-1.26500000E+08" "0.E0" "0.E0" 
"3.29440000E+02" "1.00000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "KVDIP" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "-2.48330000E+06" "-4.65170000E-02" 
"1.31310000E+09" "-1.57980000E+13" "0.E0" "3.89650000E+02" "1.00000000E+03" ) 
/  REGCASE = "DB-PURE11" PARNAME = "MULDIP" COMPI = "WT" COMPJ = "" VALUE = ( 
"-5.28430000E+01" "3.70360000E+03" "5.86600000E+00" "-5.87900000E-29" 
"1.00000000E+01" "2.73160000E+02" "6.46150000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "MULDIP" COMPI = "AC" COMPJ = "" VALUE = ( "-1.49180000E+01" 
"1.02340000E+03" "5.96100000E-01" "0.E0" "0.E0" "1.90000000E+02" 
"3.29440000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "MULDIP" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "-1.13940000E+01" "1.16870000E+03" "-7.53900000E-03" 
"0.E0" "0.E0" "1.89150000E+02" "3.89150000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "MUVDIP" COMPI = "WT" COMPJ = "" VALUE = ( "6.18390000E-07" 
"6.77790000E-01" "8.47230000E+02" "-7.39300000E+04" "0.E0" "2.73160000E+02" 
"1.07315000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "MUVDIP" COMPI = "AC" 
COMPJ = "" VALUE = ( "3.10050000E-08" "9.76200000E-01" "2.31390000E+01" "0.E0" 
"0.E0" "1.78450000E+02" "1.00000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME
 = "MUVDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( "9.42570000E-08" 
"7.84500000E-01" "9.01830000E+01" "0.E0" "0.E0" "1.89150000E+02" 
"1.00000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "NOATOM" COMPI = "WT" 
COMPJ = "" VALUE = ( "2.00000000E+00" "1.00000000E+00" ) /  REGCASE = 
"DB-PURE11" PARNAME = "NOATOM" COMPI = "AC" COMPJ = "" VALUE = ( 
"3.00000000E+00" "6.00000000E+00" "1.00000000E+00" ) /  REGCASE = "DB-PURE11" 
PARNAME = "NOATOM" COMPI = "MIBK" COMPJ = "" VALUE = ( "6.00000000E+00" 
"1.20000000E+01" "1.00000000E+00" ) /  REGCASE = "DB-PURE11" PARNAME = "PLXANT" 
COMPI = "WT" COMPJ = "" VALUE = ( "7.36490000E+01" "-7.25820000E+03" "0.E0" 
"0.E0" "-7.30370000E+00" "4.16530000E-06" "2.00000000E+00" "2.73160000E+02" 
"6.47130000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "PLXANT" COMPI = "AC" 
COMPJ = "" VALUE = ( "6.90060000E+01" "-5.59960000E+03" "0.E0" "0.E0" 
"-7.09850000E+00" "6.22370000E-06" "2.00000000E+00" "1.78450000E+02" 
"5.08200000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "PLXANT" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "8.05030000E+01" "-7.42180000E+03" "0.E0" "0.E0" 
"-8.37900000E+00" "1.81140000E-17" "6.00000000E+00" "1.89150000E+02" 
"5.74600000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "SIGDIP" COMPI = "WT" 
COMPJ = "" VALUE = ( "1.85480000E-01" "2.71700000E+00" "-3.55400000E+00" 
"2.04700000E+00" "0.E0" "2.73160000E+02" "6.47130000E+02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "SIGDIP" COMPI = "AC" COMPJ = "" VALUE = ( 
"6.22000000E-02" "1.12400000E+00" "0.E0" "0.E0" "0.E0" "1.78450000E+02" 
"5.08200000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "SIGDIP" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "5.89840000E-02" "1.26250000E+00" "0.E0" "0.E0" "0.E0" 
"1.89150000E+02" "5.74600000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "WATSOL" 
COMPI = "WT" COMPJ = "" VALUE = ( "1.76831707E+00" "-2.28297799E+03" "0.E0" 
"0.E0" "9.24912773E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "WATSOL" COMPI
 = "AC" COMPJ = "" VALUE = ( "2.42843628E+00" "-2.57076553E+03" "0.E0" "0.E0" 
"8.21741377E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "WATSOL" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "7.54214324E+00" "-4.39199842E+03" "0.E0" "0.E0" 
"5.32870916E+02" ) \ ? PROPERTIES PARAMETERS UNARY SCALAR "REVIEW-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = API SETNO = 1 UNITROW = 0 /  PARAMNAME
 = DGFORM SETNO = 1 UNITROW = 39 UNITLABEL = "cal/mol" /  PARAMNAME = DHFORM 
SETNO = 1 UNITROW = 39 UNITLABEL = "cal/mol" /  PARAMNAME = DHVLB SETNO = 1 
UNITROW = 39 UNITLABEL = "cal/mol" /  PARAMNAME = HCOM SETNO = 1 UNITROW = 39 
UNITLABEL = "cal/mol" /  PARAMNAME = MUP SETNO = 1 UNITROW = 45 UNITLABEL = 
debye /  PARAMNAME = MW SETNO = 1 UNITROW = 0 /  PARAMNAME = OMEGA SETNO = 1 
UNITROW = 0 /  PARAMNAME = PC SETNO = 1 UNITROW = 20 UNITLABEL = atm /  
PARAMNAME = RKTZRA SETNO = 1 UNITROW = 0 /  PARAMNAME = SG SETNO = 1 UNITROW
 = 0 /  PARAMNAME = TB SETNO = 1 UNITROW = 22 UNITLABEL = K /  PARAMNAME = TC 
SETNO = 1 UNITROW = 22 UNITLABEL = K /  PARAMNAME = VB SETNO = 1 UNITROW = 43 
UNITLABEL = "cc/mol" /  PARAMNAME = VC SETNO = 1 UNITROW = 43 UNITLABEL = 
"cc/mol" /  PARAMNAME = VLSTD SETNO = 1 UNITROW = 43 UNITLABEL = "cc/mol" /  
PARAMNAME = ZC SETNO = 1 UNITROW = 0 \ \ PVAL PARAMNAME2 = API CID = WT VALUE 
= DB-PURE11 \ \ PVAL PARAMNAME2 = API CID = AC VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = API CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DGFORM 
CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DGFORM CID = AC VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = DGFORM CID = MIBK VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DHFORM CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHFORM 
CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHFORM CID = MIBK VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = DHVLB CID = WT VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DHVLB CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHVLB CID
 = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = HCOM CID = WT VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = HCOM CID = AC VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = HCOM CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = MUP CID
 = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = MUP CID = AC VALUE = DB-PURE11 
\ \ PVAL PARAMNAME2 = MUP CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = 
MW CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = MW CID = AC VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = MW CID = MIBK VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = OMEGA CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = OMEGA CID
 = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = OMEGA CID = MIBK VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = PC CID = WT VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = PC CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = PC CID = 
MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = RKTZRA CID = WT VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = RKTZRA CID = AC VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = RKTZRA CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = SG CID
 = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = SG CID = AC VALUE = DB-PURE11 \ 
\ PVAL PARAMNAME2 = SG CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TB 
CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TB CID = AC VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = TB CID = MIBK VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = TC CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TC CID = AC 
VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TC CID = MIBK VALUE = DB-PURE11 \ \ 
PVAL PARAMNAME2 = VB CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VB CID
 = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VB CID = MIBK VALUE = DB-PURE11 
\ \ PVAL PARAMNAME2 = VC CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VC 
CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VC CID = MIBK VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = VLSTD CID = WT VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = VLSTD CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VLSTD CID
 = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = ZC CID = WT VALUE = DB-PURE11 
\ \ PVAL PARAMNAME2 = ZC CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = ZC 
CID = MIBK VALUE = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" 
"ATOMNO-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = ATOMNO SETNO = 1 UNITROW
 = 0 TUNITROW = 0 NEL = 10 \ \ PVAL PARAMNAME2 = ATOMNO CID = WT UNITROW2 = 0 
TUNITROW2 = 0 NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = 
DB-PURE11 VAL9 = DB-PURE11 VAL10 = DB-PURE11 \ \ PVAL PARAMNAME2 = ATOMNO CID
 = AC UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = ATOMNO CID = MIBK UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "CPIGDP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = CPIGDP SETNO = 1 UNITROW = 15 UNITLABEL
 = "cal/mol-K" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = 
CPIGDP CID = WT UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = CPIGDP CID = AC UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = CPIGDP CID = MIBK UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "CPSDIP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = CPSDIP SETNO = 1 UNITROW = 15 UNITLABEL
 = "cal/mol-K" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = 
CPSDIP CID = WT UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = CPSDIP CID = AC UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = CPSDIP CID = MIBK UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "DHVLDP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = DHVLDP SETNO = 1 UNITROW = 39 UNITLABEL
 = "cal/mol" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = 
DHVLDP CID = WT UNITROW2 = 39 UNITLABEL2 = "cal/mol" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DHVLDP CID = AC UNITROW2 = 39 UNITLABEL2 = "cal/mol" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = DHVLDP CID = MIBK UNITROW2 = 39 UNITLABEL2 = "cal/mol" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "DNLDIP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = DNLDIP SETNO = 1 UNITROW = 37 UNITLABEL
 = "mol/cc" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = DNLDIP 
CID = WT UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = 
DNLDIP CID = AC UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DNLDIP CID = MIBK UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "DNSDIP-1" ? ; "MET_MOLE" ; \ 
PROP-LIST PARAMNAME = DNSDIP SETNO = 1 UNITROW = 37 UNITLABEL = "mol/cc" 
TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = DNSDIP CID = WT 
UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = DNSDIP CID
 = AC UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K NEL2
 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 
= DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = DNSDIP 
CID = MIBK UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS 
UNARY "T-DEPENDENT" "KLDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = KLDIP 
SETNO = 1 UNITROW = 23 UNITLABEL = "kcal-m/hr-sqm-K" TUNITROW = 22 TUNITLABEL
 = K NEL = 7 \ \ PVAL PARAMNAME2 = KLDIP CID = WT UNITROW2 = 23 UNITLABEL2 = 
"kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 
VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = 
DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KLDIP CID = AC UNITROW2 = 23 
UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KLDIP CID = MIBK 
UNITROW2 = 23 UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS 
UNARY "T-DEPENDENT" "KVDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = KVDIP 
SETNO = 1 UNITROW = 23 UNITLABEL = "kcal-m/hr-sqm-K" TUNITROW = 22 TUNITLABEL
 = K NEL = 7 \ \ PVAL PARAMNAME2 = KVDIP CID = WT UNITROW2 = 23 UNITLABEL2 = 
"kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 
VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = 
DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KVDIP CID = AC UNITROW2 = 23 
UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KVDIP CID = MIBK 
UNITROW2 = 23 UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS 
UNARY "T-DEPENDENT" "MULDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = 
MULDIP SETNO = 1 UNITROW = 26 UNITLABEL = cP TUNITROW = 22 TUNITLABEL = K NEL
 = 7 \ \ PVAL PARAMNAME2 = MULDIP CID = WT UNITROW2 = 26 UNITLABEL2 = cP 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = MULDIP CID = AC UNITROW2 = 26 UNITLABEL2 = cP 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = MULDIP CID = MIBK UNITROW2 = 26 UNITLABEL2 = 
cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "MUVDIP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = MUVDIP SETNO = 1 UNITROW = 26 UNITLABEL
 = cP TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = MUVDIP CID
 = WT UNITROW2 = 26 UNITLABEL2 = cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = MUVDIP CID
 = AC UNITROW2 = 26 UNITLABEL2 = cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = MUVDIP CID
 = MIBK UNITROW2 = 26 UNITLABEL2 = cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY 
"T-DEPENDENT" "NOATOM-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = NOATOM 
SETNO = 1 UNITROW = 0 TUNITROW = 0 NEL = 10 \ \ PVAL PARAMNAME2 = NOATOM CID
 = WT UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = NOATOM CID = AC UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = NOATOM CID = MIBK UNITROW2 = 0 TUNITROW2 = 0 
NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = 
DB-PURE11 VAL10 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" 
"PLXANT-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = PLXANT SETNO = 1 UNITROW
 = 20 UNITLABEL = atm TUNITROW = 22 TUNITLABEL = K NEL = 9 \ \ PVAL 
PARAMNAME2 = PLXANT CID = WT UNITROW2 = 20 UNITLABEL2 = atm TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 9 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = 
DB-PURE11 VAL9 = DB-PURE11 \ \ PVAL PARAMNAME2 = PLXANT CID = AC UNITROW2 = 20 
UNITLABEL2 = atm TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 9 VAL1 = DB-PURE11 
VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = 
DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = PLXANT CID = MIBK UNITROW2 = 20 UNITLABEL2 = atm TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 9 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = 
DB-PURE11 VAL9 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" 
"SIGDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = SIGDIP SETNO = 1 UNITROW
 = 21 UNITLABEL = "dyne/cm" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL 
PARAMNAME2 = SIGDIP CID = WT UNITROW2 = 21 UNITLABEL2 = "dyne/cm" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = SIGDIP CID = AC UNITROW2 = 21 UNITLABEL2 = "dyne/cm" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = SIGDIP CID = MIBK UNITROW2 = 21 UNITLABEL2 = 
"dyne/cm" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = 
DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 
VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "WATSOL-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = WATSOL SETNO = 1 UNITROW = 0 TUNITROW = 0 
NEL = 5 \ \ PVAL PARAMNAME2 = WATSOL CID = WT UNITROW2 = 0 TUNITROW2 = 0 NEL2
 = 5 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 
= DB-PURE11 \ \ PVAL PARAMNAME2 = WATSOL CID = AC UNITROW2 = 0 TUNITROW2 = 0 
NEL2 = 5 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 \ \ PVAL PARAMNAME2 = WATSOL CID = MIBK UNITROW2 = 0 
TUNITROW2 = 0 NEL2 = 5 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 \ ? PROPERTIES PARAMETERS BINARY SCALAR 
"PRKIJ-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = PRKIJ SETNO = 1 BDBANK = ( 
"EOS-LIT" ) \ ? PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" 
; \ PROP-LIST PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = ANDKIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 
\ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL
 = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL
 = atm TUNITROW = 22 TUNITLABEL = K BDBANK = ( BINARY HENRY ) NEL = 6 \ ? 
PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "NRTL-1" ? ; "MET_MOLE" ; \ 
PROP-LIST PARAMNAME = NRTL SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = K 
BDBANK = ( "VLE-IG" "LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL PARAMNAME2 = 
NRTL CID1 = WT CID2 = AC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = 
VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG 
VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 
= VLE-IG /  PARAMNAME2 = NRTL CID1 = WT CID2 = MIBK UNITROW2 = 0 TUNITROW2 = 
22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG 
VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = AC CID2 = 
MIBK UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = WT CID2 = BUOH UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = AC CID2 = 
BUOH UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = MIBK CID2 = BUOH UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = WT CID2 = 
NBAC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = AC CID2 = NBAC UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = BUOH CID2 = 
NBAC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG \ ? 
PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "NRTL-2" ? ; "MET_MOLE" ; \ 
PROP-LIST PARAMNAME = NRTL SETNO = 2 UNITROW = 0 TUNITROW = 22 TUNITLABEL = K 
BDBANK = ( "VLE-IG" "LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL PARAMNAME2 = 
NRTL CID1 = WT CID2 = AC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = 
VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG 
VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 
= VLE-IG /  PARAMNAME2 = NRTL CID1 = WT CID2 = MIBK UNITROW2 = 0 TUNITROW2 = 
22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG 
VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = WT CID2 = 
BUOH UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = WT CID2 = NBAC UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = AC CID2 = 
MIBK UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = AC CID2 = BUOH UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = AC CID2 = 
NBAC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = MIBK CID2 = BUOH UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = BUOH CID2 = 
NBAC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG \ ? 
"PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 ID = 
MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 ID = 
RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 ID = 
PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 ID
 = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID
 = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL 1 ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 50. <22> <4> PRES
 = 1. <20> <3> BASIS = "MASS-FRAC" FLOWBASE = MASS TOTFLOW = 10. <-80> <3> 
TOTAL = 1. <-89> <0> JUNK = 1 \ \ MOLE-FLOW SSID1 = MIXED CID = WT FLOW = 1. 
<-3> <0> \ ? STREAM MATERIAL 2 ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP
 = 100. <22> <4> PRES = 1. <20> <5> BASIS = "MASS-FRAC" FLOWBASE = MASS 
TOTFLOW = 15. <-80> <3> TOTAL = 1. <-89> <0> JUNK = 2 \ \ MOLE-FLOW SSID1 = 
MIXED CID = BUOH FLOW = 0.6 <-3> <0> /  SSID1 = MIXED CID = NBAC FLOW = 0.4 
<-3> <0> \ ? STREAM MATERIAL 3 ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP
 = 80. <22> <4> PRES = 1. <20> <5> BASIS = "MASS-FRAC" FLOWBASE = MASS 
TOTFLOW = 10. <-80> <3> TOTAL = 1. <-89> <0> JUNK = 1 \ \ MOLE-FLOW SSID1 = 
MIXED CID = NBAC FLOW = 1. <-3> <0> \ ? BLOCK MIXER MIXER ? ; "MET_MOLE" ; ; 
TRIANGLE ; \ PARAM PRES = 1. <20> <5> \ ? BLOCK PUMP PUMP ? ; "MET_MOLE" ; ; 
ICON1 ; \ PARAM PRES = 20. <20> <5> OPT-SPEC = PRES \ ? BLOCK VALVE VALVE ? ; 
"MET_MOLE" ; ; VALVE ; \ PARAM P-OUT = 2. <20> <5> \ ? "EO-CONV-OPTI" ? \ 
DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = SIMULATION \ \ DMO-PARAMS 
MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE = RECONCILIATION \ \ 
DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L = DEFAULT \ \ 
LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFLOW = MOLEFLOW MOLEFRAC = MOLEFRAC 
MASSFRAC = MASSFRAC \ ? REPORT "FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? \ 
OPTIONS PARPLUS = "NOPARAM-PLUS" \ ? REPORT "ADA-REPORT" ? ? REPORT 
"BATCH-OPERAT" ? ; "MET_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 0
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6375
browserwidth 11745
browsertreewidth 5025
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 10
SIZE -6.77431 2.07853 -1.03044 1.09683
BLOCK
ID: MIXER
Version: 1
ICON: "TRIANGLE"
Flag 0
Section GLOBAL
At -4.800000 0.450000
Label At -0.006335 0.646833
Scale 1.000000 Modifier 0
BLOCK
ID: PUMP
Version: 1
ICON: "ICON1"
Flag 0
Section GLOBAL
At -2.350000 0.500000
Label At -0.003318 0.445937
Scale 1.000000 Modifier 0
BLOCK
ID: VALVE
Version: 1
ICON: "VALVE"
Flag 0
Section GLOBAL
At 0.294991 0.645002
Label At 0.002525 0.204212
Scale 1.983225 Modifier 0
STREAM
ID: 1
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -6.621025 0.855749
Label At 0.665894 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -6.621025 0.855749
x x -5.873175 0.855749
y y -5.873175 0.841403
x x -5.307240 0.841403
t l -5.107240 0.841403
$ D -0.006934 0.392523
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: 2
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -6.703422 0.495262
Label At 0.800918 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -6.703422 0.495262
x x -5.296681 0.495262
t l -5.096681 0.495262
$ D 0.003625 0.046382
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: 3
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -6.672523 0.103876
Label At 0.772471 0.020599
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -6.672523 0.103876
x x -5.900052 0.103876
y y -5.900052 0.124476
x x -5.296681 0.124476
t l -5.096681 0.124476
$ D 0.003625 -0.324404
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: 4
Version: 1
Flag 0
Port 0 MIXER o1
TYPE 0 TERMINAL 0
At -3.253049 0.495262
Label At -0.268966 0.000000
ROUTE 0 0
r r -3.253049 0.495262
x y -3.553049 0.495262
y x -3.553049 0.448879
x 0 -4.299695 0.448879
t r -4.499694 0.448879
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
r r -3.253049 0.495262
x x -2.799518 0.495262
y x -2.799518 0.499514
t l -2.599518 0.499514
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: 5
Version: 1
Flag 0
TYPE 0 TERMINAL 0
At -0.785942 0.731477
Label At 0.075125 0.000000
ROUTE 0 0
r r -0.785942 0.731477
x y -1.073442 0.731477
y x -1.073442 0.724739
x 0 -1.774404 0.724739
t r -1.974404 0.724739
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
r r -0.785942 0.731477
x x -0.348191 0.731477
t l -0.148191 0.731477
$ D 0.003043 0.086475
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: 6
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At 2.002866 0.623384
Label At -0.660400 0.021619
ROUTE 0 0
r l 2.002866 0.623384
x y 1.375000 0.623384
y x 1.375000 0.645002
x 0 0.941217 0.645002
t r 0.741217 0.645002
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.85249 -3.2 -3.04509 -3.36526
Size: 0.0108093
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -9.238840 4.359301 1.574605 -3.203120
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.010809

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "FaraDars" "FARADARS_PC"
 )                                                                              
 DSET RUN-STATUS IT @IT ( "NOVEMBER 27, 2016   4:06:29 P.M." "_5655tdh.inm" 0)  
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (WT AC MIBK BUOH NBAC)                               
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_5655tdh")                                      
 DSET RUN-STATUS RUNID @RUNID ("_5655tdh")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "NOVEMBER 27, 2016 4:06:29 P.M." )                    
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "SIMULATION" )                                  
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (12 123 "ASA-1" "ASA" )                       
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (1.80152800D+01 5.80800400D+01 1.00160680D+02 7.41228000D+01    
 1.16160080D+02)                                                                
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (2.89133265D-01 <2> 1.18530542D+00 <2> 2.01493048D+00 <2>    
 1.46250974D+00 <2> 2.12424047D+00 <2> )                                        
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (2.12000002D+02 <2> 1.33322003D+02 <2> 2.40800002D+02 <2>       
 2.43788002D+02 <2> 2.58998002D+02 <2> )                                        
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (0.D0 <2> 0.D0 <2> 0.D0 <2> 0.D0 <2> 0.D0 <2> 0.D0 0.D0    
 0.D0 0.D0 0.D0 0.D0 <2> 0.D0 0.D0 <2> 0.D0 -2.51369716D+02 <2>                 
 -9.96047026D-04)                                                               
 DSET ALIAS @ALIAS ( "H2O" "C3H6O-1" "C6H12O-2" "C4H10O-1" "C6H12O2-1" )        
 IDSET ID_1 (NPOINT) (#5)                                                       
 IDSET ID_2 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)                
 LSET L_1 (%ID_2 & %ID_1)                                                       
 DSET COMPONENTS MAIN COMPS @L_1 ("WT" C "H2O" "H2O" "WT" "AC" C "C3H6O-1"      
 "C3H6O-1" "AC" "MIBK" C "C6H12O-2" "C6H12O-2" "MIBK" "BUOH" C "C4H10O-1"       
 "C4H10O-1" "BUOH" "NBAC" C "C6H12O2-1" "C6H12O2-1" "NBAC" )                    
 IDSET ID_3 (PROPERTIES) (31 *2 <22> 32 *2 <20> 2 *2 3 *2)                      
 IDSET ID_4 (PROPERTIES) (298 *2 <75> )                                         
 LSET L_2 (%ID_RXBAL %ID_3 %ID_KODE %ID_4)                                      
 DSET BLOCK MIXER MIXER BLKSTAT @BLKSTAT (0 0)                                  
 DSET BLOCK MIXER MIXER COMPSTAT @L1 (0)                                        
 DSET BLOCK MIXER MIXER BLKIN @BLKIN (3 1 2 3)                                  
 DSET BLOCK MIXER MIXER TYPIN @TYPIN (3 MATERIAL MATERIAL MATERIAL)             
 DSET BLOCK MIXER MIXER BLKOUT @BLKOUT (1 4)                                    
 DSET BLOCK MIXER MIXER TYPOUT @TYPOUT (1 MATERIAL)                             
 DSET BLOCK MIXER MIXER MIX_RES @L_2 (1.79510392D+00 <2> 1.79510392D+00 <2>     
 0.D0 <2> 0.D0 7.71617927D+01 <2> 7.71617927D+01 <2> * <2> 0.D0 * <2> * <2> *   
 <2> * 1.79510392D+00 <2> 1.79510392D+00 <2> 0.D0 <2> 0.D0 7.71617927D+01 <2>   
 7.71617927D+01 <2> * <2> 0.D0 -2.52367317D+05 <2> -2.52367317D+05 <2> * <2>    
 0.D0 1.69246115D+02 <2> 1.45037738D+01 <2> 0.D0 1.00000000D+00 9 0.D0 <2> )    
 IDSET ID_5 (PROPERTIES) (22 *2 <19> 15 *2 <19> 16 *2 <19> 17 *2 <47> 19 *2 <12>
 357 *2 <33> 20 *2 <75> 21 *2 183 *2 <75> 30106 *2 30107 *2 <33> 30119 *2 <33>  
 24 *2 <20> 142 *2 4 *2 <1> 400 *2 <33> 298 *2 <75> 112 *2 <19> 990 *1 )        
 LSET L_3 (%ID_RXBAL %ID_5 %ID_KODE)                                            
 DSET BLOCK PUMP PUMP BLKSTAT @BLKSTAT (0 0)                                    
 DSET BLOCK PUMP PUMP COMPSTAT @L1 (0)                                          
 DSET BLOCK PUMP PUMP BLKIN @BLKIN (1 4)                                        
 DSET BLOCK PUMP PUMP TYPIN @TYPIN (1 MATERIAL)                                 
 DSET BLOCK PUMP PUMP BLKOUT @BLKOUT (1 5)                                      
 DSET BLOCK PUMP PUMP TYPOUT @TYPOUT (1 MATERIAL)                               
 DSET BLOCK PUMP PUMP RES_W @L_3 (1.79510392D+00 <2> 1.79510392D+00 <2> 0.D0 <2>
 0.D0 7.71617927D+01 <2> 7.71617927D+01 <2> * <2> 0.D0 * <2> * <2> * <2> *      
 1.79510392D+00 <2> 1.79510392D+00 <2> 0.D0 <2> 0.D0 7.71617927D+01 <2>         
 7.71617927D+01 <2> * <2> 0.D0 -2.52367317D+05 <2> -2.52115947D+05 <2> * <2>    
 -9.96047026D-04 9.87920133D-02 <2> 2.92086131D-02 <2> 9.87920133D-02 <2>       
 7.36691915D-02 <2> 1.45740084D+00 <2> 2.62035887D+01 <2> 2.75571701D+02 <2>    
 2.95657636D-01 2.75571701D+02 <2> 1.00000000D+00 * <2> 7.49503743D+02 <2>      
 2.90075475D+02 <2> 2.00000000D+01 * <2> * <2> * <2> * <2> 0 3)                 
 IDSET ID_6 (PROPERTIES) (1037 *1 1038 *2 <20> 1039 *2 1040 *2 1041 *2 <75>     
 1042 *2 <20> 1043 *2 1046 *2 1045 *2 1049 *2)                                  
 LSET L_4 (%ID_RXBAL %ID_6)                                                     
 DSET BLOCK VALVE VALVE BLKSTAT @BLKSTAT (0 0)                                  
 DSET BLOCK VALVE VALVE COMPSTAT @L1 (0)                                        
 DSET BLOCK VALVE VALVE BLKIN @BLKIN (1 5)                                      
 DSET BLOCK VALVE VALVE TYPIN @TYPIN (1 MATERIAL)                               
 DSET BLOCK VALVE VALVE BLKOUT @BLKOUT (1 6)                                    
 DSET BLOCK VALVE VALVE TYPOUT @TYPOUT (1 MATERIAL)                             
 DSET BLOCK VALVE VALVE RES_Q @L_4 (1.79510392D+00 <2> 1.79510392D+00 <2> 0.D0  
 <2> 0.D0 7.71617927D+01 <2> 7.71617927D+01 <2> * <2> 0.D0 * <2> * <2> * <2> *  
 1.79510392D+00 <2> 1.79510392D+00 <2> 0.D0 <2> 0.D0 7.71617927D+01 <2>         
 7.71617927D+01 <2> * <2> 0.D0 -2.52115947D+05 <2> -2.52115947D+05 <2> * <2>    
 0.D0 1 2.90075475D+01 <2> * * 2.61067928D+02 <2> * <2> * * * 1.00000000D+00)   
 IDSET ID_7 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )      
 LSET L_5 ( %ID_7 )                                                             
 IDSET ID_8 (PROPERTIES) (253 *2)                                               
 IDSET ID_9 (PROPERTIES) (253 *2 <11> )                                         
 IDSET ID_10 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_11 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_12 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_13 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_14 (PROPERTIES) (8101 *2 <11> 8002 *2 8004 *2 )                       
 IDSET ID_15 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_6 ( %ISODES (( %ID_NCC & %ID_14 %ID_15) & %IDS_1) )                     
 DSET STREAM MATERIAL 1 STR_MAIN @L_6 (* MIXER LIQUID 1.22375153D+00 <2> 0.D0   
 <2> 0.D0 <2> 0.D0 <2> 0.D0 <2> 1.00000000D+00 0.D0 0.D0 0.D0 0.D0              
 1.00000000D+00 0.D0 0.D0 0.D0 0.D0 1.22375153D+00 <2> 2.20462265D+01 <2>       
 3.64416527D-01 <2> 1.22000003D+02 <2> 1.46959488D+01 <2> 0.D0 1.00000000D+00   
 0.D0 -1.22058306D+05 <2> -6.77526552D+03 <2> -1.49369038D+05 <2>               
 -3.75011844D+01 <2> -2.08163206D+00 <2> 3.35811213D+00 <2> 6.04973303D+01 <2>  
 1.80152800D+01 3.53827274D-01 <2> )                                            
 DSET STREAM MATERIAL 1 RES_STR @L_5 (1.22000003D+02 <2> 1.46959488D+01 <2>     
 2.20462265D+01 <2> 3.64416527D-01 <2> 1.22375153D+00 <2> 0.D0 )                
 DSET STREAM MATERIAL 2 STR_MAIN @L_6 (* MIXER LIQUID 0.D0 <2> 0.D0 <2> 0.D0 <2>
 2.67685568D-01 <2> 1.13875058D-01 <2> 0.D0 0.D0 0.D0 7.01554483D-01            
 2.98445517D-01 0.D0 0.D0 0.D0 6.00000000D-01 4.00000000D-01 3.81560627D-01 <2> 
 3.30693397D+01 <2> 7.01827396D-01 <2> 2.12000002D+02 <2> 1.45037738D+01 <2>    
 0.D0 1.00000000D+00 0.D0 -1.59419081D+05 <2> -1.83940910D+03 <2>               
 -6.08280443D+04 <2> -1.29145917D+02 <2> -1.49011131D+00 <2> 5.43667342D-01 <2> 
 4.71189079D+01 <2> 8.66686378D+01 6.33390755D-01 <2> )                         
 DSET STREAM MATERIAL 2 RES_STR @L_5 (2.12000002D+02 <2> 1.45037738D+01 <2>     
 3.30693397D+01 <2> 7.01827396D-01 <2> 3.81560627D-01 <2> 0.D0 )                
 DSET STREAM MATERIAL 3 STR_MAIN @L_6 (* MIXER LIQUID 0.D0 <2> 0.D0 <2> 0.D0 <2>
 0.D0 <2> 1.89791764D-01 <2> 0.D0 0.D0 0.D0 0.D0 1.00000000D+00 0.D0 0.D0 0.D0  
 0.D0 1.00000000D+00 1.89791764D-01 <2> 2.20462265D+01 <2> 4.37253249D-01 <2>   
 1.76000003D+02 <2> 1.45037738D+01 <2> 0.D0 1.00000000D+00 0.D0 -2.22192124D+05 
 <2> -1.91280967D+03 <2> -4.21702351D+04 <2> -1.56112167D+02 <2>                
 -1.34393990D+00 <2> 4.34054563D-01 <2> 5.04198128D+01 <2> 1.16160080D+02       
 4.03163344D-01 <2> )                                                           
 DSET STREAM MATERIAL 3 RES_STR @L_5 (1.76000003D+02 <2> 1.45037738D+01 <2>     
 2.20462265D+01 <2> 4.37253249D-01 <2> 1.89791764D-01 <2> 0.D0 )                
 DSET STREAM MATERIAL 4 STR_MAIN @L_6 (MIXER PUMP LIQUID 1.22375153D+00 <2>     
 0.D0 <2> 0.D0 <2> 2.67685568D-01 <2> 3.03666822D-01 <2> 6.81716260D-01 0.D0    
 0.D0 1.49119817D-01 1.69163923D-01 2.85714286D-01 0.D0 0.D0 2.57142857D-01     
 4.57142857D-01 1.79510392D+00 <2> 7.71617927D+01 <2> 1.45740084D+00 <2>        
 1.69246115D+02 <2> 1.45037738D+01 <2> 0.D0 1.00000000D+00 0.D0 -1.40586467D+05 
 <2> -3.27062539D+03 <2> -2.52367317D+05 <2> -6.80340155D+01 <2>                
 -1.58275390D+00 <2> 1.23171602D+00 <2> 5.29447988D+01 <2> 4.29845825D+01       
 1.39038137D+00 <2> )                                                           
 DSET STREAM MATERIAL 4 RES_STR @L_5 (1.69246115D+02 <2> 1.45037738D+01 <2>     
 7.71617927D+01 <2> 1.45740084D+00 <2> 1.79510392D+00 <2> 0.D0 )                
 DSET STREAM MATERIAL 5 STR_MAIN @L_6 (PUMP VALVE LIQUID 1.22375153D+00 <2>     
 0.D0 <2> 0.D0 <2> 2.67685568D-01 <2> 3.03666822D-01 <2> 6.81716260D-01 0.D0    
 0.D0 1.49119817D-01 1.69163923D-01 2.85714286D-01 0.D0 0.D0 2.57142857D-01     
 4.57142857D-01 1.79510392D+00 <2> 7.71617927D+01 <2> 1.46269543D+00 <2>        
 1.73787635D+02 <2> 2.90075475D+02 <2> 0.D0 1.00000000D+00 0.D0 -1.40446436D+05 
 <2> -3.26736769D+03 <2> -2.52115947D+05 <2> -6.78136729D+01 <2>                
 -1.57762781D+00 <2> 1.22725752D+00 <2> 5.27531522D+01 <2> 4.29845825D+01       
 1.39038137D+00 <2> )                                                           
 DSET STREAM MATERIAL 5 RES_STR @L_5 (1.73787635D+02 <2> 2.90075475D+02 <2>     
 7.71617927D+01 <2> 1.46269543D+00 <2> 1.79510392D+00 <2> 0.D0 )                
 DSET STREAM MATERIAL 6 STR_MAIN @L_6 (VALVE * LIQUID 1.22375153D+00 <2> 0.D0   
 <2> 0.D0 <2> 2.67685568D-01 <2> 3.03666822D-01 <2> 6.81716260D-01 0.D0 0.D0    
 1.49119817D-01 1.69163923D-01 2.85714286D-01 0.D0 0.D0 2.57142857D-01          
 4.57142857D-01 1.79510392D+00 <2> 7.71617927D+01 <2> 1.46269545D+00 <2>        
 1.73787655D+02 <2> 2.90075475D+01 <2> 0.D0 1.00000000D+00 0.D0 -1.40446436D+05 
 <2> -3.26736769D+03 <2> -2.52115947D+05 <2> -6.78136719D+01 <2>                
 -1.57762779D+00 <2> 1.22725750D+00 <2> 5.27531513D+01 <2> 4.29845825D+01       
 1.39038137D+00 <2> )                                                           
 DSET STREAM MATERIAL 6 RES_STR @L_5 (1.73787655D+02 <2> 2.90075475D+01 <2>     
 7.71617927D+01 <2> 1.46269545D+00 <2> 1.79510392D+00 <2> 0.D0 )                
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET ID_16 (NPOINT) ( #5)                                                     
 IDSET ID_17 (PROPERTIES) (747 *6)                                              
 LSET L_7 ( %ID_16 & %ID_17)                                                    
 DSET RUN-STATUS ERRTXT @L_7 (                                                  
 "The following messages were issued during Input Translation:"                 
 ""                                                                             
 "   INFORMATION"                                                               
 "   BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD"                    
 "   ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD"                       
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
