MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Mon Nov 14 10:08:40 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
RCSTR
RCSTR
Built-In
RCSTR
? SETUP MAIN ? \ TITLE TITLE = "reaction 3" \ \ SIMULATE INTERACTIVE = NO 
MOLEFLOW = NOMOLEFLOW MOLEFRAC = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? 
SETUP GLOBAL ? \ "IN-UNITS" INSET = ENG \ \ "STREAM-CLASS" SCLASS = CONVEN \ 
? SETUP DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP 
"CUSTOM-UOM" ? ? SETUP "UNITS-SET" METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = A PROJECT-ID = A PROJECT-NAME = "A" USER-NAME = "A" \ ? 
SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ DESCRIP DESCRIP = ( 
"General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = AN ANAME = C6H7N-1 OUTNAME = AN TYPE
 = CONV DBNAME1 = "ANILINE" ANAME1 = "C6H7N-1" /  CID = H2 ANAME = H2 OUTNAME
 = H2 TYPE = CONV DBNAME1 = "HYDROGEN" ANAME1 = "H2" /  CID = CHA ANAME = 
C6H13N-D1 OUTNAME = CHA TYPE = CONV DBNAME1 = "CYCLOHEXYLAMINE" ANAME1 = 
"C6H13N-D1" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET GLOBAL 
? \ BLOCK BLKID = RCSTR BLKTYPE = RCSTR IN = ( AN M0-1 H2 M0-1 ) OUT = ( 
PRODUCT M0-1 ) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? PROPERTIES MAIN ? \ 
GPROPERTIES GBASEOPSET = "PENG-ROB" GOPSETNAME = "PENG-ROB" PARCON = -2 \ ? 
PROPERTIES "OPTION-SETS" MXBONNEL ? \ PARAM BASE = MXBONNEL \ ? PROPERTIES 
"OPTION-SETS" NRTL ? \ PARAM BASE = NRTL \ ? PROPERTIES "OPTION-SETS" 
"PENG-ROB" ? \ PARAM BASE = "PENG-ROB" \ ? PROPERTIES "OPTION-SETS" SRK ? \ 
PARAM BASE = SRK \ ? PROPERTIES "OPTION-SETS" UNIFAC ? \ PARAM BASE = UNIFAC 
\ ? PROPERTIES "MOLEC-STRUCT" AN ? ? PROPERTIES "MOLEC-STRUCT" CHA ? ? 
PROPERTIES "MOLEC-STRUCT" H2 ? ? PROPERTIES PARAMETERS BINARY SCALAR "PRKIJ-1" 
? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = PRKIJ SETNO = 1 BDBANK = ( "EOS-LIT" 
) \ ? PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS 
BINARY SCALAR "SRKAIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = SRKAIJ 
SETNO = 1 \ ? PROPERTIES PARAMETERS BINARY SCALAR "SRKBIJ-1" ? ; "ENG_MOLE" ; 
\ PROP-LIST PARAMNAME = SRKBIJ SETNO = 1 UNITROW = 22 UNITLABEL = F \ ? 
PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = ANDKIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL
 = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; 
"ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 
22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" 
"HENRY-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = HENRY SETNO = 1 UNITROW = 
20 UNITLABEL = psi TUNITROW = 22 TUNITLABEL = F BDBANK = ( BINARY HENRY ) NEL
 = 6 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "NRTL-1" ? ; "ENG_MOLE" ; 
\ PROP-LIST PARAMNAME = NRTL SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL
 = F BDBANK = ( "VLE-IG" "LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL 
PARAMNAME2 = NRTL CID1 = AN CID2 = CHA UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = F VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG \ ? PROPERTIES PARAMETERS UNIBINARY 
SCALAR "GMUFB-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = GMUFB SETNO = 1 \ ? 
"PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 ID = 
MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 ID = 
RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 ID = 
PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 ID
 = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID
 = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL AN ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 100. <22> <2> 
PRES = 650. <20> <2> TOTAL = 100. <-89> <0> JUNK = 1 \ \ MOLE-FLOW SSID1 = 
MIXED CID = AN FLOW = 100. <-89> <2> \ ? STREAM MATERIAL H2 ? ; "ENG_MOLE" ; 
\ SUBSTREAM SSID = MIXED TEMP = 100. <22> <2> PRES = 650. <20> <2> TOTAL = 
400. <-89> <0> JUNK = 1 \ \ MOLE-FLOW SSID1 = MIXED CID = H2 FLOW = 400. 
<-89> <2> \ ? "STREAM-SUM" ? ? BLOCK RCSTR RCSTR ? ; "ENG_MOLE" ; ; ICON1 ; \ 
PARAM SPEC-TYPE = "TOT-VOL-PH-VOL-FRAC" VOL = 1200. <27> <2> TEMP = 250. <22> 
<2> PRES = 595. <20> <2> NPHASE = 2 SPEC-PHASE = CONDENSED REACT-VOL-FR = 0.8 
<0> <0> \ \ PRODUCTS SID = PRODUCT \ \ "BLOCK-OPTION" BLKOPFREWAT = NO \ \ 
REACTIONS RXN-ID = ( "R-1" ) \ ? "EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT 
\ \ DMO-PARAMS MODE = SIMULATION \ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" 
\ \ DMO-PARAMS MODE = RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ 
LSSQP-PARAMS MODE-L = DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ 
LSSQP-PARAMS MODE-L = "PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = 
RECONCILIATION \ \ LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? 
REPORT "BLOCK-REPORT" ? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFLOW = 
NOMOLEFLOW MOLEFRAC = MOLEFRAC \ ? REPORT "FLOWSHEET-RE" ? ? REPORT 
"PROPERTY-REP" ? ? REPORT "ADA-REPORT" ? ? REPORT "BATCH-OPERAT" ? ; "ENG_MOLE" 
; ? REACTIONS POWERLAW "R-1" ? ; "ENG_MOLE" ; \ REAC-DATA R-D-REACNO = 1 
PRE-EXP = 1750. <0> <0> ACT-ENERGY = 11111. <39> <3> \ \ STOIC REACNO = 1 
STOIC-CID = AN STOIC-SUBS = MIXED COEF = -1. <0> <0> EXPONENT = 1. <0> <0> /  
REACNO = 1 STOIC-CID = H2 STOIC-SUBS = MIXED COEF = -3. <0> <0> EXPONENT = 1. 
<0> <0> \ \ STOIC1 REACNO1 = 1 STOIC-CID1 = CHA STOIC-SUBS1 = MIXED COEF1 = 
1. <0> <0> \ \ FORCONTROL FCVAR1 = CHA \ 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6465
browserwidth 11970
browsertreewidth 5250
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 6
SIZE -11.95 0.704532 -4.45 1.44759
BLOCK
ID: RCSTR
Version: 1
ICON: "ICON1"
Flag 0
Section GLOBAL
At -2.706160 0.401294
Label At 0.123566 0.311796
Annotation At -0.450000 -0.638000
Scale 2.882353 Modifier 0
STREAM
ID: AN
Version: 1
Flag 0
Port 1 RCSTR i1
TYPE 0 TERMINAL 1
At -5.551528 0.705702
Label At 0.388264 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -5.551528 0.705702
x x -4.775000 0.705702
y y -4.775000 0.733881
x x -4.205678 0.733881
t l -4.005678 0.733881
$ D 0.000437 0.332264
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: H2
Version: 1
Flag 0
Port 1 RCSTR i1
TYPE 0 TERMINAL 1
At -5.645621 -0.302444
Label At 0.410311 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -5.645621 -0.302444
x x -4.825000 -0.302444
y y -4.825000 -0.233940
x x -4.205678 -0.233940
t l -4.005678 -0.233940
$ D 0.000437 -0.635556
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: PRODUCT
Version: 1
Flag 0
Port 0 RCSTR o1
TYPE 0 TERMINAL 2
At 0.547491 0.396537
Label At -0.486245 0.000000
ROUTE 0 0
r l 0.547491 0.396537
x y -0.425000 0.396537
y x -0.425000 0.401616
x 0 -1.198938 0.401616
t r -1.398938 0.401616
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -0.6 -2.7 0.879052 -3.14757
Size: 0.00513295
Font: 1 0 =Times New Roman
TABLE
Version: 2
CanUpdate: 1
Dim: -11.95 -1.6 -8.15 -4.45
Size: 1 0.00513295
Font: 1 0 =Times New Roman
Tag
Tag
11 3
2 0
5
1
0
0
0
0
0
0
0
0
Stream ID
To
From
Phase
Stream ID
To
From
Phase
reaction 3

PRODUCT
AN
H2

RCSTR
RCSTR
RCSTR


MIXED
LIQUID
VAPOR
Temperature
Pressure
Vapor Frac
Mole Flow
Mass Flow
Volume Flow
Enthalpy
Mole Frac
  AN
  H2
  CHA
F
psi

lbmol/hr
lb/hr
cuft/hr
MMBtu/hr




     250.0
     100.0
     100.0
    595.00
    650.00
    650.00
     0.660
     0.000
     1.000
   290.055
   100.000
   400.000
 10119.184
  9312.832
   806.352
  2679.301
   147.753
  3774.998
    -2.896
     1.598
     0.069
 
 
 
     0.103
     1.000
          
     0.655
          
     1.000
     0.241
          
          
# of PFS Objects = 0
VIEWPORT -9.048066 -2.149386 -1.874595 -4.394871
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.005133

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "Hossein Khakpour"      
 "HOSSEINKHAKPOUR" )                                                            
 DSET RUN-STATUS IT @IT ( "NOVEMBER 14, 2016   10:05:15 A.M." "_0154ynx.inm" 0) 
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (AN H2 CHA)                                          
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_0154ynx")                                      
 DSET RUN-STATUS RUNID @RUNID ("_0154ynx")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "NOVEMBER 14, 2016 10:05:15 A.M." )                   
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "REACTION 3" )                                  
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (A A "A" "A" )                                
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (9.31283200D+01 2.01588000D+00 9.91759600D+01)                  
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (1.46774778D+00 <2> 8.57913662D-01 <2> 1.84165876D+00 <2> )  
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (3.63200001D+02 <2> -4.22967993D+02 <2> 2.74100002D+02 <2> )    
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (6.99816655D+01 <2> 2.09944997D+02 <2> -6.99816655D+01 <2> 
 6.99816655D-01 5.24862492D-01 -1.00000000D+00 2.09944997D+02 <2> 0.D0          
 -1.81898940D-12 <2> -1.79756530D-16 4.56300954D+06 <2> 1.57557904D+00)         
 DSET ALIAS @ALIAS ( "C6H7N-1" "H2" "C6H13N-D1" )                               
 IDSET ID_12 (NPOINT) (#3)                                                      
 IDSET ID_13 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)               
 LSET L_4 (%ID_13 & %ID_12)                                                     
 DSET COMPONENTS MAIN COMPS @L_4 ("AN" C "C6H7N-1" "C6H7N-1" "AN" "H2" C "H2"   
 "H2" "H2" "CHA" C "C6H13N-D1" "C6H13N-D1" "CHA" )                              
 IDSET ID_14 (PROPERTIES) (1 *2 <13> 31 *2 <22> 1052 *2 <13> 515 *2 <27> 148 *2 
 <24> 1053 *2 <27> 1054 *2 <27> 1055 *2 <27> 1056 *2 <27> 1057 *2 <27> 1058 *2  
 <24> 1059 *2 <24> )                                                            
 LSET L_5 (%ID_RXBAL %ID_14)                                                    
 DSET BLOCK RCSTR RCSTR BLKSTAT @BLKSTAT (0 0)                                  
 DSET BLOCK RCSTR RCSTR COMPSTAT @L1 (0)                                        
 DSET BLOCK RCSTR RCSTR BLKIN @BLKIN (2 AN H2)                                  
 DSET BLOCK RCSTR RCSTR TYPIN @TYPIN (2 MATERIAL MATERIAL)                      
 DSET BLOCK RCSTR RCSTR BLKOUT @BLKOUT (1 PRODUCT)                              
 DSET BLOCK RCSTR RCSTR TYPOUT @TYPOUT (1 MATERIAL)                             
 DSET BLOCK RCSTR RCSTR RES_Q @L_5 (5.00000000D+02 <2> 2.90055003D+02 <2>       
 -2.09944997D+02 <2> 0.D0 1.01191840D+04 <2> 1.01191840D+04 <2> * <2>           
 -1.79756530D-16 * <2> * <2> * <2> * 5.00000000D+02 <2> 2.90055003D+02 <2>      
 -2.09944997D+02 <2> 0.D0 1.01191840D+04 <2> 1.01191840D+04 <2> * <2>           
 -1.79756530D-16 1.66692536D+06 <2> -2.89608418D+06 <2> * <2> 1.57557904D+00    
 -4.56300954D+06 <2> 2.50000000D+02 <2> -4.56300954D+06 <2> 1.20000000D+03 <2>  
 4.47878042D-01 <2> 2.40000000D+02 <2> 9.60000000D+02 <2> * <2> * <2>           
 9.60000000D+02 <2> 9.62830613D-02 <2> 5.14330190D+00 <2> )                     
 IDSET ID_15 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )     
 LSET L_6 ( %ID_15 )                                                            
 IDSET ID_16 (PROPERTIES) (253 *2)                                              
 IDSET ID_17 (PROPERTIES) (253 *2 <11> )                                        
 IDSET ID_18 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_19 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_20 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_21 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_22 (PROPERTIES) (8002 *2 )                                            
 IDSET ID_23 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_7 ( %ISODES (( %ID_NCC & %ID_22 %ID_23) & %IDS_1) )                     
 DSET STREAM MATERIAL AN STR_MAIN @L_7 (* RCSTR LIQUID 1.00000000D+00 0.D0 0.D0 
 1.00000000D+02 <2> 9.31283200D+03 <2> 1.47753307D+02 <2> 1.00000000D+02 <2>    
 6.50000000D+02 <2> 0.D0 1.00000000D+00 0.D0 1.59841661D+04 <2> 1.71635933D+02  
 <2> 1.59841660D+06 <2> -9.05531208D+01 <2> -9.72347840D-01 <2> 6.76803818D-01  
 <2> 6.30296025D+01 <2> 9.31283200D+01 1.46774777D+02 <2> )                     
 DSET STREAM MATERIAL AN RES_STR @L_6 (1.00000000D+02 <2> 6.50000000D+02 <2>    
 9.31283200D+03 <2> 1.47753307D+02 <2> 1.00000000D+02 <2> 0.D0 )                
 DSET STREAM MATERIAL H2 STR_MAIN @L_7 (* RCSTR VAPOR 0.D0 1.00000000D+00 0.D0  
 4.00000000D+02 <2> 8.06352000D+02 <2> 3.77499766D+03 <2> 1.00000000D+02 <2>    
 6.50000000D+02 <2> 1.00000000D+00 0.D0 0.D0 1.71271897D+02 <2> 8.49613551D+01  
 <2> 6.85087584D+04 <2> -7.25536049D+00 <2> -3.59910336D+00 <2> 1.05960333D-01  
 <2> 2.13603316D-01 <2> 2.01588000D+00 3.43165462D+02 <2> )                     
 DSET STREAM MATERIAL H2 RES_STR @L_6 (1.00000000D+02 <2> 6.50000000D+02 <2>    
 8.06352000D+02 <2> 3.77499766D+03 <2> 4.00000000D+02 <2> 1.00000000D+00 )      
 DSET STREAM MATERIAL PRODUCT STR_MAIN @L_7 (RCSTR * MIXED 1.03491869D-01       
 6.55237804D-01 2.41270327D-01 2.90055003D+02 <2> 1.01191840D+04 <2>            
 2.67930085D+03 <2> 2.50000000D+02 <2> 5.95000000D+02 <2> 6.60242337D-01        
 3.39757663D-01 0.D0 -9.98460345D+03 <2> -2.86197404D+02 <2> -2.89608418D+06 <2>
 -5.03248476D+01 <2> -1.44250503D+00 <2> 1.08257723D-01 <2> 3.77680028D+00 <2>  
 3.48871210D+01 3.35992473D+02 <2> )                                            
 DSET STREAM MATERIAL PRODUCT RES_STR @L_6 (2.50000000D+02 <2> 5.95000000D+02   
 <2> 1.01191840D+04 <2> 2.67930085D+03 <2> 2.90055003D+02 <2> 6.60242337D-01 )  
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET ID_24 (NPOINT) ( #5)                                                     
 IDSET ID_25 (PROPERTIES) (747 *6)                                              
 LSET L_8 ( %ID_24 & %ID_25)                                                    
 DSET RUN-STATUS ERRTXT @L_8 (                                                  
 "The following messages were issued during Input Translation:"                 
 ""                                                                             
 "   INFORMATION"                                                               
 "   BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD"                    
 "   ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD"                       
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
