MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Sun Nov 27 16:54:51 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
FLASH
Flash2
Built-In
FLASH2
? SETUP MAIN ? \ TITLE TITLE = "simulation" \ \ SIMULATE INTERACTIVE = NO 
MOLEFLOW = MOLEFLOW MOLEFRAC = MOLEFRAC MASSFRAC = MASSFRAC TFFFILE = "GEN_M" 
VISITED = 1 \ ? SETUP GLOBAL ? \ "IN-UNITS" INSET = MET OUTSET = MET \ \ 
"STREAM-CLASS" SCLASS = CONVEN \ ? SETUP DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" 
? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = 12 PROJECT-ID = 123 PROJECT-NAME = "ASA-1" USER-NAME = 
"FLASH DRUM" \ ? SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ DESCRIP 
DESCRIP = ( "General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = WT ANAME = H2O OUTNAME = WT TYPE = 
CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  CID = AC ANAME = C3H6O-1 OUTNAME = 
AC TYPE = CONV DBNAME1 = "ACETONE" ANAME1 = "C3H6O-1" /  CID = MIBK ANAME = 
C6H12O-2 OUTNAME = MIBK DBNAME1 = "METHYL-ISOBUTYL-KETONE" ANAME1 = "C6H12O-2" 
/  CID = BUOH ANAME = C4H10O-1 OUTNAME = BUOH TYPE = CONV DBNAME1 = "N-BUTANOL" 
ANAME1 = "C4H10O-1" /  CID = NBAC ANAME = C6H12O2-1 OUTNAME = NBAC DBNAME1 = 
"N-BUTYL-ACETATE" ANAME1 = "C6H12O2-1" /  CID = ACT ANAME = C2H4O2-1 OUTNAME
 = ACT TYPE = CONV DBNAME1 = "ACETIC-ACID" ANAME1 = "C2H4O2-1" \ ? COMPONENTS 
"COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET GLOBAL ? \ BLOCK BLKID = FLASH 
BLKTYPE = FLASH2 IN = ( FEED M0-1 ) OUT = ( ACT M0-1 WT M1-2 ) \ \ "DEF-STREAM" 
SCLASS = CONVEN \ ? PROPERTIES MAIN ? \ GPROPERTIES GBASEOPSET = NRTL 
GOPSETNAME = NRTL PARCON = -2 \ ? PROPERTIES "OPTION-SETS" IDEAL ? \ PARAM 
BASE = IDEAL \ ? PROPERTIES "OPTION-SETS" NRTL ? \ PARAM BASE = NRTL \ ? 
PROPERTIES "OPTION-SETS" "NRTL-HOC" ? \ PARAM BASE = "NRTL-HOC" \ ? 
PROPERTIES "OPTION-SETS" "PENG-ROB" ? \ PARAM BASE = "PENG-ROB" \ ? 
PROPERTIES "MOLEC-STRUCT" AC ? ? PROPERTIES "MOLEC-STRUCT" ACT ? ? PROPERTIES 
"MOLEC-STRUCT" BUOH ? ? PROPERTIES "MOLEC-STRUCT" MIBK ? ? PROPERTIES 
"MOLEC-STRUCT" NBAC ? ? PROPERTIES "MOLEC-STRUCT" WT ? ? PROPERTIES REGPAR ? 
\ FRED REGCASE = "DB-PURE11" PARNAME = "API" COMPI = "WT" COMPJ = "" VALUE = 
( "1.00000000E+01" ) /  REGCASE = "DB-PURE11" PARNAME = "API" COMPI = "AC" 
COMPJ = "" VALUE = ( "4.85000000E+01" ) /  REGCASE = "DB-PURE11" PARNAME = 
"API" COMPI = "MIBK" COMPJ = "" VALUE = ( "4.57562000E+01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DGFORM" COMPI = "WT" COMPJ = "" VALUE = ( 
"-2.28590000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = "DGFORM" COMPI = "AC" 
COMPJ = "" VALUE = ( "-1.51300000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = 
"DGFORM" COMPI = "MIBK" COMPJ = "" VALUE = ( "-1.35100000E+08" ) /  REGCASE
 = "DB-PURE11" PARNAME = "DHFORM" COMPI = "WT" COMPJ = "" VALUE = ( 
"-2.41814000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = "DHFORM" COMPI = "AC" 
COMPJ = "" VALUE = ( "-2.15700000E+08" ) /  REGCASE = "DB-PURE11" PARNAME = 
"DHFORM" COMPI = "MIBK" COMPJ = "" VALUE = ( "-2.86400000E+08" ) /  REGCASE
 = "DB-PURE11" PARNAME = "DHVLB" COMPI = "WT" COMPJ = "" VALUE = ( 
"4.07992000E+07" ) /  REGCASE = "DB-PURE11" PARNAME = "DHVLB" COMPI = "AC" 
COMPJ = "" VALUE = ( "2.95566000E+07" ) /  REGCASE = "DB-PURE11" PARNAME = 
"DHVLB" COMPI = "MIBK" COMPJ = "" VALUE = ( "3.45593000E+07" ) /  REGCASE = 
"DB-PURE11" PARNAME = "HCOM" COMPI = "WT" COMPJ = "" VALUE = ( "0.E0" ) /  
REGCASE = "DB-PURE11" PARNAME = "HCOM" COMPI = "AC" COMPJ = "" VALUE = ( 
"-1.65900000E+09" ) /  REGCASE = "DB-PURE11" PARNAME = "HCOM" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "-3.47620000E+09" ) /  REGCASE = "DB-PURE11" PARNAME = 
"MUP" COMPI = "WT" COMPJ = "" VALUE = ( "5.84934000E-25" ) /  REGCASE = 
"DB-PURE11" PARNAME = "MUP" COMPI = "AC" COMPJ = "" VALUE = ( "9.11056000E-25" 
) /  REGCASE = "DB-PURE11" PARNAME = "MUP" COMPI = "MIBK" COMPJ = "" VALUE = 
( "8.50382000E-25" ) /  REGCASE = "DB-PURE11" PARNAME = "MW" COMPI = "WT" 
COMPJ = "" VALUE = ( "1.80152800E+01" ) /  REGCASE = "DB-PURE11" PARNAME = "MW" 
COMPI = "AC" COMPJ = "" VALUE = ( "5.80800400E+01" ) /  REGCASE = "DB-PURE11" 
PARNAME = "MW" COMPI = "MIBK" COMPJ = "" VALUE = ( "1.00160680E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "OMEGA" COMPI = "WT" COMPJ = "" VALUE = ( 
"3.44861000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "OMEGA" COMPI = "AC" 
COMPJ = "" VALUE = ( "3.06527000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = 
"OMEGA" COMPI = "MIBK" COMPJ = "" VALUE = ( "3.55671000E-01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "PC" COMPI = "WT" COMPJ = "" VALUE = ( "2.20550000E+07" 
) /  REGCASE = "DB-PURE11" PARNAME = "PC" COMPI = "AC" COMPJ = "" VALUE = ( 
"4.70100000E+06" ) /  REGCASE = "DB-PURE11" PARNAME = "PC" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "3.27000000E+06" ) /  REGCASE = "DB-PURE11" PARNAME = 
"RKTZRA" COMPI = "WT" COMPJ = "" VALUE = ( "2.43172000E-01" ) /  REGCASE = 
"DB-PURE11" PARNAME = "RKTZRA" COMPI = "AC" COMPJ = "" VALUE = ( 
"2.45200000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "RKTZRA" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "2.58900000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "SG" 
COMPI = "WT" COMPJ = "" VALUE = ( "1.00000000E+00" ) /  REGCASE = "DB-PURE11" 
PARNAME = "SG" COMPI = "AC" COMPJ = "" VALUE = ( "7.86000000E-01" ) /  
REGCASE = "DB-PURE11" PARNAME = "SG" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"7.98280000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "TB" COMPI = "WT" COMPJ
 = "" VALUE = ( "3.73150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "TB" 
COMPI = "AC" COMPJ = "" VALUE = ( "3.29440000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "TB" COMPI = "MIBK" COMPJ = "" VALUE = ( "3.89150000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "TC" COMPI = "WT" COMPJ = "" VALUE = ( 
"6.47130000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "TC" COMPI = "AC" COMPJ
 = "" VALUE = ( "5.08200000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "TC" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "5.74600000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "VB" COMPI = "WT" COMPJ = "" VALUE = ( "1.88308000E-02" ) /  
REGCASE = "DB-PURE11" PARNAME = "VB" COMPI = "AC" COMPJ = "" VALUE = ( 
"7.74659000E-02" ) /  REGCASE = "DB-PURE11" PARNAME = "VB" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "1.41450000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "VC" 
COMPI = "WT" COMPJ = "" VALUE = ( "5.59478000E-02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "VC" COMPI = "AC" COMPJ = "" VALUE = ( "2.09000000E-01" ) /  
REGCASE = "DB-PURE11" PARNAME = "VC" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"3.69000000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "VLSTD" COMPI = "WT" 
COMPJ = "" VALUE = ( "1.80500000E-02" ) /  REGCASE = "DB-PURE11" PARNAME = 
"VLSTD" COMPI = "AC" COMPJ = "" VALUE = ( "7.39962000E-02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "VLSTD" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"1.25788000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "ZC" COMPI = "WT" COMPJ
 = "" VALUE = ( "2.29000000E-01" ) /  REGCASE = "DB-PURE11" PARNAME = "ZC" 
COMPI = "AC" COMPJ = "" VALUE = ( "2.33000000E-01" ) /  REGCASE = "DB-PURE11" 
PARNAME = "ZC" COMPI = "MIBK" COMPJ = "" VALUE = ( "2.53000000E-01" ) /  
REGCASE = "DB-PURE11" PARNAME = "ATOMNO" COMPI = "WT" COMPJ = "" VALUE = ( 
"1.00000000E+00" "8.00000000E+00" ) /  REGCASE = "DB-PURE11" PARNAME = "ATOMNO" 
COMPI = "AC" COMPJ = "" VALUE = ( "6.00000000E+00" "1.00000000E+00" 
"8.00000000E+00" ) /  REGCASE = "DB-PURE11" PARNAME = "ATOMNO" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "6.00000000E+00" "1.00000000E+00" "8.00000000E+00" ) /  
REGCASE = "DB-PURE11" PARNAME = "CPIGDP" COMPI = "WT" COMPJ = "" VALUE = ( 
"3.33630000E+04" "2.67900000E+04" "2.61050000E+03" "8.89600000E+03" 
"1.16900000E+03" "1.00000000E+02" "2.27315000E+03" ) /  REGCASE = "DB-PURE11" 
PARNAME = "CPIGDP" COMPI = "AC" COMPJ = "" VALUE = ( "5.70400000E+04" 
"1.63200000E+05" "1.60700000E+03" "9.68000000E+04" "7.31500000E+02" 
"2.00000000E+02" "1.50000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "CPIGDP" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "1.22700000E+05" "2.19500000E+05" 
"8.42000000E+02" "1.19100000E+05" "2.46000000E+03" "2.98150000E+02" 
"1.50015000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "CPSDIP" COMPI = "WT" 
COMPJ = "" VALUE = ( "-2.62490000E+02" "1.40520000E+02" "0.E0" "0.E0" "0.E0" 
"3.15000000E+00" "2.73150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "CPSDIP" 
COMPI = "AC" COMPJ = "" VALUE = ( "-1.20000000E+04" "1.27600000E+03" 
"-6.17000000E+00" "1.32000000E-02" "0.E0" "3.00000000E+01" "1.78450000E+02" ) 
/  REGCASE = "DB-PURE11" PARNAME = "CPSDIP" COMPI = "MIBK" COMPJ = "" VALUE
 = ( "1.69000000E+05" "0.E0" "0.E0" "0.E0" "0.E0" "1.89150000E+02" 
"1.89150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DHVLDP" COMPI = "WT" 
COMPJ = "" VALUE = ( "5.20530000E+07" "3.19900000E-01" "-2.12000000E-01" 
"2.57950000E-01" "0.E0" "2.73160000E+02" "6.47130000E+02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DHVLDP" COMPI = "AC" COMPJ = "" VALUE = ( 
"4.21500000E+07" "3.39700000E-01" "0.E0" "0.E0" "0.E0" "1.78450000E+02" 
"5.08200000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DHVLDP" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "5.46870000E+07" "4.05830000E-01" "0.E0" "0.E0" "0.E0" 
"1.89150000E+02" "5.74600000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNLDIP" 
COMPI = "WT" COMPJ = "" VALUE = ( "1.78630000E+01" "5.86060000E+01" 
"-9.53960000E+01" "2.13890000E+02" "-1.41260000E+02" "2.73160000E+02" 
"6.47130000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNLDIP" COMPI = "AC" 
COMPJ = "" VALUE = ( "1.23320000E+00" "2.58860000E-01" "5.08200000E+02" 
"2.91300000E-01" "0.E0" "1.78450000E+02" "5.08200000E+02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DNLDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"7.16870000E-01" "2.64530000E-01" "5.74600000E+02" "2.89180000E-01" "0.E0" 
"1.89150000E+02" "5.74600000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "DNSDIP" 
COMPI = "WT" COMPJ = "" VALUE = ( "5.30300000E+01" "-7.84090000E-03" "0.E0" 
"0.E0" "0.E0" "2.33150000E+02" "2.73150000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "DNSDIP" COMPI = "AC" COMPJ = "" VALUE = ( "1.66770000E+01" "0.E0" 
"0.E0" "0.E0" "0.E0" "1.74150000E+02" "1.74150000E+02" ) /  REGCASE = 
"DB-PURE11" PARNAME = "DNSDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"1.04000000E+01" "0.E0" "0.E0" "0.E0" "0.E0" "1.89150000E+02" "1.89150000E+02" 
) /  REGCASE = "DB-PURE11" PARNAME = "KLDIP" COMPI = "WT" COMPJ = "" VALUE = 
( "-4.32000000E-01" "5.72550000E-03" "-8.07800000E-06" "1.86100000E-09" "0.E0" 
"2.73160000E+02" "6.33150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "KLDIP" 
COMPI = "AC" COMPJ = "" VALUE = ( "2.87800000E-01" "-4.27000000E-04" "0.E0" 
"0.E0" "0.E0" "1.78450000E+02" "3.43150000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "KLDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( "2.30100000E-01" 
"-2.88990000E-04" "0.E0" "0.E0" "0.E0" "1.89150000E+02" "4.51420000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "KVDIP" COMPI = "WT" COMPJ = "" VALUE = ( 
"2.16060000E-03" "7.68390000E-01" "3.94050000E+03" "-4.45340000E+05" "0.E0" 
"2.73160000E+02" "1.07315000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "KVDIP" 
COMPI = "AC" COMPJ = "" VALUE = ( "-2.68000000E+01" "9.09800000E-01" 
"-1.26500000E+08" "0.E0" "0.E0" "3.29440000E+02" "1.00000000E+03" ) /  
REGCASE = "DB-PURE11" PARNAME = "KVDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"-2.48330000E+06" "-4.65170000E-02" "1.31310000E+09" "-1.57980000E+13" "0.E0" 
"3.89650000E+02" "1.00000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "MULDIP" 
COMPI = "WT" COMPJ = "" VALUE = ( "-5.28430000E+01" "3.70360000E+03" 
"5.86600000E+00" "-5.87900000E-29" "1.00000000E+01" "2.73160000E+02" 
"6.46150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "MULDIP" COMPI = "AC" 
COMPJ = "" VALUE = ( "-1.49180000E+01" "1.02340000E+03" "5.96100000E-01" "0.E0" 
"0.E0" "1.90000000E+02" "3.29440000E+02" ) /  REGCASE = "DB-PURE11" PARNAME
 = "MULDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( "-1.13940000E+01" 
"1.16870000E+03" "-7.53900000E-03" "0.E0" "0.E0" "1.89150000E+02" 
"3.89150000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "MUVDIP" COMPI = "WT" 
COMPJ = "" VALUE = ( "6.18390000E-07" "6.77790000E-01" "8.47230000E+02" 
"-7.39300000E+04" "0.E0" "2.73160000E+02" "1.07315000E+03" ) /  REGCASE = 
"DB-PURE11" PARNAME = "MUVDIP" COMPI = "AC" COMPJ = "" VALUE = ( 
"3.10050000E-08" "9.76200000E-01" "2.31390000E+01" "0.E0" "0.E0" 
"1.78450000E+02" "1.00000000E+03" ) /  REGCASE = "DB-PURE11" PARNAME = "MUVDIP" 
COMPI = "MIBK" COMPJ = "" VALUE = ( "9.42570000E-08" "7.84500000E-01" 
"9.01830000E+01" "0.E0" "0.E0" "1.89150000E+02" "1.00000000E+03" ) /  REGCASE
 = "DB-PURE11" PARNAME = "NOATOM" COMPI = "WT" COMPJ = "" VALUE = ( 
"2.00000000E+00" "1.00000000E+00" ) /  REGCASE = "DB-PURE11" PARNAME = "NOATOM" 
COMPI = "AC" COMPJ = "" VALUE = ( "3.00000000E+00" "6.00000000E+00" 
"1.00000000E+00" ) /  REGCASE = "DB-PURE11" PARNAME = "NOATOM" COMPI = "MIBK" 
COMPJ = "" VALUE = ( "6.00000000E+00" "1.20000000E+01" "1.00000000E+00" ) /  
REGCASE = "DB-PURE11" PARNAME = "PLXANT" COMPI = "WT" COMPJ = "" VALUE = ( 
"7.36490000E+01" "-7.25820000E+03" "0.E0" "0.E0" "-7.30370000E+00" 
"4.16530000E-06" "2.00000000E+00" "2.73160000E+02" "6.47130000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "PLXANT" COMPI = "AC" COMPJ = "" VALUE = ( 
"6.90060000E+01" "-5.59960000E+03" "0.E0" "0.E0" "-7.09850000E+00" 
"6.22370000E-06" "2.00000000E+00" "1.78450000E+02" "5.08200000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "PLXANT" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"8.05030000E+01" "-7.42180000E+03" "0.E0" "0.E0" "-8.37900000E+00" 
"1.81140000E-17" "6.00000000E+00" "1.89150000E+02" "5.74600000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "SIGDIP" COMPI = "WT" COMPJ = "" VALUE = ( 
"1.85480000E-01" "2.71700000E+00" "-3.55400000E+00" "2.04700000E+00" "0.E0" 
"2.73160000E+02" "6.47130000E+02" ) /  REGCASE = "DB-PURE11" PARNAME = "SIGDIP" 
COMPI = "AC" COMPJ = "" VALUE = ( "6.22000000E-02" "1.12400000E+00" "0.E0" 
"0.E0" "0.E0" "1.78450000E+02" "5.08200000E+02" ) /  REGCASE = "DB-PURE11" 
PARNAME = "SIGDIP" COMPI = "MIBK" COMPJ = "" VALUE = ( "5.89840000E-02" 
"1.26250000E+00" "0.E0" "0.E0" "0.E0" "1.89150000E+02" "5.74600000E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "WATSOL" COMPI = "WT" COMPJ = "" VALUE = ( 
"1.76831707E+00" "-2.28297799E+03" "0.E0" "0.E0" "9.24912773E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "WATSOL" COMPI = "AC" COMPJ = "" VALUE = ( 
"2.42843628E+00" "-2.57076553E+03" "0.E0" "0.E0" "8.21741377E+02" ) /  
REGCASE = "DB-PURE11" PARNAME = "WATSOL" COMPI = "MIBK" COMPJ = "" VALUE = ( 
"7.54214324E+00" "-4.39199842E+03" "0.E0" "0.E0" "5.32870916E+02" ) \ ? 
PROPERTIES PARAMETERS UNARY SCALAR "REVIEW-1" ? ; "MET_MOLE" ; \ PROP-LIST 
PARAMNAME = API SETNO = 1 UNITROW = 0 /  PARAMNAME = DGFORM SETNO = 1 UNITROW
 = 39 UNITLABEL = "cal/mol" /  PARAMNAME = DHFORM SETNO = 1 UNITROW = 39 
UNITLABEL = "cal/mol" /  PARAMNAME = DHVLB SETNO = 1 UNITROW = 39 UNITLABEL
 = "cal/mol" /  PARAMNAME = HCOM SETNO = 1 UNITROW = 39 UNITLABEL = "cal/mol" 
/  PARAMNAME = MUP SETNO = 1 UNITROW = 45 UNITLABEL = debye /  PARAMNAME = MW 
SETNO = 1 UNITROW = 0 /  PARAMNAME = OMEGA SETNO = 1 UNITROW = 0 /  PARAMNAME
 = PC SETNO = 1 UNITROW = 20 UNITLABEL = atm /  PARAMNAME = RKTZRA SETNO = 1 
UNITROW = 0 /  PARAMNAME = SG SETNO = 1 UNITROW = 0 /  PARAMNAME = TB SETNO
 = 1 UNITROW = 22 UNITLABEL = K /  PARAMNAME = TC SETNO = 1 UNITROW = 22 
UNITLABEL = K /  PARAMNAME = VB SETNO = 1 UNITROW = 43 UNITLABEL = "cc/mol" 
/  PARAMNAME = VC SETNO = 1 UNITROW = 43 UNITLABEL = "cc/mol" /  PARAMNAME = 
VLSTD SETNO = 1 UNITROW = 43 UNITLABEL = "cc/mol" /  PARAMNAME = ZC SETNO = 1 
UNITROW = 0 \ \ PVAL PARAMNAME2 = API CID = WT VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = API CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = API CID = 
MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DGFORM CID = WT VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = DGFORM CID = AC VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DGFORM CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHFORM 
CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHFORM CID = AC VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = DHFORM CID = MIBK VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DHVLB CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHVLB CID
 = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = DHVLB CID = MIBK VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = HCOM CID = WT VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = HCOM CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = HCOM CID
 = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = MUP CID = WT VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = MUP CID = AC VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = MUP CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = MW CID = 
WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = MW CID = AC VALUE = DB-PURE11 \ \ 
PVAL PARAMNAME2 = MW CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = OMEGA 
CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = OMEGA CID = AC VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = OMEGA CID = MIBK VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = PC CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = PC CID = AC 
VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = PC CID = MIBK VALUE = DB-PURE11 \ \ 
PVAL PARAMNAME2 = RKTZRA CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = 
RKTZRA CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = RKTZRA CID = MIBK 
VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = SG CID = WT VALUE = DB-PURE11 \ \ 
PVAL PARAMNAME2 = SG CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = SG CID
 = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TB CID = WT VALUE = DB-PURE11 
\ \ PVAL PARAMNAME2 = TB CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TB 
CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = TC CID = WT VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = TC CID = AC VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = TC CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VB CID = 
WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VB CID = AC VALUE = DB-PURE11 \ \ 
PVAL PARAMNAME2 = VB CID = MIBK VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VC 
CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VC CID = AC VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = VC CID = MIBK VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = VLSTD CID = WT VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VLSTD CID
 = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = VLSTD CID = MIBK VALUE = 
DB-PURE11 \ \ PVAL PARAMNAME2 = ZC CID = WT VALUE = DB-PURE11 \ \ PVAL 
PARAMNAME2 = ZC CID = AC VALUE = DB-PURE11 \ \ PVAL PARAMNAME2 = ZC CID = 
MIBK VALUE = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "ATOMNO-1" 
? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = ATOMNO SETNO = 1 UNITROW = 0 
TUNITROW = 0 NEL = 10 \ \ PVAL PARAMNAME2 = ATOMNO CID = WT UNITROW2 = 0 
TUNITROW2 = 0 NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = 
DB-PURE11 VAL9 = DB-PURE11 VAL10 = DB-PURE11 \ \ PVAL PARAMNAME2 = ATOMNO CID
 = AC UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = ATOMNO CID = MIBK UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "CPIGDP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = CPIGDP SETNO = 1 UNITROW = 15 UNITLABEL
 = "cal/mol-K" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = 
CPIGDP CID = WT UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = CPIGDP CID = AC UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = CPIGDP CID = MIBK UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "CPSDIP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = CPSDIP SETNO = 1 UNITROW = 15 UNITLABEL
 = "cal/mol-K" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = 
CPSDIP CID = WT UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = CPSDIP CID = AC UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = CPSDIP CID = MIBK UNITROW2 = 15 UNITLABEL2 = "cal/mol-K" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "DHVLDP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = DHVLDP SETNO = 1 UNITROW = 39 UNITLABEL
 = "cal/mol" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = 
DHVLDP CID = WT UNITROW2 = 39 UNITLABEL2 = "cal/mol" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DHVLDP CID = AC UNITROW2 = 39 UNITLABEL2 = "cal/mol" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = DHVLDP CID = MIBK UNITROW2 = 39 UNITLABEL2 = "cal/mol" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "DNLDIP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = DNLDIP SETNO = 1 UNITROW = 37 UNITLABEL
 = "mol/cc" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = DNLDIP 
CID = WT UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = 
DNLDIP CID = AC UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = DNLDIP CID = MIBK UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "DNSDIP-1" ? ; "MET_MOLE" ; \ 
PROP-LIST PARAMNAME = DNSDIP SETNO = 1 UNITROW = 37 UNITLABEL = "mol/cc" 
TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = DNSDIP CID = WT 
UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = DNSDIP CID
 = AC UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K NEL2
 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 
= DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = DNSDIP 
CID = MIBK UNITROW2 = 37 UNITLABEL2 = "mol/cc" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS 
UNARY "T-DEPENDENT" "KLDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = KLDIP 
SETNO = 1 UNITROW = 23 UNITLABEL = "kcal-m/hr-sqm-K" TUNITROW = 22 TUNITLABEL
 = K NEL = 7 \ \ PVAL PARAMNAME2 = KLDIP CID = WT UNITROW2 = 23 UNITLABEL2 = 
"kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 
VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = 
DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KLDIP CID = AC UNITROW2 = 23 
UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KLDIP CID = MIBK 
UNITROW2 = 23 UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS 
UNARY "T-DEPENDENT" "KVDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = KVDIP 
SETNO = 1 UNITROW = 23 UNITLABEL = "kcal-m/hr-sqm-K" TUNITROW = 22 TUNITLABEL
 = K NEL = 7 \ \ PVAL PARAMNAME2 = KVDIP CID = WT UNITROW2 = 23 UNITLABEL2 = 
"kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 
VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = 
DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KVDIP CID = AC UNITROW2 = 23 
UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = KVDIP CID = MIBK 
UNITROW2 = 23 UNITLABEL2 = "kcal-m/hr-sqm-K" TUNITROW2 = 22 TUNITLABEL2 = K 
NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS 
UNARY "T-DEPENDENT" "MULDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = 
MULDIP SETNO = 1 UNITROW = 26 UNITLABEL = cP TUNITROW = 22 TUNITLABEL = K NEL
 = 7 \ \ PVAL PARAMNAME2 = MULDIP CID = WT UNITROW2 = 26 UNITLABEL2 = cP 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = MULDIP CID = AC UNITROW2 = 26 UNITLABEL2 = cP 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = MULDIP CID = MIBK UNITROW2 = 26 UNITLABEL2 = 
cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "MUVDIP-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = MUVDIP SETNO = 1 UNITROW = 26 UNITLABEL
 = cP TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL PARAMNAME2 = MUVDIP CID
 = WT UNITROW2 = 26 UNITLABEL2 = cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = MUVDIP CID
 = AC UNITROW2 = 26 UNITLABEL2 = cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ \ PVAL PARAMNAME2 = MUVDIP CID
 = MIBK UNITROW2 = 26 UNITLABEL2 = cP TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 
VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = 
DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY 
"T-DEPENDENT" "NOATOM-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = NOATOM 
SETNO = 1 UNITROW = 0 TUNITROW = 0 NEL = 10 \ \ PVAL PARAMNAME2 = NOATOM CID
 = WT UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = NOATOM CID = AC UNITROW2 = 0 TUNITROW2 = 0 NEL2 = 10 VAL1 = 
DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 
VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 VAL10 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = NOATOM CID = MIBK UNITROW2 = 0 TUNITROW2 = 0 
NEL2 = 10 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = 
DB-PURE11 VAL10 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" 
"PLXANT-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = PLXANT SETNO = 1 UNITROW
 = 20 UNITLABEL = atm TUNITROW = 22 TUNITLABEL = K NEL = 9 \ \ PVAL 
PARAMNAME2 = PLXANT CID = WT UNITROW2 = 20 UNITLABEL2 = atm TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 9 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = 
DB-PURE11 VAL9 = DB-PURE11 \ \ PVAL PARAMNAME2 = PLXANT CID = AC UNITROW2 = 20 
UNITLABEL2 = atm TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 9 VAL1 = DB-PURE11 
VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = 
DB-PURE11 VAL7 = DB-PURE11 VAL8 = DB-PURE11 VAL9 = DB-PURE11 \ \ PVAL 
PARAMNAME2 = PLXANT CID = MIBK UNITROW2 = 20 UNITLABEL2 = atm TUNITROW2 = 22 
TUNITLABEL2 = K NEL2 = 9 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 VAL8 = 
DB-PURE11 VAL9 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" 
"SIGDIP-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = SIGDIP SETNO = 1 UNITROW
 = 21 UNITLABEL = "dyne/cm" TUNITROW = 22 TUNITLABEL = K NEL = 7 \ \ PVAL 
PARAMNAME2 = SIGDIP CID = WT UNITROW2 = 21 UNITLABEL2 = "dyne/cm" TUNITROW2
 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = 
DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = DB-PURE11 
\ \ PVAL PARAMNAME2 = SIGDIP CID = AC UNITROW2 = 21 UNITLABEL2 = "dyne/cm" 
TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = DB-PURE11 
VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 VAL7 = 
DB-PURE11 \ \ PVAL PARAMNAME2 = SIGDIP CID = MIBK UNITROW2 = 21 UNITLABEL2 = 
"dyne/cm" TUNITROW2 = 22 TUNITLABEL2 = K NEL2 = 7 VAL1 = DB-PURE11 VAL2 = 
DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 = DB-PURE11 VAL6 = DB-PURE11 
VAL7 = DB-PURE11 \ ? PROPERTIES PARAMETERS UNARY "T-DEPENDENT" "WATSOL-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = WATSOL SETNO = 1 UNITROW = 0 TUNITROW = 0 
NEL = 5 \ \ PVAL PARAMNAME2 = WATSOL CID = WT UNITROW2 = 0 TUNITROW2 = 0 NEL2
 = 5 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 VAL5 
= DB-PURE11 \ \ PVAL PARAMNAME2 = WATSOL CID = AC UNITROW2 = 0 TUNITROW2 = 0 
NEL2 = 5 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 VAL4 = DB-PURE11 
VAL5 = DB-PURE11 \ \ PVAL PARAMNAME2 = WATSOL CID = MIBK UNITROW2 = 0 
TUNITROW2 = 0 NEL2 = 5 VAL1 = DB-PURE11 VAL2 = DB-PURE11 VAL3 = DB-PURE11 
VAL4 = DB-PURE11 VAL5 = DB-PURE11 \ ? PROPERTIES PARAMETERS BINARY SCALAR 
"HOCETA-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = HOCETA SETNO = 1 BDBANK
 = ( "EOS-LIT" ) \ \ BPVAL PARAMNAME2 = HOCETA CID1 = WT CID2 = WT VALUE = 
EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = WT CID2 = AC VALUE = EOS-LIT \ \ 
BPVAL PARAMNAME2 = HOCETA CID1 = WT CID2 = MIBK VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = WT CID2 = BUOH VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = WT CID2 = NBAC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = WT CID2 = ACT VALUE = EOS-LIT \ \ BPVAL PARAMNAME2
 = HOCETA CID1 = AC CID2 = WT VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA 
CID1 = AC CID2 = AC VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = AC 
CID2 = MIBK VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = AC CID2 = 
BUOH VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = AC CID2 = NBAC 
VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = AC CID2 = ACT VALUE = 
EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = MIBK CID2 = WT VALUE = EOS-LIT \ 
\ BPVAL PARAMNAME2 = HOCETA CID1 = MIBK CID2 = AC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = MIBK CID2 = MIBK VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = MIBK CID2 = BUOH VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = MIBK CID2 = NBAC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = MIBK CID2 = ACT VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = BUOH CID2 = WT VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = BUOH CID2 = AC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = BUOH CID2 = MIBK VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = BUOH CID2 = BUOH VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = BUOH CID2 = NBAC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = BUOH CID2 = ACT VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = NBAC CID2 = WT VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = NBAC CID2 = AC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = NBAC CID2 = MIBK VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = NBAC CID2 = BUOH VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = NBAC CID2 = NBAC VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = NBAC CID2 = ACT VALUE = EOS-LIT \ \ BPVAL 
PARAMNAME2 = HOCETA CID1 = ACT CID2 = WT VALUE = EOS-LIT \ \ BPVAL PARAMNAME2
 = HOCETA CID1 = ACT CID2 = AC VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA 
CID1 = ACT CID2 = MIBK VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = 
ACT CID2 = BUOH VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = ACT CID2
 = NBAC VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = ACT CID2 = ACT 
VALUE = EOS-LIT \ ? PROPERTIES PARAMETERS BINARY SCALAR "PRKIJ-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = PRKIJ SETNO = 1 BDBANK = ( "EOS-LIT" ) \ 
? PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 
\ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; "MET_MOLE" ; \ 
PROP-LIST PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL = atm TUNITROW
 = 22 TUNITLABEL = K BDBANK = ( BINARY HENRY ) NEL = 6 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "NRTL-1" ? ; "MET_MOLE" ; \ PROP-LIST 
PARAMNAME = NRTL SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = K BDBANK = 
( "VLE-IG" "LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL PARAMNAME2 = NRTL CID1
 = WT CID2 = AC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG 
VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = 
VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = 
VLE-IG /  PARAMNAME2 = NRTL CID1 = WT CID2 = MIBK UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = AC CID2 = 
MIBK UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = WT CID2 = BUOH UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = AC CID2 = 
BUOH UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = MIBK CID2 = BUOH UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = WT CID2 = 
NBAC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  
PARAMNAME2 = NRTL CID1 = AC CID2 = NBAC UNITROW2 = 0 TUNITROW2 = 22 
TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 
= VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = BUOH CID2 = 
NBAC UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG \ ? 
"PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 ID = 
MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 ID = 
RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 ID = 
PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 ID
 = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID
 = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 105. <22> <4> 
PRES = 1. <20> <3> BASIS = "MOLE-FRAC" TOTFLOW = 100. <-89> <3> TOTAL = 1. 
<-89> <0> JUNK = 2 \ \ MOLE-FLOW SSID1 = MIXED CID = WT FLOW = 0.5 <-4> <0> 
/  SSID1 = MIXED CID = ACT FLOW = 0.5 <-4> <0> \ ? "STREAM-SUM" ? ? BLOCK 
FLASH2 FLASH ? ; "MET_MOLE" ; ; "V-DRUM1" ; \ PARAM TEMP = 105. <22> <4> PRES
 = 1. <20> <3> \ ? "EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ 
DMO-PARAMS MODE = SIMULATION \ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ 
DMO-PARAMS MODE = RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ 
LSSQP-PARAMS MODE-L = DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ 
LSSQP-PARAMS MODE-L = "PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = 
RECONCILIATION \ \ LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? 
REPORT "BLOCK-REPORT" ? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFLOW = 
MOLEFLOW MOLEFRAC = MOLEFRAC MASSFRAC = MASSFRAC \ ? REPORT "FLOWSHEET-RE" ? 
? REPORT "PROPERTY-REP" ? \ OPTIONS PARPLUS = "NOPARAM-PLUS" \ ? REPORT 
"ADA-REPORT" ? ? REPORT "BATCH-OPERAT" ? ; "MET_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 0
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6375
browserwidth 11745
browsertreewidth 5025
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 5
SIZE -7.35 -1.10038 -5.65 0.855191
BLOCK
ID: FLASH
Version: 1
ICON: "V-DRUM1"
Flag 0
Section GLOBAL
At -2.650522 0.102435
Label At 0.150522 0.447565
Scale 1.000000 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
TYPE 0 TERMINAL 1
At -4.283011 0.061237
Label At 0.683012 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -4.283011 0.061237
x x -3.600000 0.061237
y y -3.600000 0.081836
x x -3.102862 0.081836
t l -2.902862 0.081836
$ D -0.002766 -0.019709
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: ACT
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At -1.182826 0.766761
Label At -0.638692 0.000000
ROUTE 0 0
r l -1.182826 0.766761
x y -2.650788 0.766761
y 0 -2.650788 0.702219
t u -2.650788 0.502219
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: WT
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At -1.368219 -0.597939
Label At -0.641285 0.000000
ROUTE 0 0
r l -1.368219 -0.597939
x y -2.650788 -0.597939
y 0 -2.650788 -0.495568
t d -2.650788 -0.295568
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.85249 -3.2 -3.08628 -3.35528
Size: 0.00954755
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -7.544985 4.465837 1.112975 -3.107044
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.009548

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "FaraDars" "FARADARS_PC"
 )                                                                              
 DSET RUN-STATUS IT @IT ( "NOVEMBER 27, 2016   4:46:35 P.M." "_2136yqy.inm" 0)  
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (WT AC MIBK BUOH NBAC ACT)                           
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_2136yqy")                                      
 DSET RUN-STATUS RUNID @RUNID ("_2136yqy")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "NOVEMBER 27, 2016 4:46:35 P.M." )                    
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "SIMULATION" )                                  
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (12 123 "ASA-1" "FLASH DRUM" )                
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (1.80152800D+01 5.80800400D+01 1.00160680D+02 7.41228000D+01    
 1.16160080D+02 6.00525600D+01)                                                 
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (1.80500000D+01 <3> 7.39962000D+01 <3> 1.25788000D+02 <3>    
 9.13015000D+01 <3> 1.32612000D+02 <3> 5.76314000D+01 <3> )                     
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (3.73150000D+02 <1> 3.29440000D+02 <1> 3.89150000D+02 <1>       
 3.90810000D+02 <1> 3.99260000D+02 <1> 3.91050000D+02 <1> )                     
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3>     
 0.D0 0.D0 0.D0 0.D0 0.D0 0.D0 0.D0 <3> 0.D0 0.D0 <3> 0.D0 0.D0 <3> 0.D0)       
 DSET ALIAS @ALIAS ( "H2O" "C3H6O-1" "C6H12O-2" "C4H10O-1" "C6H12O2-1"          
 "C2H4O2-1" )                                                                   
 IDSET ID_1 (NPOINT) (#6)                                                       
 IDSET ID_2 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)                
 LSET L_1 (%ID_2 & %ID_1)                                                       
 DSET COMPONENTS MAIN COMPS @L_1 ("WT" C "H2O" "H2O" "WT" "AC" C "C3H6O-1"      
 "C3H6O-1" "AC" "MIBK" C "C6H12O-2" "C6H12O-2" "MIBK" "BUOH" C "C4H10O-1"       
 "C4H10O-1" "BUOH" "NBAC" C "C6H12O2-1" "C6H12O2-1" "NBAC" "ACT" C "C2H4O2-1"   
 "C2H4O2-1" "ACT" )                                                             
 IDSET ID_3 (PROPERTIES) (1052 *2 <13> )                                        
 IDSET ID_4 (PROPERTIES) (298 *2 <75> )                                         
 LSET L_2 (%ID_RXBAL %ID_TPQV %ID_3 %ID_KODE %ID_4)                             
 DSET BLOCK FLASH2 FLASH BLKSTAT @BLKSTAT (0 0)                                 
 DSET BLOCK FLASH2 FLASH COMPSTAT @L1 (0)                                       
 DSET BLOCK FLASH2 FLASH BLKIN @BLKIN (1 FEED)                                  
 DSET BLOCK FLASH2 FLASH TYPIN @TYPIN (1 MATERIAL)                              
 DSET BLOCK FLASH2 FLASH BLKOUT @BLKOUT (2 ACT WT)                              
 DSET BLOCK FLASH2 FLASH TYPOUT @TYPOUT (2 MATERIAL MATERIAL)                   
 DSET BLOCK FLASH2 FLASH RES_Q @L_2 (1.00000000D+02 <3> 1.00000000D+02 <3> 0.D0 
 <3> 0.D0 3.90339200D+03 <3> 3.90339200D+03 <3> * <3> 0.D0 * <3> * <3> * <3> *  
 1.00000000D+02 <3> 1.00000000D+02 <3> 0.D0 <3> 0.D0 3.90339200D+03 <3>         
 3.90339200D+03 <3> * <3> 0.D0 -2.42399453D+06 <3> -2.42399453D+06 <3> * <3>    
 0.D0 0.D0 <3> 3.78150000D+02 <1> 1.00000000D+00 <3> 0.D0 1.00000000D+00 0.D0   
 <3> 11 0.D0 <3> )                                                              
 IDSET ID_5 (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 7001 *2 <22>     
 7002 *2 <20> 899 *2 )                                                          
 LSET L_3 ( %ID_5 )                                                             
 DSET BLOCK FLASH2 FLASH FLS2_INR @L_3 ( * <1> 3.78150000D+02 <1>               
 1.01325000D+05 <1> * * <1> * <1> 0.D0 )                                        
 IDSET ID_6 (COMPONENTS) ( WT ACT )                                             
 LSET L_4 ( %ID_XY & %ID_6)                                                     
 DSET BLOCK FLASH2 FLASH VLE @L_4 ( 5.00000000D-01 5.00000000D-01               
 6.43340179D-01 1.19122669D+00 5.00000000D-01 5.00000000D-01 3.56659821D-01     
 6.60401312D-01 )                                                               
 IDSET ID_7 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )      
 LSET L_5 ( %ID_7 )                                                             
 IDSET ID_8 (PROPERTIES) (253 *2)                                               
 IDSET ID_9 (PROPERTIES) (253 *2 <11> )                                         
 IDSET ID_10 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_11 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_12 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_13 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_14 (PROPERTIES) (8101 *2 <11> 8002 *2 8004 *2 )                       
 IDSET ID_15 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_6 ( %ISODES (( %ID_NCC & %ID_14 %ID_15) & %IDS_1) )                     
 DSET STREAM MATERIAL ACT STR_MAIN @L_6 (FLASH * MISSING 0.D0 <3> 0.D0 <3> 0.D0 
 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 0.D0 0.D0 0.D0 0.D0 0.D0 * * * * * * 0.D0  
 <3> 0.D0 <3> 0.D0 <3> * <1> 1.00000000D+00 <3> * * * * <3> * <3> * <3> * <3> * 
 <3> * <3> * <3> * 0.D0 <3> )                                                   
 DSET STREAM MATERIAL ACT RES_STR @L_5 (* <1> 1.00000000D+00 <3> 0.D0 <3> 0.D0  
 <3> 0.D0 <3> * )                                                               
 DSET STREAM MATERIAL FEED STR_MAIN @L_6 (* FLASH LIQUID 5.00000000D+01 <3>     
 0.D0 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3> 5.00000000D+01 <3> 5.00000000D-01 0.D0     
 0.D0 0.D0 0.D0 5.00000000D-01 2.30764422D-01 0.D0 0.D0 0.D0 0.D0               
 7.69235578D-01 1.00000000D+02 <3> 3.90339200D+03 <3> 7.17789814D+01 <3>        
 3.78150000D+02 <1> 1.00000000D+00 <3> 0.D0 1.00000000D+00 0.D0 -8.72638025D+04 
 <3> -2.23558901D+03 <3> -2.42399453D+06 <3> -4.43932609D+01 <3>                
 -1.13729958D+00 <3> 2.32194246D-02 <3> 9.06345162D-01 <3> 3.90339200D+01       
 6.30678326D+01 <3> )                                                           
 DSET STREAM MATERIAL FEED RES_STR @L_5 (3.78150000D+02 <1> 1.00000000D+00 <3>  
 3.90339200D+03 <3> 7.17789814D+01 <3> 1.00000000D+02 <3> 0.D0 )                
 DSET STREAM MATERIAL WT STR_MAIN @L_6 (FLASH * LIQUID 5.00000000D+01 <3> 0.D0  
 <3> 0.D0 <3> 0.D0 <3> 0.D0 <3> 5.00000000D+01 <3> 5.00000000D-01 0.D0 0.D0     
 0.D0 0.D0 5.00000000D-01 2.30764422D-01 0.D0 0.D0 0.D0 0.D0 7.69235578D-01     
 1.00000000D+02 <3> 3.90339200D+03 <3> 7.17789814D+01 <3> 3.78150000D+02 <1>    
 1.00000000D+00 <3> 0.D0 1.00000000D+00 0.D0 -8.72638025D+04 <3>                
 -2.23558901D+03 <3> -2.42399453D+06 <3> -4.43932609D+01 <3> -1.13729958D+00 <3>
 2.32194246D-02 <3> 9.06345162D-01 <3> 3.90339200D+01 6.30678326D+01 <3> )      
 DSET STREAM MATERIAL WT RES_STR @L_5 (3.78150000D+02 <1> 1.00000000D+00 <3>    
 3.90339200D+03 <3> 7.17789814D+01 <3> 1.00000000D+02 <3> 0.D0 )                
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET ID_16 (NPOINT) ( #9)                                                     
 IDSET ID_17 (PROPERTIES) (747 *6)                                              
 LSET L_7 ( %ID_16 & %ID_17)                                                    
 DSET RUN-STATUS ERRTXT @L_7 (                                                  
 "The following messages were issued during Input Translation:"                 
 ""                                                                             
 "   INFORMATION"                                                               
 "   BINARY PARAMETERS HOCETA (DATA SET 1) FOR MODEL ESHOC"                     
 "   ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESHOC"                         
 ""                                                                             
 "   INFORMATION"                                                               
 "   BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD"                    
 "   ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD"                       
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
