MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Thu Dec 08 11:15:18 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
2
>VERSION 0
MIXER
Mixer
Built-In
MIXER
>VERSION 0
FLASH1
Flash3
Built-In
FLASH3
? SETUP MAIN ? \ TITLE TITLE = "Tutorial" \ \ SIMULATE INTERACTIVE = NO 
MASSFRAC = MASSFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? SETUP GLOBAL ? \ 
"IN-UNITS" INSET = ENG OUTSET = ENG \ \ "STREAM-CLASS" SCLASS = CONVEN \ ? 
SETUP DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP "CUSTOM-UOM" 
? ? SETUP "UNITS-SET" METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = 1 PROJECT-ID = 1 PROJECT-NAME = "HOS3124@GMAIL.COM" 
USER-NAME = "HOSSEIN KHAKPOUR" \ ? SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION 
? \ DESCRIP DESCRIP = ( "General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = WATER ANAME = H2O OUTNAME = WATER TYPE
 = CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  CID = ACETONE ANAME = C3H6O-1 
OUTNAME = ACETONE TYPE = CONV DBNAME1 = "ACETONE" ANAME1 = "C3H6O-1" /  CID
 = MIBK ANAME = C6H12O-2 OUTNAME = MIBK DBNAME1 = "METHYL-ISOBUTYL-KETONE" 
ANAME1 = "C6H12O-2" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET 
GLOBAL ? \ BLOCK BLKID = MIXER BLKTYPE = MIXER IN = ( FEED M0-1 MIBK M0-1 ) 
OUT = ( PRUDUCT M0-1 ) \ \ BLOCK BLKID = FLASH1 BLKTYPE = FLASH3 IN = ( 
PRUDUCT M0-1 ) OUT = ( VAPOR1 M0-1 WA1 M1-2 MA1 M2-3 ) \ \ "DEF-STREAM" 
SCLASS = CONVEN \ ? PROPERTIES MAIN ? \ GPROPERTIES GBASEOPSET = NRTL 
GOPSETNAME = NRTL GFREE-WATER = STEAMNBS PARCON = -2 \ ? PROPERTIES 
"OPTION-SETS" IDEAL ? \ PARAM BASE = IDEAL \ ? PROPERTIES "OPTION-SETS" NRTL 
? \ PARAM BASE = NRTL \ ? PROPERTIES "OPTION-SETS" "PENG-ROB" ? \ PARAM BASE
 = "PENG-ROB" \ ? PROPERTIES "OPTION-SETS" SRK ? \ PARAM BASE = SRK \ ? 
PROPERTIES "OPTION-SETS" STEAMNBS ? \ PARAM BASE = STEAMNBS \ ? PROPERTIES 
"OPTION-SETS" UNIFAC ? \ PARAM BASE = UNIFAC \ ? PROPERTIES "MOLEC-STRUCT" 
ACETONE ? ? PROPERTIES "MOLEC-STRUCT" MIBK ? ? PROPERTIES "MOLEC-STRUCT" 
WATER ? ? PROPERTIES PARAMETERS BINARY SCALAR "PRKIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = PRKIJ SETNO = 1 BDBANK = ( "EOS-LIT" ) \ ? PROPERTIES 
PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = 
RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY SCALAR "SRKAIJ-1" 
? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = SRKAIJ SETNO = 1 \ ? PROPERTIES 
PARAMETERS BINARY SCALAR "SRKBIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = 
SRKBIJ SETNO = 1 UNITROW = 22 UNITLABEL = F \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 
\ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL = psi TUNITROW
 = 22 TUNITLABEL = F BDBANK = ( BINARY HENRY ) NEL = 6 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "NRTL-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = NRTL SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F BDBANK = 
( "VLE-IG" "LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL PARAMNAME2 = NRTL CID1
 = WATER CID2 = ACETONE UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = 
VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG 
VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 
= VLE-IG /  PARAMNAME2 = NRTL CID1 = WATER CID2 = MIBK UNITROW2 = 0 TUNITROW2
 = 22 TUNITLABEL2 = F VAL1 = VLE-IG VAL2 = VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG 
VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = 
VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG /  PARAMNAME2 = NRTL CID1 = ACETONE CID2
 = MIBK UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = VLE-IG VAL2 = 
VLE-IG VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG 
VAL8 = VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG \ ? 
PROPERTIES PARAMETERS UNIBINARY SCALAR "GMUFB-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = GMUFB SETNO = 1 \ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 
ID = MASSVFRA \ \ P1 ID = MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS
 = ( "J/kg" ) \ \ P1 ID = RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS
 = ( "J/kg-K" ) \ \ P1 ID = PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS
 = ( "N-sec/sqm" ) \ \ P1 ID = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX 
UNITS = ( "N/m" ) \ \ P1 ID = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION 
DESCRIPTION = "Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" 
MAIN THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = 
CPMX UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = 
( V L ) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 75. <22> <2> 
PRES = 50. <20> <2> BASIS = "MASS-FRAC" FLOWBASE = MASS TOTFLOW = 100. <-80> 
<2> TOTAL = 1. <-89> <0> JUNK = 2 \ \ MOLE-FLOW SSID1 = MIXED CID = WATER 
FLOW = 0.5 <-3> <0> /  SSID1 = MIXED CID = ACETONE FLOW = 0.5 <-3> <0> \ ? 
STREAM MATERIAL MIBK ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 75. 
<22> <2> PRES = 50. <20> <2> FLOWBASE = MASS TOTFLOW = 100. <-80> <2> TOTAL
 = 1. <-89> <0> JUNK = 1 \ \ MOLE-FLOW SSID1 = MIXED CID = MIBK FLOW = 1. 
<-89> <2> \ ? "STREAM-SUM" ? ? BLOCK MIXER MIXER ? ; "ENG_MOLE" ; ; TRIANGLE 
; \ PARAM NPHASE = 1 PHASE = L \ \ "BLOCK-OPTION" BLKOPFREWAT = NO \ ? BLOCK 
FLASH3 FLASH1 ? ; "ENG_MOLE" ; ; "V-DRUM2" ; \ PARAM TEMP = 75. <22> <2> PRES
 = 50. <20> <2> \ ? "EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ 
DMO-PARAMS MODE = SIMULATION \ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ 
DMO-PARAMS MODE = RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ 
LSSQP-PARAMS MODE-L = DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ 
LSSQP-PARAMS MODE-L = "PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = 
RECONCILIATION \ \ LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? 
REPORT "BLOCK-REPORT" ? ? REPORT "STREAM-REPOR" ? \ OPTIONS MASSFRAC = 
MASSFRAC \ ? REPORT "FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT 
"ADA-REPORT" ? ? REPORT "BATCH-OPERAT" ? ; "ENG_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 0
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6465
browserwidth 10335
browsertreewidth 2445
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 9
SIZE -3.49687 4.44732 -0.902789 1.79474
BLOCK
ID: MIXER
Version: 1
ICON: "TRIANGLE"
Flag 0
Section GLOBAL
At -1.100000 0.400000
Label At 0.000931 0.417170
Scale 1.896570 Modifier 0
BLOCK
ID: FLASH1
Version: 1
ICON: "V-DRUM2"
Flag 0
Section GLOBAL
At 2.396916 0.446956
Label At -0.208903 0.448971
Scale 1.900000 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -3.496874 1.145497
Label At 0.892962 0.006994
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -3.496874 1.145497
x x -2.676914 1.145497
y y -2.676914 1.152491
x x -1.861719 1.152491
t l -1.661719 1.152491
$ D 0.007833 0.754616
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: MIBK
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -3.496874 -0.198699
Label At 0.896874 0.027219
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -3.496874 -0.198699
x x -2.600000 -0.198699
y y -2.600000 -0.171480
x x -1.865358 -0.171480
t l -1.665357 -0.171480
$ D 0.004194 -0.569355
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: PRUDUCT
Version: 1
Flag 0
Port 0 MIXER o1
Port 1 FLASH1 i1
TYPE 0 TERMINAL 0
At 1.135792 0.410577
Label At -0.498014 -0.012702
ROUTE 0 0
r r 1.135792 0.410577
x y 0.698292 0.410577
y x 0.698292 0.397875
x 0 -0.330449 0.397875
t r -0.530449 0.397875
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
r r 1.135792 0.410577
x x 1.720910 0.410577
y x 1.720910 0.407533
t l 1.920910 0.407533
$ D -0.002319 -0.037731
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: VAPOR1
Version: 1
Flag 0
Port 0 FLASH1 o1
TYPE 0 TERMINAL 2
At 4.380113 1.794744
Label At -0.991599 0.000000
ROUTE 0 0
r l 4.380113 1.794744
x y 2.396916 1.794744
y 0 2.396916 1.406546
t u 2.396916 1.206545
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: WA1
Version: 1
Flag 0
Port 0 FLASH1 o2
TYPE 0 TERMINAL 2
At 4.446242 0.446956
Label At -0.894287 -0.001692
ROUTE 0 0
r l 4.446242 0.446956
x y 3.650000 0.446956
y x 3.650000 0.445264
x 0 3.073985 0.445264
t r 2.873985 0.445264
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: MA1
Version: 1
Flag 0
Port 0 FLASH1 o3
TYPE 0 TERMINAL 2
At 4.447323 -0.902789
Label At -1.025203 0.000000
ROUTE 0 0
r l 4.447323 -0.902789
x y 2.396916 -0.902789
y 0 2.396916 -0.509250
t d 2.396916 -0.309250
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.91161 -3.2 -3.14714 -3.34924
Size: 0.0153354
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -9.173952 10.117972 3.536355 -3.241889
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.015335

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "FaraDars" "FARADARS_PC"
 )                                                                              
 DSET RUN-STATUS IT @IT ( "DECEMBER 8, 2016    10:59:06 A.M." "_5835wiv.inm" 0) 
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (WATER ACETONE MIBK)                                 
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_5835wiv")                                      
 DSET RUN-STATUS RUNID @RUNID ("_5835wiv")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "DECEMBER 8, 2016 10:59:06 A.M." )                    
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "TUTORIAL" )                                    
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (1 1 "HOS3124@GMAIL.COM" "HOSSEIN KHAKPOUR" ) 
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (1.80152800D+01 5.80800400D+01 1.00160680D+02)                  
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (2.89133265D-01 <2> 1.18530542D+00 <2> 2.01493048D+00 <2> )  
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (2.12000002D+02 <2> 1.33322003D+02 <2> 2.40800002D+02 <2> )     
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (4.57931648D-09 <2> -1.51263957D-09 <2> -3.06667680D-09 <2>
 1.64995337D-09 -1.75708333D-09 -3.07160433D-09 0.D0 <2> 0.D0 -3.12516931D-07   
 <2> -1.56258465D-09 -1.40691368D+03 <2> -2.44335380D-03)                       
 DSET ALIAS @ALIAS ( "H2O" "C3H6O-1" "C6H12O-2" )                               
 IDSET ID_1 (NPOINT) (#3)                                                       
 IDSET ID_2 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)                
 LSET L_1 (%ID_2 & %ID_1)                                                       
 DSET COMPONENTS MAIN COMPS @L_1 ("WATER" C "H2O" "H2O" "WATER" "ACETONE" C     
 "C3H6O-1" "C3H6O-1" "ACETONE" "MIBK" C "C6H12O-2" "C6H12O-2" "MIBK" )          
 IDSET ID_3 (PROPERTIES) (1052 *2 <13> )                                        
 LSET L_2 (%ID_RXBAL %ID_TPQV %ID_3 %ID_KODE )                                  
 DSET BLOCK FLASH3 FLASH1 BLKSTAT @BLKSTAT (0 0)                                
 DSET BLOCK FLASH3 FLASH1 COMPSTAT @L1 (0)                                      
 DSET BLOCK FLASH3 FLASH1 BLKIN @BLKIN (1 PRUDUCT)                              
 DSET BLOCK FLASH3 FLASH1 TYPIN @TYPIN (1 MATERIAL)                             
 DSET BLOCK FLASH3 FLASH1 BLKOUT @BLKOUT (3 VAPOR1 WA1 MA1)                     
 DSET BLOCK FLASH3 FLASH1 TYPOUT @TYPOUT (3 MATERIAL MATERIAL MATERIAL)         
 DSET BLOCK FLASH3 FLASH1 RES_Q @L_2 (4.63469848D+00 <2> 4.63469848D+00 <2>     
 0.D0 <2> 0.D0 2.00000000D+02 <2> 2.00000000D+02 <2> * <2> -1.56258451D-09 * <2>
 * <2> * <2> * 4.63469848D+00 <2> 4.63469848D+00 <2> 0.D0 <2> 0.D0              
 2.00000000D+02 <2> 2.00000000D+02 <2> * <2> -1.56258451D-09 -5.75812509D+05 <2>
 -5.74405595D+05 <2> * <2> -2.44335380D-03 1.40691368D+03 <2> 7.50000000D+01 <2>
 5.00000000D+01 <2> 0.D0 4.18202366D-01 1.40691368D+03 <2> 17)                  
 DSET BLOCK FLASH3 FLASH1 VLE3 @VLE3 ( 5.98835451D-01 1.64804586D-01            
 9.10821480D-01 2.10512829D-01 4.86420777D-02 8.80161241D-03 1.85746916D-01     
 3.29115967D-01 8.26917084D-02 6.78739957D-01 7.85361734D-02 3.12581343D-01     
 2.15417633D-01 5.06079447D-01 6.48681150D-03 1.10747215D-01 8.33369628D-03     
 6.50174797D-01 )                                                               
 IDSET ID_4 (PROPERTIES) (31 *2 <22> 32 *2 <20> 2 *2 3 *2)                      
 IDSET ID_5 (PROPERTIES) (298 *2 <75> )                                         
 LSET L_3 (%ID_RXBAL %ID_4 %ID_KODE %ID_5)                                      
 DSET BLOCK MIXER MIXER BLKSTAT @BLKSTAT (0 0)                                  
 DSET BLOCK MIXER MIXER COMPSTAT @L1 (0)                                        
 DSET BLOCK MIXER MIXER BLKIN @BLKIN (2 FEED MIBK)                              
 DSET BLOCK MIXER MIXER TYPIN @TYPIN (2 MATERIAL MATERIAL)                      
 DSET BLOCK MIXER MIXER BLKOUT @BLKOUT (1 PRUDUCT)                              
 DSET BLOCK MIXER MIXER TYPOUT @TYPOUT (1 MATERIAL)                             
 DSET BLOCK MIXER MIXER MIX_RES @L_3 (4.63469848D+00 <2> 4.63469848D+00 <2>     
 0.D0 <2> 0.D0 2.00000000D+02 <2> 2.00000000D+02 <2> * <2> 0.D0 * <2> * <2> *   
 <2> * 4.63469848D+00 <2> 4.63469848D+00 <2> 0.D0 <2> 0.D0 2.00000000D+02 <2>   
 2.00000000D+02 <2> * <2> 0.D0 -5.75812509D+05 <2> -5.75812509D+05 <2> * <2>    
 2.02175743D-16 6.52912417D+01 <2> 5.00000000D+01 <2> 0.D0 1.00000000D+00 3     
 0.D0 <2> )                                                                     
 IDSET ID_6 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )      
 LSET L_4 ( %ID_6 )                                                             
 IDSET ID_7 (PROPERTIES) (253 *2)                                               
 IDSET ID_8 (PROPERTIES) (253 *2 <11> )                                         
 IDSET ID_9 (PROPERTIES) (253 *2 <12> )                                         
 IDSET ID_10 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_11 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_12 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_13 (PROPERTIES) (8101 *2 <11> 8004 *2 )                               
 IDSET ID_14 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_5 ( %ISODES (( %ID_NCC & %ID_13 %ID_14) & %IDS_1) )                     
 DSET STREAM MATERIAL FEED STR_MAIN @L_5 (* MIXER LIQUID 2.77542175D+00 <2>     
 8.60880950D-01 <2> 0.D0 <2> 5.00000000D-01 5.00000000D-01 0.D0 3.63630270D+00  
 <2> 1.00000000D+02 <2> 1.82646657D+00 <2> 7.50000000D+01 <2> 5.00000000D+01 <2>
 0.D0 1.00000000D+00 0.D0 -1.19720049D+05 <2> -4.35338339D+03 <2>               
 -4.35338337D+05 <2> -4.82911968D+01 <2> -1.75601409D+00 <2> 1.99089479D+00 <2> 
 5.47505243D+01 <2> 2.75004608D+01 1.82287360D+00 <2> )                         
 DSET STREAM MATERIAL FEED RES_STR @L_4 (7.50000000D+01 <2> 5.00000000D+01 <2>  
 1.00000000D+02 <2> 1.82646657D+00 <2> 3.63630270D+00 <2> 0.D0 )                
 DSET STREAM MATERIAL MA1 STR_MAIN @L_5 (FLASH1 * LIQUID 2.45599060D+00 <2>     
 2.22974604D-01 <2> 1.74914057D-02 <2> 7.50586891D-01 2.19692669D-01            
 2.97204402D-02 2.69645661D+00 <2> 5.89476833D+01 <2> 1.01143533D+00 <2>        
 7.50000000D+01 <2> 5.00000000D+01 <2> 0.D0 1.00000000D+00 0.D0 -1.21900769D+05 
 <2> -5.57613318D+03 <2> -3.28700132D+05 <2> -4.27888041D+01 <2>                
 -1.95729751D+00 <2> 2.66597041D+00 <2> 5.82812196D+01 <2> 2.18611652D+01       
 1.00964555D+00 <2> )                                                           
 DSET STREAM MATERIAL MA1 RES_STR @L_4 (7.50000000D+01 <2> 5.00000000D+01 <2>   
 5.89476833D+01 <2> 1.01143533D+00 <2> 2.69645661D+00 <2> 0.D0 )                
 DSET STREAM MATERIAL MIBK STR_MAIN @L_5 (* MIXER LIQUID 0.D0 <2> 0.D0 <2>      
 9.98395778D-01 <2> 0.D0 0.D0 1.00000000D+00 9.98395778D-01 <2> 1.00000000D+02  
 <2> 2.01833153D+00 <2> 7.50000000D+01 <2> 5.00000000D+01 <2> 0.D0              
 1.00000000D+00 0.D0 -1.40699887D+05 <2> -1.40474173D+03 <2> -1.40474172D+05 <2>
 -1.46708117D+02 <2> -1.46472765D+00 <2> 4.94663927D-01 <2> 4.95458753D+01 <2>  
 1.00160680D+02 2.01169807D+00 <2> )                                            
 DSET STREAM MATERIAL MIBK RES_STR @L_4 (7.50000000D+01 <2> 5.00000000D+01 <2>  
 1.00000000D+02 <2> 2.01833153D+00 <2> 9.98395778D-01 <2> 0.D0 )                
 DSET STREAM MATERIAL PRUDUCT STR_MAIN @L_5 (MIXER FLASH1 LIQUID 2.77542175D+00 
 <2> 8.60880950D-01 <2> 9.98395778D-01 <2> 2.50000000D-01 2.50000000D-01        
 5.00000000D-01 4.63469848D+00 <2> 2.00000000D+02 <2> 3.73588818D+00 <2>        
 6.52912417D+01 <2> 5.00000000D+01 <2> 0.D0 1.00000000D+00 0.D0 -1.24239476D+05 
 <2> -2.87906256D+03 <2> -5.75812509D+05 <2> -6.93427375D+01 <2>                
 -1.60691340D+00 <2> 1.24058814D+00 <2> 5.35347941D+01 <2> 4.31527533D+01       
 3.83457167D+00 <2> )                                                           
 DSET STREAM MATERIAL PRUDUCT RES_STR @L_4 (6.52912417D+01 <2> 5.00000000D+01   
 <2> 2.00000000D+02 <2> 3.73588818D+00 <2> 4.63469848D+00 <2> 0.D0 )            
 DSET STREAM MATERIAL VAPOR1 STR_MAIN @L_5 (FLASH1 * MISSING 0.D0 <2> 0.D0 <2>  
 0.D0 <2> * * * 0.D0 <2> 0.D0 <2> 0.D0 <2> * <2> 5.00000000D+01 <2> * * * * <2> 
 * <2> * <2> * <2> * <2> * <2> * <2> * 0.D0 <2> )                               
 DSET STREAM MATERIAL VAPOR1 RES_STR @L_4 (* <2> 5.00000000D+01 <2> 0.D0 <2>    
 0.D0 <2> 0.D0 <2> * )                                                          
 DSET STREAM MATERIAL WA1 STR_MAIN @L_5 (FLASH1 * LIQUID 3.19431150D-01 <2>     
 6.37906348D-01 <2> 9.80904375D-01 <2> 4.07979232D-02 2.62665846D-01            
 6.96536231D-01 1.93824187D+00 <2> 1.41052317D+02 <2> 2.78186917D+00 <2>        
 7.50000000D+01 <2> 5.00000000D+01 <2> 0.D0 1.00000000D+00 0.D0 -1.26767184D+05 
 <2> -1.74194561D+03 <2> -2.45705464D+05 <2> -1.04452914D+02 <2>                
 -1.43531859D+00 <2> 6.96740859D-01 <2> 5.07041531D+01 <2> 7.27733308D+01       
 2.82492613D+00 <2> )                                                           
 DSET STREAM MATERIAL WA1 RES_STR @L_4 (7.50000000D+01 <2> 5.00000000D+01 <2>   
 1.41052317D+02 <2> 2.78186917D+00 <2> 1.93824187D+00 <2> 0.D0 )                
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET ID_15 (NPOINT) ( #10)                                                    
 IDSET ID_16 (PROPERTIES) (747 *6)                                              
 LSET L_6 ( %ID_15 & %ID_16)                                                    
 DSET RUN-STATUS ERRTXT @L_6 (                                                  
 "The following messages were issued during Input Translation:"                 
 ""                                                                             
 "   INFORMATION"                                                               
 "   BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD"                    
 "   ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD"                       
 ""                                                                             
 "*  WARNING IN THE 'STREAM' PARAGRAPH WHICH BEGINS ON LINE 68"                 
 "   STREAM NAME: MIBK"                                                         
 "   COMPONENT MOLE FLOWS OF SUBSTREAM: 'MIXED'"                                
 "   ARE NORMALIZED TO THE TOTAL MOLE FLOW VALUE."                              
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
