MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Thu Dec 08 10:27:24 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
MIXER
Mixer
Built-In
MIXER
? SETUP MAIN ? \ TITLE TITLE = "Tutorial" \ \ SIMULATE INTERACTIVE = NO 
MASSFRAC = MASSFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? SETUP GLOBAL ? \ 
"IN-UNITS" INSET = ENG \ \ "STREAM-CLASS" SCLASS = CONVEN \ ? SETUP 
DIAGNOSTICS ? ? SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" 
METCBAR ? \ DESCRIPTION DESCRIPTION = 
"Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ MMLOCAL \ \ UNITSET 
BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 4 3 3 3 3 1 3 3 3 4 
3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 3 3 3 3 3 3 
3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ DESCRIPTION 
DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" \ \ MMLOCAL 
\ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 8 3 4 3 3 3 
3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 3 3 3 4 
3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? \ 
DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" \ 
\ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 5 
1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = 1 PROJECT-ID = 1 PROJECT-NAME = "HOS3124@GMAIL.COM" 
USER-NAME = "HOSSEIN KHAKPOUR" \ ? SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION 
? \ DESCRIP DESCRIP = ( "General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = WATER ANAME = H2O OUTNAME = WATER TYPE
 = CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  CID = ACETONE ANAME = C3H6O-1 
OUTNAME = ACETONE TYPE = CONV DBNAME1 = "ACETONE" ANAME1 = "C3H6O-1" /  CID
 = MIBK ANAME = C6H12O-2 OUTNAME = MIBK DBNAME1 = "METHYL-ISOBUTYL-KETONE" 
ANAME1 = "C6H12O-2" \ ? COMPONENTS "COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET 
GLOBAL ? \ BLOCK BLKID = MIXER BLKTYPE = MIXER IN = ( FEED M0-1 MIBK M0-1 ) 
OUT = ( PRUDUCT M0-1 ) \ \ "DEF-STREAM" SCLASS = CONVEN \ ? PROPERTIES MAIN ? 
\ GPROPERTIES GBASEOPSET = IDEAL GOPSETNAME = IDEAL PARCON = -1 \ ? 
PROPERTIES "OPTION-SETS" IDEAL ? \ PARAM BASE = IDEAL \ ? PROPERTIES 
"MOLEC-STRUCT" ACETONE ? ? PROPERTIES "MOLEC-STRUCT" MIBK ? ? PROPERTIES 
"MOLEC-STRUCT" WATER ? ? PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; 
"ENG_MOLE" ; \ PROP-LIST PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? 
PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = ANDKIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL
 = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; 
"ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 
22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" 
"HENRY-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = HENRY SETNO = 1 UNITROW = 
20 UNITLABEL = psi TUNITROW = 22 TUNITLABEL = F BDBANK = ( BINARY HENRY ) NEL
 = 6 \ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 
ID = MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 
ID = RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 
ID = PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 
ID = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 
ID = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 75. <22> <2> 
PRES = 50. <20> <2> BASIS = "MASS-FRAC" FLOWBASE = MASS TOTFLOW = 100. <-80> 
<2> TOTAL = 1. <-89> <0> JUNK = 2 \ \ MOLE-FLOW SSID1 = MIXED CID = WATER 
FLOW = 0.5 <-3> <0> /  SSID1 = MIXED CID = ACETONE FLOW = 0.5 <-3> <0> \ ? 
STREAM MATERIAL MIBK ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 75. 
<22> <2> PRES = 50. <20> <2> FLOWBASE = MASS TOTFLOW = 100. <-80> <2> TOTAL
 = 1. <-89> <0> JUNK = 1 \ \ MOLE-FLOW SSID1 = MIXED CID = MIBK FLOW = 1. 
<-89> <2> \ ? BLOCK MIXER MIXER ? ; "ENG_MOLE" ; ; TRIANGLE ; \ PARAM NPHASE
 = 1 PHASE = L \ \ "BLOCK-OPTION" BLKOPFREWAT = NO \ ? "EO-CONV-OPTI" ? \ 
DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = SIMULATION \ \ DMO-PARAMS 
MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE = RECONCILIATION \ \ 
DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L = DEFAULT \ \ 
LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MASSFRAC = MASSFRAC \ ? REPORT 
"FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT "ADA-REPORT" ? ? REPORT 
"BATCH-OPERAT" ? ; "ENG_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6465
browserwidth 10335
browsertreewidth 2445
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 5
SIZE -3.49491 1.69369 -0.806165 1.59924
BLOCK
ID: MIXER
Version: 1
ICON: "TRIANGLE"
Flag 0
Section GLOBAL
At -1.102240 0.396538
Label At 0.000931 0.417170
Scale 2.405406 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -3.494909 1.404684
Label At 0.819959 -0.053768
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -3.494909 1.404684
x x -2.674949 1.404684
y y -2.674949 1.350916
x x -2.014664 1.350916
t l -1.814664 1.350916
$ D 0.009934 0.957074
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: MIBK
Version: 1
Flag 0
Port 1 MIXER i1
TYPE 0 TERMINAL 1
At -3.494909 -0.396538
Label At 0.698982 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -3.494909 -0.396538
x x -2.674949 -0.396538
y y -2.674949 -0.373116
x x -2.030346 -0.373116
t l -1.830346 -0.373116
$ D -0.005748 -0.766959
$ C 0.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: PRUDUCT
Version: 1
Flag 0
Port 0 MIXER o1
TYPE 0 TERMINAL 2
At 1.693686 0.396538
Label At -1.315779 -0.002695
ROUTE 0 0
r l 1.693686 0.396538
x y 0.650000 0.396538
y x 0.650000 0.393842
x 0 -0.179883 0.393842
t r -0.379883 0.393842
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.91161 -3.2 -3.10509 -3.36721
Size: 0.013442
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -9.032994 7.876986 3.300000 -2.641345
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.013442

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "Hossein Khakpour"      
 "FARADARS_PC" )                                                                
 DSET RUN-STATUS IT @IT ( "DECEMBER 8, 2016    10:25:45 A.M." "" 0)             
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (WATER ACETONE MIBK)                                 
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_0911yin")                                      
 DSET RUN-STATUS RUNID @RUNID ("_0911yin")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "DECEMBER 8, 2016 10:25:45 A.M." )                    
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "TUTORIAL" )                                    
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (1 1 "HOS3124@GMAIL.COM" "HOSSEIN KHAKPOUR" ) 
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (1.80152800D+01 5.80800400D+01 1.00160680D+02)                  
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (2.89133265D-01 <2> 1.18530542D+00 <2> 2.01493048D+00 <2> )  
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (2.12000002D+02 <2> 1.33322003D+02 <2> 2.40800002D+02 <2> )     
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (0.D0 <2> 0.D0 <2> 0.D0 <2> 0.D0 0.D0 0.D0 0.D0 <2> 0.D0   
 0.D0 <2> 0.D0 1.16415322D-10 <2> 2.03207727D-16)                               
 DSET ALIAS @ALIAS ( "H2O" "C3H6O-1" "C6H12O-2" )                               
 IDSET ID_53 (NPOINT) (#3)                                                      
 IDSET ID_54 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)               
 LSET L_17 (%ID_54 & %ID_53)                                                    
 DSET COMPONENTS MAIN COMPS @L_17 ("WATER" C "H2O" "H2O" "WATER" "ACETONE" C    
 "C3H6O-1" "C3H6O-1" "ACETONE" "MIBK" C "C6H12O-2" "C6H12O-2" "MIBK" )          
 IDSET ID_55 (PROPERTIES) (31 *2 <22> 32 *2 <20> 2 *2 3 *2)                     
 IDSET ID_56 (PROPERTIES) (298 *2 <75> )                                        
 LSET L_18 (%ID_RXBAL %ID_55 %ID_KODE %ID_56)                                   
 DSET BLOCK MIXER MIXER BLKSTAT @BLKSTAT (0 0)                                  
 DSET BLOCK MIXER MIXER COMPSTAT @L1 (0)                                        
 DSET BLOCK MIXER MIXER BLKIN @BLKIN (2 FEED MIBK)                              
 DSET BLOCK MIXER MIXER TYPIN @TYPIN (2 MATERIAL MATERIAL)                      
 DSET BLOCK MIXER MIXER BLKOUT @BLKOUT (1 PRUDUCT)                              
 DSET BLOCK MIXER MIXER TYPOUT @TYPOUT (1 MATERIAL)                             
 DSET BLOCK MIXER MIXER MIX_RES @L_18 (4.63469848D+00 <2> 4.63469848D+00 <2>    
 0.D0 <2> 0.D0 2.00000000D+02 <2> 2.00000000D+02 <2> * <2> 0.D0 * <2> * <2> *   
 <2> * 4.63469848D+00 <2> 4.63469848D+00 <2> 0.D0 <2> 0.D0 2.00000000D+02 <2>   
 2.00000000D+02 <2> * <2> 0.D0 -5.72888262D+05 <2> -5.72888262D+05 <2> * <2>    
 2.03207727D-16 7.49999775D+01 <2> 5.00000000D+01 <2> 0.D0 1.00000000D+00 3     
 0.D0 <2> )                                                                     
 IDSET ID_57 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )     
 LSET L_19 ( %ID_57 )                                                           
 IDSET ID_58 (PROPERTIES) (253 *2)                                              
 IDSET ID_59 (PROPERTIES) (253 *2 <11> )                                        
 IDSET ID_60 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_61 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_62 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_63 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_64 (PROPERTIES) (8101 *2 <11> 8004 *2 )                               
 IDSET ID_65 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_20 ( %ISODES (( %ID_NCC & %ID_64 %ID_65) & %IDS_1) )                    
 DSET STREAM MATERIAL FEED STR_MAIN @L_20 (* MIXER LIQUID 2.77542175D+00 <2>    
 8.60880950D-01 <2> 0.D0 <2> 5.00000000D-01 5.00000000D-01 0.D0 3.63630270D+00  
 <2> 1.00000000D+02 <2> 1.82646657D+00 <2> 7.50000000D+01 <2> 5.00000000D+01 <2>
 0.D0 1.00000000D+00 0.D0 -1.18915868D+05 <2> -4.32414092D+03 <2>               
 -4.32414090D+05 <2> -4.62183733D+01 <2> -1.68063996D+00 <2> 1.99089479D+00 <2> 
 5.47505243D+01 <2> 2.75004608D+01 1.82287360D+00 <2> )                         
 DSET STREAM MATERIAL FEED RES_STR @L_19 (7.50000000D+01 <2> 5.00000000D+01 <2> 
 1.00000000D+02 <2> 1.82646657D+00 <2> 3.63630270D+00 <2> 0.D0 )                
 DSET STREAM MATERIAL MIBK STR_MAIN @L_20 (* MIXER LIQUID 0.D0 <2> 0.D0 <2>     
 9.98395778D-01 <2> 0.D0 0.D0 1.00000000D+00 9.98395778D-01 <2> 1.00000000D+02  
 <2> 2.01833153D+00 <2> 7.50000000D+01 <2> 5.00000000D+01 <2> 0.D0              
 1.00000000D+00 0.D0 -1.40699887D+05 <2> -1.40474173D+03 <2> -1.40474172D+05 <2>
 -1.46708117D+02 <2> -1.46472765D+00 <2> 4.94663927D-01 <2> 4.95458753D+01 <2>  
 1.00160680D+02 2.01169807D+00 <2> )                                            
 DSET STREAM MATERIAL MIBK RES_STR @L_19 (7.50000000D+01 <2> 5.00000000D+01 <2> 
 1.00000000D+02 <2> 2.01833153D+00 <2> 9.98395778D-01 <2> 0.D0 )                
 DSET STREAM MATERIAL PRUDUCT STR_MAIN @L_20 (MIXER * LIQUID 2.77542175D+00 <2> 
 8.60880950D-01 <2> 9.98395778D-01 <2> 2.50000000D-01 2.50000000D-01            
 5.00000000D-01 4.63469848D+00 <2> 2.00000000D+02 <2> 3.76152776D+00 <2>        
 7.49999775D+01 <2> 5.00000000D+01 <2> 0.D0 1.00000000D+00 0.D0 -1.23608530D+05 
 <2> -2.86444132D+03 <2> -5.72888262D+05 <2> -6.68309199D+01 <2>                
 -1.54870582D+00 <2> 1.23213196D+00 <2> 5.31698865D+01 <2> 4.31527533D+01       
 3.83457167D+00 <2> )                                                           
 DSET STREAM MATERIAL PRUDUCT RES_STR @L_19 (7.49999775D+01 <2> 5.00000000D+01  
 <2> 2.00000000D+02 <2> 3.76152776D+00 <2> 4.63469848D+00 <2> 0.D0 )            
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
