MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Sun Dec 11 13:01:58 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
B1
RadFrac
Built-In
RADFRAC
? SETUP MAIN ? \ TITLE TITLE = "DIST2" \ \ SIMULATE INTERACTIVE = NO MOLEFRAC
 = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? SETUP GLOBAL ? \ "IN-UNITS" 
INSET = ENG \ \ "STREAM-CLASS" SCLASS = CONVEN \ ? SETUP DIAGNOSTICS ? ? 
SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" METCBAR ? \ 
DESCRIPTION DESCRIPTION = "Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ 
MMLOCAL \ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 
4 3 3 3 3 1 3 3 3 4 3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 
3 3 3 4 3 3 3 3 3 3 3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ 
DESCRIPTION DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" 
\ \ MMLOCAL \ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 
8 3 4 3 3 3 3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 
3 3 3 3 3 4 3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? 
\ DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" 
\ \ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 
5 1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT ACCOUNT = D PROJECT-ID = D PROJECT-NAME = "D" USER-NAME = "D" \ ? 
SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ DESCRIP DESCRIP = ( 
"General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = BZ ANAME = C6H6 OUTNAME = BZ TYPE = 
CONV DBNAME1 = "BENZENE" ANAME1 = "C6H6" /  CID = TL ANAME = C7H8 OUTNAME = 
TL TYPE = CONV DBNAME1 = "TOLUENE" ANAME1 = "C7H8" \ ? COMPONENTS "COMP-LIST" 
GLOBAL ? ? SOLVE ? ? FLOWSHEET GLOBAL ? \ BLOCK BLKID = B1 BLKTYPE = RADFRAC 
IN = ( FEED2 M0-1 ) OUT = ( DIST2 M1-2 BOT2 M2-3 ) \ \ "DEF-STREAM" SCLASS = 
CONVEN \ ? PROPERTIES MAIN ? \ GPROPERTIES GBASEOPSET = NRTL GOPSETNAME = 
NRTL PARCON = -1 \ ? PROPERTIES "OPTION-SETS" NRTL ? \ PARAM BASE = NRTL \ ? 
PROPERTIES "MOLEC-STRUCT" BZ ? ? PROPERTIES "MOLEC-STRUCT" TL ? ? PROPERTIES 
PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = 
RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" 
"ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDKIJ SETNO = 1 UNITROW
 = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY 
"T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = ANDMIJ 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? PROPERTIES 
PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; "ENG_MOLE" ; \ PROP-LIST 
PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL = psi TUNITROW = 22 
TUNITLABEL = F BDBANK = ( BINARY HENRY ) NEL = 6 \ ? PROPERTIES PARAMETERS 
BINARY "T-DEPENDENT" "NRTL-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = NRTL 
SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F BDBANK = ( "VLE-IG" 
"LLE-ASPEN" "VLE-LIT" ) NEL = 12 \ \ BPVAL PARAMNAME2 = NRTL CID1 = BZ CID2
 = TL UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = F VAL1 = VLE-IG VAL2 = VLE-IG 
VAL3 = VLE-IG VAL4 = VLE-IG VAL5 = VLE-IG VAL6 = VLE-IG VAL7 = VLE-IG VAL8 = 
VLE-IG VAL9 = VLE-IG VAL10 = VLE-IG VAL11 = VLE-IG VAL12 = VLE-IG \ ? 
"PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = MASSVFRA \ \ P1 ID = 
MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( "J/kg" ) \ \ P1 ID = 
RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( "J/kg-K" ) \ \ P1 ID = 
PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( "N-sec/sqm" ) \ \ P1 ID
 = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX UNITS = ( "N/m" ) \ \ P1 ID
 = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION DESCRIPTION = 
"Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" MAIN 
THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = CPMX 
UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L 
) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED2 ? ; "ENG_MOLE" ; \ SUBSTREAM SSID = MIXED PRES = 100. <20> 
<10> VFRAC = 0. <0> <0> BASIS = "MOLE-FRAC" TOTFLOW = 100. <-89> <3> TOTAL = 
1. <-89> <0> JUNK = 2 \ \ MOLE-FLOW SSID1 = MIXED CID = BZ FLOW = 0.4 <-4> 
<0> /  SSID1 = MIXED CID = TL FLOW = 0.6 <-4> <0> \ ? BLOCK RADFRAC B1 ? ; 
"ENG_MOLE" ; ; FRACT1 ; \ PARAM NSTAGE = 7 \ \ "COL-CONFIG" CONDENSER = TOTAL 
\ \ FEEDS FEED-SID = FEED2 FEED-STAGE = 4 \ \ PRODUCTS PROD-STREAM = DIST2 
PROD-STAGE = 1 PROD-PHASE = L P-S = N /  PROD-STREAM = BOT2 PROD-STAGE = 7 
PROD-PHASE = L P-S = N \ \ "P-SPEC2" PRES1 = 100. <20> <10> \ \ "COL-SPECS" 
BASIS-RDV = 0.0 <-1> <0> D-BASIS = MOLE BASIS-D = 37.5 <-89> <3> RR-BASIS = 
MOLE BASIS-RR = 3. <-1> <0> \ \ TRAY-SIZE TS-SECNO = 1 TS-STAGE1 = 2 
TS-STAGE2 = 6 TS-TRAYTYPE = CAPS TS-TSPACE = 2. <17> <2> \ \ TRAY-RATE 
TA-SECNO = 1 TR-STAGE1 = 2 TR-STAGE2 = 6 TA-TRAYTYPE = CAPS TR-DIAM = 1. <17> 
<1> TA-P-UPDATE = YES \ \ "KLL-VECS" \ \ "TRSZ-VECS" \ \ "PCKSR-VECS" \ ? 
"EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = SIMULATION 
\ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE = 
RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L = 
DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFRAC = MOLEFRAC \ ? REPORT 
"FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT "ADA-REPORT" ? ? REPORT 
"BATCH-OPERAT" ? ; "ENG_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6465
browserwidth 10335
browsertreewidth 2445
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 5
SIZE -7.54766 -3.09837 -2.18587 1.4
BLOCK
ID: B1
Version: 1
ICON: "FRACT1"
Flag 0
Section GLOBAL
At -5.699389 -0.399201
Label At -0.056312 1.007015
Scale 1.786667 Modifier 0
STREAM
ID: FEED2
Version: 1
Flag 0
Port 1 B1 i1
TYPE 0 TERMINAL 1
At -7.547658 -0.399201
Label At 0.668118 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -7.547658 -0.399201
x x -6.825000 -0.399201
y y -6.825000 -0.399200
x x -6.303108 -0.399200
t l -6.103108 -0.399200
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: DIST2
Version: 1
Flag 0
Port 0 B1 o2
TYPE 0 TERMINAL 2
At -3.494908 0.595504
Label At -0.650854 0.000000
ROUTE 0 0
r l -3.494908 0.595504
x y -4.200000 0.595504
y x -4.200000 0.540861
x 0 -4.699168 0.540861
t r -4.899168 0.540861
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: BOT2
Version: 1
Flag 0
Port 0 B1 o3
TYPE 0 TERMINAL 2
At -3.098371 -1.904700
Label At -0.896692 0.029437
ROUTE 0 0
r l -3.098371 -1.904700
x y -3.875000 -1.904700
y x -3.875000 -1.875262
x 0 -4.435292 -1.875262
t r -4.635292 -1.875262
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.91161 -3.2 -3.10509 -3.35912
Size: 0.013442
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -9.032994 7.876986 2.044547 -3.896797
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.013442
