MM "11.1" FLAVOR "NO" VERSION "11.1" DATETIME "Thu Dec 08 09:32:05 2016" 
MACHINE "WIN-NT/VC"  ; 
startlibrary
version1
NumLibs = 1
Built-In
NumCats = 9
Mixers/Splitters
active
Separators
active
Heat Exchangers
active
Columns
active
Reactors
active
Pressure Changers
active
Manipulators
active
Solids
active
User Models
active
endlibrary
; 
1
>VERSION 0
FLASH
Flash2
Built-In
FLASH2
? SETUP MAIN ? \ TITLE TITLE = "flash" \ \ SIMULATE INTERACTIVE = NO MOLEFRAC
 = MOLEFRAC TFFFILE = "GEN_E" VISITED = 1 \ ? SETUP GLOBAL ? \ "IN-UNITS" 
INSET = MET \ \ "STREAM-CLASS" SCLASS = CONVEN \ ? SETUP DIAGNOSTICS ? ? 
SETUP "SIM-OPTIONS" ? ; "ENG_MOLE" ; ? SETUP "UNITS-SET" METCBAR ? \ 
DESCRIPTION DESCRIPTION = "Metric Units with C, BAR, MMKCAL/HR, and CUM" \ \ 
MMLOCAL \ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 5 3 
4 3 3 3 3 1 3 3 3 4 3 7 3 3 3 1 1 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 3 3 
3 3 3 4 3 3 3 3 3 3 3 3 3 4 5 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" METCKGCM ? \ 
DESCRIPTION DESCRIPTION = "Metric Units with C, KG/SQCM, MMKCAL/HR, and CUM" 
\ \ MMLOCAL \ \ UNITSET BASESET = MET ( 3 3 3 3 3 3 3 3 3 3 3 7 7 3 3 5 3 3 3 
8 3 4 3 3 3 3 1 3 3 3 4 3 7 3 3 3 3 3 4 4 3 3 3 3 3 3 3 3 3 3 3 3 5 3 3 3 3 3 
3 3 3 3 3 4 3 3 3 3 3 3 3 3 3 4 8 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 
3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 3 ) \ ? SETUP "UNITS-SET" "SI-CBAR" ? 
\ DESCRIPTION DESCRIPTION = "International System Units with C, BAR, and /HR" 
\ \ MMLOCAL \ \ UNITSET BASESET = SI ( 1 1 1 1 1 1 1 1 1 3 3 7 1 1 1 1 1 1 1 
5 1 4 1 1 1 1 1 1 1 1 4 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 4 5 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 
1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 1 ) \ ? SETUP "ACCOUNT-INFO" ? \ 
ACCOUNT USER-NAME = "FLASH" \ ? SETUP "RUN-CONTROL" ? ? SETUP DESCRIPTION ? \ 
DESCRIP DESCRIP = ( "General Simulation with English Units :" 
"F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr." " " "Property Method: None" " " 
"Flow basis for input: Mole" " " "Stream report composition: Mole flow" ) \ ? 
DATABANKS ? \ DATABANKS FILE-SYM-NAM = ( PURE11 AQUEOUS SOLIDS INORGANIC ) \ 
? COMPONENTS MAIN ? \ COMPONENTS CID = WT ANAME = H2O OUTNAME = WT TYPE = 
CONV DBNAME1 = "WATER" ANAME1 = "H2O" /  CID = ACT ANAME = C2H4O2-1 OUTNAME
 = ACT TYPE = CONV DBNAME1 = "ACETIC-ACID" ANAME1 = "C2H4O2-1" \ ? COMPONENTS 
"COMP-LIST" GLOBAL ? ? SOLVE ? ? FLOWSHEET GLOBAL ? \ BLOCK BLKID = FLASH 
BLKTYPE = FLASH2 IN = ( FEED M0-1 ) OUT = ( V M0-1 L M1-2 ) \ \ "DEF-STREAM" 
SCLASS = CONVEN \ ? PROPERTIES MAIN ? \ GPROPERTIES GBASEOPSET = IDEAL 
GOPSETNAME = IDEAL PARCON = -2 \ ? PROPERTIES "OPTION-SETS" IDEAL ? \ PARAM 
BASE = IDEAL \ ? PROPERTIES "OPTION-SETS" NRTL ? \ PARAM BASE = NRTL \ ? 
PROPERTIES "OPTION-SETS" "NRTL-HOC" ? \ PARAM BASE = "NRTL-HOC" \ ? 
PROPERTIES "MOLEC-STRUCT" ACT ? ? PROPERTIES "MOLEC-STRUCT" WT ? ? PROPERTIES 
PARAMETERS BINARY SCALAR "HOCETA-1" ? ; "MET_MOLE" ; \ PROP-LIST PARAMNAME = 
HOCETA SETNO = 1 BDBANK = ( "EOS-LIT" ) \ \ BPVAL PARAMNAME2 = HOCETA CID1 = 
WT CID2 = WT VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = WT CID2 = 
ACT VALUE = EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = ACT CID2 = WT VALUE 
= EOS-LIT \ \ BPVAL PARAMNAME2 = HOCETA CID1 = ACT CID2 = ACT VALUE = EOS-LIT 
\ ? PROPERTIES PARAMETERS BINARY SCALAR "RKTKIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = RKTKIJ SETNO = 1 UNITROW = 0 \ ? PROPERTIES PARAMETERS 
BINARY "T-DEPENDENT" "ANDKIJ-1" ? ; "ENG_MOLE" ; \ PROP-LIST PARAMNAME = 
ANDKIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = F NEL = 2 \ ? 
PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "ANDMIJ-1" ? ; "ENG_MOLE" ; \ 
PROP-LIST PARAMNAME = ANDMIJ SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL
 = F NEL = 2 \ ? PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "HENRY-1" ? ; 
"MET_MOLE" ; \ PROP-LIST PARAMNAME = HENRY SETNO = 1 UNITROW = 20 UNITLABEL
 = atm TUNITROW = 22 TUNITLABEL = K BDBANK = ( BINARY HENRY ) NEL = 6 \ ? 
PROPERTIES PARAMETERS BINARY "T-DEPENDENT" "NRTL-1" ? ; "MET_MOLE" ; \ 
PROP-LIST PARAMNAME = NRTL SETNO = 1 UNITROW = 0 TUNITROW = 22 TUNITLABEL = K 
BDBANK = ( "VLE-HOC" "LLE-ASPEN" ) NEL = 12 \ \ BPVAL PARAMNAME2 = NRTL CID1
 = WT CID2 = ACT UNITROW2 = 0 TUNITROW2 = 22 TUNITLABEL2 = K VAL1 = VLE-HOC 
VAL2 = VLE-HOC VAL3 = VLE-HOC VAL4 = VLE-HOC VAL5 = VLE-HOC VAL6 = VLE-HOC 
VAL7 = VLE-HOC VAL8 = VLE-HOC VAL9 = VLE-HOC VAL10 = VLE-HOC VAL11 = VLE-HOC 
VAL12 = VLE-HOC \ ? "PROP-SET" MAIN HXDESIGN ? ; "SI_MOLE" ; \ P1 ID = 
MASSVFRA \ \ P1 ID = MASSFLMX UNITS = ( "kg/sec" ) \ \ P1 ID = HMX UNITS = ( 
"J/kg" ) \ \ P1 ID = RHOMX UNITS = ( "kg/cum" ) \ \ P1 ID = CPMX UNITS = ( 
"J/kg-K" ) \ \ P1 ID = PCMX UNITS = ( "N/sqm" ) \ \ P1 ID = MUMX UNITS = ( 
"N-sec/sqm" ) \ \ P1 ID = KMX UNITS = ( "Watt/m-K" ) \ \ P1 ID = SIGMAMX 
UNITS = ( "N/m" ) \ \ P1 ID = MWMX \ \ P2 PHASE = ( T V L ) \ \ DESCRIPTION 
DESCRIPTION = "Thermal and Transport, for heat exchanger design" \ ? "PROP-SET" 
MAIN THERMAL ? ; "ENG_MOLE" ; \ P1 ID = HMX UNITS = ( "Btu/lb" ) \ \ P1 ID = 
CPMX UNITS = ( "Btu/lb-R" ) \ \ P1 ID = KMX \ \ P2 SUBSTREAM = MIXED PHASE = 
( V L ) \ \ DESCRIPTION DESCRIPTION = 
"Enthalpy, heat capacity, and thermal conductivity" \ ? "PROP-SET" MAIN 
TXPORT ? ; "ENG_MOLE" ; \ P1 ID = RHOMX UNITS = ( "lb/cuft" ) \ \ P1 ID = 
MUMX \ \ P1 ID = SIGMAMX \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ 
DESCRIPTION DESCRIPTION = "Density, viscosity, and surface tension" \ ? 
"PROP-SET" MAIN VLE ? ; "ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 
ID = PL \ \ P2 SUBSTREAM = MIXED PHASE = ( V L ) \ \ DESCRIPTION DESCRIPTION
 = "Fugacity, activity, and vapor pressure" \ ? "PROP-SET" MAIN VLLE ? ; 
"ENG_MOLE" ; \ P1 ID = PHIMX \ \ P1 ID = GAMMA \ \ P1 ID = PL \ \ P2 
SUBSTREAM = MIXED PHASE = ( V L1 L2 ) \ \ DESCRIPTION DESCRIPTION = 
"Fugacity, activity, and vapor pressure" \ ? "STREAM-NAMES" ? ? STREAM 
MATERIAL FEED ? ; "MET_MOLE" ; \ SUBSTREAM SSID = MIXED TEMP = 105. <22> <4> 
PRES = 1. <20> <3> BASIS = "MOLE-FRAC" TOTFLOW = 100. <-89> <3> TOTAL = 1. 
<-89> <0> JUNK = 2 \ \ MOLE-FLOW SSID1 = MIXED CID = WT FLOW = 0.5 <-4> <0> 
/  SSID1 = MIXED CID = ACT FLOW = 0.5 <-4> <0> \ ? BLOCK FLASH2 FLASH ? ; 
"MET_MOLE" ; ; "V-DRUM1" ; \ PARAM TEMP = 105. <22> <4> PRES = 1. <20> <3> \ 
? "EO-CONV-OPTI" ? \ DMO-PARAMS MODE = DEFAULT \ \ DMO-PARAMS MODE = 
SIMULATION \ \ DMO-PARAMS MODE = "PARAMETER-ESTIMATION" \ \ DMO-PARAMS MODE
 = RECONCILIATION \ \ DMO-PARAMS MODE = OPTIMIZATION \ \ LSSQP-PARAMS MODE-L
 = DEFAULT \ \ LSSQP-PARAMS MODE-L = SIMULATION \ \ LSSQP-PARAMS MODE-L = 
"PARAMETER-ESTIMATION" \ \ LSSQP-PARAMS MODE-L = RECONCILIATION \ \ 
LSSQP-PARAMS MODE-L = OPTIMIZATION \ ? REPORT REPORT ? ? REPORT "BLOCK-REPORT" 
? ? REPORT "STREAM-REPOR" ? \ OPTIONS MOLEFRAC = MOLEFRAC \ ? REPORT 
"FLOWSHEET-RE" ? ? REPORT "PROPERTY-REP" ? ? REPORT "ADA-REPORT" ? ? REPORT 
"BATCH-OPERAT" ? ; "MET_MOLE" ; 

 GRAPHICS_BACKUP
PFS V 5.00
$CONFIG
paramdata ENRTL-RK
paramdata VLE-IG
paramdata VLE-RK
paramdata VLE-HOC
paramdata LLE-LIT
paramdata LLE-ASPEN
paramdata VLE-LIT
paramdata BINARY
paramdata EOS-LIT
paramdata HENRY
purebank PURE11
purebank AQUEOUS
purebank SOLIDS
purebank INORGANIC
regdbank 1
ftn_check 1
autoblockid 1
autostreamid 1
showblockid 1
showstreamid 1
autoplacement 1
grid 2
gridresolution 0.100000
scale 0
streamprefix 
blockprefix B
labelscale 1.000000
qwformat %.0f
tempformat %.0f
presformat %.0f
flowformat %.0f
strmqwformat %.0f
vflowformat %.0f
mflowformat %.0f
vfracformat %.2f
pseudobatch 0
partial 1
animation 1
runanyway 0
tooldrawvisible 0
browserheight 6465
browserwidth 10335
browsertreewidth 2445
polyplusenabled 1
dynaplusenabled 1
bfracenabled 1
rtfenabled 1
pinchenabled 0
linklimit 500
material_color 0
material_style 983041
material_width 1
heat_color 0
heat_style 983042
heat_width 1
heat_termid Q
work_color 0
work_style 983043
work_width 1
work_termid W
connections_color 9
connections_style 983044
connections_width 1
measurements_color 4
measurements_style 983044
measurements_width 1
displayeoconn 0
displayeomeas 1
displayeomeastype 2
showeoviews 0
eoautosave 1
#
#
PFSVData {A0DFFFE6-908E-11CE-A964-0000C08C668E}
# of PFS Objects = 5
SIZE -0.286957 5.08323 -3.11553 1.53727
BLOCK
ID: FLASH
Version: 1
ICON: "V-DRUM1"
Flag 0
Section GLOBAL
At 3.095030 -0.696894
Label At -0.280777 0.460742
Scale 3.900000 Modifier 0
STREAM
ID: FEED
Version: 1
Flag 0
TYPE 0 TERMINAL 1
At -0.204970 -0.696894
Label At 1.072472 0.000000
ROUTE 0 0
$ $ 0.0 0.0
ROUTE 1 0
r r -0.204970 -0.696894
x x 0.950000 -0.696894
y y 0.950000 -0.700367
x x 1.921688 -0.700367
t l 2.121688 -0.700367
$ C 1.000000 0.0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: V
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At 4.693788 1.445031
Label At -0.799898 0.000000
ROUTE 0 0
r l 4.693788 1.445031
x y 3.093991 1.445031
y 0 3.093991 1.062263
t u 3.093991 0.862263
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
STREAM
ID: L
Version: 1
Flag 0
TYPE 0 TERMINAL 2
At 5.001241 -3.043788
Label At -0.953625 0.000000
ROUTE 0 0
r l 5.001241 -3.043788
x y 3.093991 -3.043788
y 0 3.093991 -2.449106
t d 3.093991 -2.249106
$ C 1.000000 0.0
$ $ 0.0 0.0
ROUTE 1 0
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 1
$ $ 0.0 0.0
ROUTE 1 1
$ $ 0.0 0.0
At 0.000000 0.000000
Label At 0.000000 0.000000
ROUTE 0 2
$ $ 0.0 0.0
ROUTE 1 2
$ $ 0.0 0.0
LEGEND
Version: 2
Dim: -3.70994 -3.2 -3.09503 -3.3205
Size: 0.0204969
Font: 1 0 =Times New Roman
# of PFS Objects = 0
VIEWPORT -7.809317 17.975775 3.300000 -5.759627
LAYOUT
TableFormat 1
Pages 1 1 1 1
PAGESETUP
PAPERSIZE 1
PAPERSOURCE 1
ORIENTATION 1
PRINTPAGENO 1 1
LEFTMARGIN 0.5"
RIGHTMARGIN 0.5"
TOPMARGIN 0.5"
BOTTOMMARGIN 0.5"
PFDFLAG 255 255
PFDMODE 0
SCALE 0.020497

$_SUMMARY_FILE
 MMSUMMARY11.1                                                                  
 IDSET RUNID (PROPERTIES) (114 *5)                                              
 IDSET IT (PROPERTIES) (117 *6 119 *6 115 *1)                                   
 LSET RUNID (%RUNID)                                                            
 LSET IT (%IT)                                                                  
 IDSET VERS (PROPERTIES) (345 *6 346 *6 347 *6 348 *6 355 *6)                   
 LSET VERS (%VERS)                                                              
 DSET RUN-STATUS VERS @VERS ( "11.1" "WIN32" "TEAM_EAT" "FaraDars" "FARADARS_PC"
 )                                                                              
 DSET RUN-STATUS IT @IT ( "DECEMBER 8, 2016    9:23:11 A.M." "_0523esh.inm" 0)  
 DSET RUN-STATUS CURRENCY @CURRENCY ( "$" )                                     
 IDSET ID_NCC (COMPONENTS) (WT ACT)                                             
 IDSET ALIAS (COMPONENTS) (1 *6)                                                
 LSET ALIAS ( %ID_NCC & %ALIAS)                                                 
 DSET RUN-STATUS RUNID @RUNID ("_0523esh")                                      
 DSET RUN-STATUS RUNID @RUNID ("_0523esh")                                      
 IDSET STATUS (PROPERTIES) (125 *1 126 *1 127 *1 128 *1 129 *1 130 *1)          
 LSET STATUS (%STATUS)                                                          
 IDSET PPSTAT (PROPERTIES) (272 *1)                                             
 LSET PPSTAT (%PPSTAT)                                                          
 DSET RUN-STATUS PPSTAT @PPSTAT (2)                                             
 IDSET IDRXBAL0 (PROPERTIES) ( 73 *2 <11> 74 *2 75 *2 <10> 76 *2 77 *2 <13> 78  
 *2)                                                                            
 IDSET ID_RXBAL (PROPERTIES) ( 73 *2 <11> 358 *2 <11> 359 *2 <11> 74 *2 75 *2   
 <10> 360 *2 <10> 361 *2 <10> 76 *2 362 *2 <10> 363 *2 <10> 364 *2 <10> 365 *2  
 366 *2 <11> 367 *2 <11> 368 *2 <11> 369 *2 370 *2 <10> 371 *2 <10> 372 *2 <10> 
 373 *2 77 *2 <13> 374 *2 <13> 375 *2 <13> 78 *2)                               
 IDSET ID_MOLE (PROPERTIES) ( 79 *2 <11> 80 *2)                                 
 LSET FLWBAL ( %ID_NCC & %ID_MOLE %IDRXBAL0)                                    
 IDSET ID_XY (PROPERTIES) (43 *2 36 *2 39 *2 40 *2)                             
 IDSET ID_XX (PROPERTIES) (43 *2 37 *2 38 *2 40 *2)                             
 IDSET ID_XXY (PROPERTIES) (43 *2 37 *2 38 *2 39 *2 41 *2 42 *2)                
 LSET VLE ( %ID_XY & %ID_NCC)                                                   
 LSET LLE ( %ID_XX & %ID_NCC)                                                   
 LSET VLE3 ( %ID_XXY & %ID_NCC)                                                 
 IDSET ID_KODE (PROPERTIES) (44 *1)                                             
 IDSET BLKIN (BLKIN) (STREAMID ?)                                               
 LSET BLKIN (%BLKIN)                                                            
 IDSET BLKOUT (BLKOUT) (STREAMID ?)                                             
 LSET BLKOUT (%BLKOUT)                                                          
 IDSET TYPIN (TYPIN) (STREAMID ?)                                               
 LSET TYPIN (%TYPIN)                                                            
 IDSET TYPOUT (TYPOUT) (STREAMID ?)                                             
 LSET TYPOUT (%TYPOUT)                                                          
 IDSET PORT_NO (PROPERTIES) (236 *1 237 *1 238 *1)                              
 IDSET IDS_0 (SUBSTREAM) ($TOTAL)                                               
 IDSET IDS_1 (SUBSTREAM) (MIXED)                                                
 IDSET BLKSTAT (PROPERTIES) (120 *1 121 *1)                                     
 IDSET BLKMSG (PROPERTIES) (122 *6)                                             
 LSET BLKSTAT (%BLKSTAT)                                                        
 LSET BLKMSG (%BLKMSG)                                                          
 IDSET DESC (PROPERTIES) (113 *6)                                               
 LSET DESC (%DESC)                                                              
 IDSET IDPH_V (PHASE) (VAPOR)                                                   
 IDSET IDPH_L (PHASE) (LIQUID)                                                  
 IDSET IDPH_S (PHASE) (SOLID)                                                   
 IDSET IDPH_L1 (PHASE) (LIQUID_1)                                               
 IDSET IDPH_T (PHASE) (TOTAL)                                                   
 IDSET IDPH_L2 (PHASE) (LIQUID_2)                                               
 IDSET IDWET (BASIS) (WET)                                                      
 IDSET IDDRY (BASIS) (DRY)                                                      
 IDSET SP (PROPERTIES) (118 *6)                                                 
 LSET SP (%SP)                                                                  
 IDSET SPSTAT (SPSTAT) (116 *1)                                                 
 LSET SPSTAT ( %SPSTAT)                                                         
 IDSET IDERR (PROPERTIES) (131 *1)                                              
 DSET RUN-STATUS SP @SP ( "DECEMBER 8, 2016 9:23:11 A.M." )                     
 IDSET TITLE (PROPERTIES) (113 *6)                                              
 LSET TITLE (%TITLE)                                                            
 DSET RUN-STATUS TITLE @TITLE ( "FLASH" )                                       
 IDSET ACCOUNT (PROPERTIES) (222 *5 347 *5 355 *6 348 *6)                       
 LSET ACCOUNT (%ACCOUNT)                                                        
 DSET RUN-STATUS ACCOUNT @ACCOUNT (* * * "FLASH" )                              
 IDSET FOR (PROPERTIES) (737 *1)                                                
 LSET FOR (%FOR)                                                                
 IDSET FORSTAT (PROPERTIES) (738 *1)                                            
 LSET FORSTAT (%FORSTAT)                                                        
 IDSET MW (PROPERTIES) (269 *2)                                                 
 LSET MW (%MW & %ID_NCC)                                                        
 DSET MW MW @MW (1.80152800D+01 6.00525600D+01)                                 
 IDSET VST (PROPERTIES) (270 *2 <43> )                                          
 LSET VST (%VST & %ID_NCC)                                                      
 DSET VST VST @VST (1.80500000D+01 <3> 5.76314000D+01 <3> )                     
 IDSET TB (PROPERTIES) (271 *2 <22> )                                           
 LSET TB (%TB & %ID_NCC)                                                        
 DSET TB TB @TB (3.73150000D+02 <1> 3.91050000D+02 <1> )                        
 IDSET ISODES (PROPERTIES) (123 *5 124 *5 132 *5)                               
 IDSET ID_WORK (PROPERTIES) (112 *2 <19> )                                      
 LSET L_WORK (%ISODES %ID_WORK)                                                 
 IDSET ID_HEAT (PROPERTIES) (1 *2 <13> 815 *2 <22> 816 *2 <22> )                
 LSET L_HEAT (%ISODES %ID_HEAT)                                                 
 IDSET ID_LTVC (PROPERTIES) (817 *2 <22> )                                      
 IDSET ID_LQVC (PROPERTIES) (818 *2 <13> )                                      
 IDSET ID_TPQV (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 3 *2)         
 IDSET ID_QTP (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 3 *2)               
 IDSET TOTAL (PROPERTIES) (524 *2 <10> 525 *2 <10> 526 *2 <10> )                
 IDSET ENERGY (PROPERTIES) (504 *2 <13> 505 *2 <13> 506 *2 <13> 1 *2 <13> )     
 IDSET TOTAX (PROPERTIES) (524 *2 <18> 525 *2 <18> 526 *2 <18> )                
 IDSET ENERGX (PROPERTIES) (504 *2 <5> 505 *2 <5> 506 *2 <5> 1 *2 <5> )         
 LSET BPSBAL3 ( %TOTAL %ENERGY)                                                 
 LSET BPBATCH ( %TOTAX %ENERGX)                                                 
 DSET RUN-STATUS FORSTAT @FORSTAT (2)                                           
 DSET FLWBAL @FLWBAL (0.D0 <3> 0.D0 <3> 0.D0 0.D0 0.D0 <3> 0.D0 0.D0 <3> 0.D0   
 0.D0 <3> 0.D0)                                                                 
 DSET ALIAS @ALIAS ( "H2O" "C2H4O2-1" )                                         
 IDSET ID_15 (NPOINT) (#2)                                                      
 IDSET ID_16 (PROPERTIES) (339 *6 132 *5 1196 *6 1197 *6 1198 *6)               
 LSET L_6 (%ID_16 & %ID_15)                                                     
 DSET COMPONENTS MAIN COMPS @L_6 ("WT" C "H2O" "H2O" "WT" "ACT" C "C2H4O2-1"    
 "C2H4O2-1" "ACT" )                                                             
 IDSET ID_17 (PROPERTIES) (1052 *2 <13> )                                       
 IDSET ID_18 (PROPERTIES) (298 *2 <75> )                                        
 LSET L_7 (%ID_RXBAL %ID_TPQV %ID_17 %ID_KODE %ID_18)                           
 DSET BLOCK FLASH2 FLASH BLKSTAT @BLKSTAT (0 0)                                 
 DSET BLOCK FLASH2 FLASH COMPSTAT @L1 (0)                                       
 DSET BLOCK FLASH2 FLASH BLKIN @BLKIN (1 FEED)                                  
 DSET BLOCK FLASH2 FLASH TYPIN @TYPIN (1 MATERIAL)                              
 DSET BLOCK FLASH2 FLASH BLKOUT @BLKOUT (2 V L)                                 
 DSET BLOCK FLASH2 FLASH TYPOUT @TYPOUT (2 MATERIAL MATERIAL)                   
 DSET BLOCK FLASH2 FLASH RES_Q @L_7 (1.00000000D+02 <3> 1.00000000D+02 <3> 0.D0 
 <3> 0.D0 3.90339200D+03 <3> 3.90339200D+03 <3> * <3> 0.D0 * <3> * <3> * <3> *  
 1.00000000D+02 <3> 1.00000000D+02 <3> 0.D0 <3> 0.D0 3.90339200D+03 <3>         
 3.90339200D+03 <3> * <3> 0.D0 -2.42399453D+06 <3> -2.42399453D+06 <3> * <3>    
 0.D0 0.D0 <3> 3.78150000D+02 <1> 1.00000000D+00 <3> 0.D0 1.00000000D+00 0.D0   
 <3> 11 0.D0 <3> )                                                              
 IDSET ID_19 (PROPERTIES) (1 *2 <13> 31 *2 <22> 32 *2 <20> 2 *2 7001 *2 <22>    
 7002 *2 <20> 899 *2 )                                                          
 LSET L_8 ( %ID_19 )                                                            
 DSET BLOCK FLASH2 FLASH FLS2_INR @L_8 ( * <1> 3.78150000D+02 <1>               
 1.01325000D+05 <1> * * <1> * <1> 0.D0 )                                        
 DSET BLOCK FLASH2 FLASH VLE @VLE ( 5.00000000D-01 5.00000000D-01               
 6.43340179D-01 1.19122669D+00 5.00000000D-01 5.00000000D-01 3.56659821D-01     
 6.60401312D-01 )                                                               
 IDSET ID_20 (PROPERTIES) (7001 *2 7002 *2 8103 *2 8101 *2 204 *2 7003 *2 )     
 LSET L_9 ( %ID_20 )                                                            
 IDSET ID_21 (PROPERTIES) (253 *2)                                              
 IDSET ID_22 (PROPERTIES) (253 *2 <11> )                                        
 IDSET ID_23 (PROPERTIES) (253 *2 <12> )                                        
 IDSET ID_24 (PROPERTIES) (253 *2 <17> )                                        
 IDSET ID_25 (PROPERTIES) (253 *2 <27> )                                        
 IDSET ID_26 (PROPERTIES) (253 *2 <59> )                                        
 IDSET ID_27 (PROPERTIES) (8101 *2 <11> 8002 *2 )                               
 IDSET ID_28 (PROPERTIES) (8001 *2 <11> 8003 *2 <10> 8010 *2 <12> 7001 *2 <22>  
 7002 *2 <20> 7003 *2 7004 *2 7006 *2 2002 *2 <39> 2002 *2 <40> 2002 *2 <13>    
 2003 *2 <41> 2003 *2 <42> 11006 *2 <37> 11006 *2 <38> 11007 *2 8005 *2 <12> )  
 LSET L_10 ( %ISODES (( %ID_NCC & %ID_27 %ID_28) & %IDS_1) )                    
 DSET STREAM MATERIAL FEED STR_MAIN @L_10 (* FLASH LIQUID 5.00000000D+01 <3>    
 5.00000000D+01 <3> 5.00000000D-01 5.00000000D-01 1.00000000D+02 <3>            
 3.90339200D+03 <3> 7.17789814D+01 <3> 3.78150000D+02 <1> 1.00000000D+00 <3>    
 0.D0 1.00000000D+00 0.D0 -8.72638025D+04 <3> -2.23558901D+03 <3>               
 -2.42399453D+06 <3> -4.43932609D+01 <3> -1.13729958D+00 <3> 2.32194246D-02 <3> 
 9.06345162D-01 <3> 3.90339200D+01 6.30678326D+01 <3> )                         
 DSET STREAM MATERIAL FEED RES_STR @L_9 (3.78150000D+02 <1> 1.00000000D+00 <3>  
 3.90339200D+03 <3> 7.17789814D+01 <3> 1.00000000D+02 <3> 0.D0 )                
 DSET STREAM MATERIAL L STR_MAIN @L_10 (FLASH * LIQUID 5.00000000D+01 <3>       
 5.00000000D+01 <3> 5.00000000D-01 5.00000000D-01 1.00000000D+02 <3>            
 3.90339200D+03 <3> 7.17789814D+01 <3> 3.78150000D+02 <1> 1.00000000D+00 <3>    
 0.D0 1.00000000D+00 0.D0 -8.72638025D+04 <3> -2.23558901D+03 <3>               
 -2.42399453D+06 <3> -4.43932609D+01 <3> -1.13729958D+00 <3> 2.32194246D-02 <3> 
 9.06345162D-01 <3> 3.90339200D+01 6.30678326D+01 <3> )                         
 DSET STREAM MATERIAL L RES_STR @L_9 (3.78150000D+02 <1> 1.00000000D+00 <3>     
 3.90339200D+03 <3> 7.17789814D+01 <3> 1.00000000D+02 <3> 0.D0 )                
 DSET STREAM MATERIAL V STR_MAIN @L_10 (FLASH * MISSING 0.D0 <3> 0.D0 <3> 0.D0  
 0.D0 0.D0 <3> 0.D0 <3> 0.D0 <3> * <1> 1.00000000D+00 <3> * * * * <3> * <3> *   
 <3> * <3> * <3> * <3> * <3> * 0.D0 <3> )                                       
 DSET STREAM MATERIAL V RES_STR @L_9 (* <1> 1.00000000D+00 <3> 0.D0 <3> 0.D0 <3>
 0.D0 <3> * )                                                                   
 IDSET RSTAT (PROPERTIES) (739 *1)                                              
 LSET RSTAT ( %RSTAT)                                                           
 DSET RUN-STATUS RPTSTAT @RSTAT (0)                                             
 DSET RUN-STATUS OLDSTAT @STATUS ( 0 2 2 2 0 0 )                                
 DSET RUN-STATUS STATUS @STATUS ( 8 * * * * * )                                 
 DSET RUN-STATUS COMPSTAT @L_1 (0)                                              
 IDSET ID_29 (NPOINT) ( #5)                                                     
 IDSET ID_30 (PROPERTIES) (747 *6)                                              
 LSET L_11 ( %ID_29 & %ID_30)                                                   
 DSET RUN-STATUS ERRTXT @L_11 (                                                 
 "The following messages were issued during Input Translation:"                 
 ""                                                                             
 "   INFORMATION"                                                               
 "   BINARY PARAMETERS HOCETA (DATA SET 1) FOR MODEL ESHOC"                     
 "   ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESHOC"                         
 )                                                                              
 IDSET TSTAT (PROPERTIES) (741 *1)                                              
 LSET TSTAT ( %TSTAT)                                                           
 DSET RUN-STATUS TOTSTAT @TSTAT (0)                                             
 DSET SPSTAT @SPSTAT (0)                                                        
