


                                     +
                                   + + +
                                   + + +
                                   + + +
                             +     + + +     +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                     +     + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                     +       +     + + +     +       +
                                   + + +
                                   + + +
                                   + + +
 ASPENTECH                         + + +
                                   + + +
 FLOWSHEET SIMULATION              + + +
 FOR THE PROCESS INDUSTRIES        + + +
                                     +


                                                                        TM
 AAAAA   SSSSS   PPPPP   EEEEE   NN    N   PPPPP   L       U   U   SSSSS
 A   A   S       P   P   E       N N   N   P   P   L       U   U   S    
 AAAAA   SSSSS   PPPPP   EEEEE   N   N N   PPPPP   L       U   U   SSSSS
 A   A       S   P       E       N    NN   P       L       U   U       S
 A   A   SSSSS   P       EEEEE   N     N   P       LLLLL   UUUUU   SSSSS

 ASPEN PLUS IS A TRADEMARK OF           HOTLINE:
 ASPEN TECHNOLOGY, INC.                 U.S.A. 888/996-7001
 TEN CANAL PARK                         EUROPE (32) 2/724-0100
 CAMBRIDGE, MASSACHUSETTS 02141                             
 617/949-1000

 PLATFORM: WIN32                                         NOVEMBER 14, 2016   
 VERSION: 11.1   Build 192                               MONDAY      
 INSTALLATION: TEAM_EAT                                  10:05:15 A.M.       

 THIS COPY OF ASPEN PLUS LICENSED TO                                 


      ASPEN PLUS (R) IS A PROPRIETARY PRODUCT OF ASPEN TECHNOLOGY, INC.
      (ASPENTECH), AND MAY BE USED ONLY UNDER AGREEMENT WITH ASPENTECH.
      RESTRICTED RIGHTS LEGEND:  USE, REPRODUCTION, OR DISCLOSURE BY THE
      U.S. GOVERNMENT IS SUBJECT TO RESTRICTIONS SET FORTH IN 
      (i) FAR 52.227-14, Alt. III, (ii) FAR 52.227-19, (iii) DFARS 
      252.227-7013(c)(1)(ii), or (iv) THE ACCOMPANYING LICENSE AGREEMENT,
      AS APPLICABLE. FOR PURPOSES OF THE FAR, THIS SOFTWARE SHALL BE DEEMED
      TO BE "UNPUBLISHED" AND LICENSED WITH DISCLOSURE PROHIBITIONS.
      CONTRACTOR/SUBCONTRACTOR: ASPEN TECHNOLOGY, INC. TEN CANAL PARK,
      CAMBRIDGE, MA 02141.
 *** INPUT SUMMARY ***

 >>CURRENT RUN

   ORIGINAL RUN                           NOVEMBER 14, 2016   
   10:05:15 A.M.                          MONDAY      
   INPUT FILE: _0154ynx.inm                                                                    
   RUN ID : _0154ynx
     1    ;
     2    ;Input file created by Aspen Plus Rel. 11.1 at 10:05:14 Mon Nov 14, 2016
     3    ;Directory E:\Aspen Plus\Education  Runid reactor 2
     4    ;
     5
     6
     7
     8    TITLE 'reaction 3'
     9
    10    IN-UNITS ENG
    11
    12    DEF-STREAMS CONVEN ALL
    13
    14    ACCOUNT-INFO ACCOUNT=A PROJECT-ID=A PROJECT-NAME="A"  &
    15            USER-NAME="A"
    16
    17    DESCRIPTION "
    18        General Simulation with English Units :
    19        F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr.
    20
    21        Property Method: None
    22
    23        Flow basis for input: Mole
    24
    25        Stream report composition: Mole flow
    26        "
    27
    28    DATABANKS PURE11  / AQUEOUS  / SOLIDS  / INORGANIC  /  &
    29            NOASPENPCD
    30
    31    PROP-SOURCES PURE11  / AQUEOUS  / SOLIDS  / INORGANIC
    32
    33    COMPONENTS
    34        AN C6H7N-1 /
    35        H2 H2 /
    36        CHA C6H13N-D1
    37
    38    FLOWSHEET
    39        BLOCK RCSTR IN=AN H2 OUT=PRODUCT
    40
    41    PROPERTIES PENG-ROB
    42        PROPERTIES MXBONNEL / NRTL / SRK / UNIFAC
    43
    44    PROP-DATA NRTL-1
    45        IN-UNITS ENG
    46        PROP-LIST NRTL
    47        BPVAL AN CHA 3.545800000 -1859.934945 .3000000000 0.0 0.0  &
    48            0.0 159.6020027 358.6100011
    49        BPVAL CHA AN -2.402200000 1244.103470 .3000000000 0.0 0.0  &
    50            0.0 159.6020027 358.6100011
    51
    52    STREAM AN
    53        SUBSTREAM MIXED TEMP=100. PRES=650.
    54        MOLE-FLOW AN 100.
    55
    56    STREAM H2
    57        SUBSTREAM MIXED TEMP=100. PRES=650.
    58        MOLE-FLOW H2 400.
    59
    60    BLOCK RCSTR RCSTR
    61        PARAM VOL=1200. TEMP=250. PRES=595. NPHASE=2 PHASE=L  &
    62            PHASE-VOL-FR=0.8
    63        BLOCK-OPTION FREE-WATER=NO
    64        REACTIONS RXN-IDS=R-1
    65
    66    EO-CONV-OPTI
    67
    68    STREAM-REPOR NOMOLEFLOW MOLEFRAC
    69
    70    REACTIONS R-1 POWERLAW
    71        REAC-DATA 1
    72        RATE-CON 1 PRE-EXP=1750. ACT-ENERGY=11111. <cal/mol>
    73        STOIC 1 MIXED AN -1. / H2 -3. / CHA 1.
    74        POWLAW-EXP 1 MIXED AN 1. / MIXED H2 1.
    75    ;
    76    ;
    77    ;
    78    ;
    79    ;
 *** INPUT TRANSLATOR MESSAGES ***


      INFORMATION                                              (ESBPLD.1)       
      BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD                    
      ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD                       
 
 

 PDF updated                                                                      TIME =      0.13

 *** CALCULATION TRACE ***

 REACTION 3                                                      

 *** FLOWSHEET ANALYSIS MESSAGES ***

 FLOWSHEET CONNECTIVITY BY STREAMS       

   STREAM     SOURCE     DEST           STREAM     SOURCE     DEST
   H2         ----       RCSTR          AN         ----       RCSTR   
   PRODUCT    RCSTR      ----                                         

 FLOWSHEET CONNECTIVITY BY BLOCKS        

   BLOCK        INLETS                         OUTLETS
   RCSTR        AN H2                          PRODUCT                     

      COMPUTATION ORDER FOR THE FLOWSHEET IS:
      RCSTR 

Calculations begin                                                              time      3.10


 SIMULATION CALCULATIONS BEGIN                                                    TIME =      3.10

      ENTHALPY CALCULATION FOR INLET STREAM AN OF BLOCK RCSTR                     TIME =      3.10
      KODE = 2  NTRIAL =   1  T =   310.93  P =  0.4482E+07  V =  0.0000E+00  Q =  0.0000E+00

      ENTHALPY CALCULATION FOR INLET STREAM H2 OF BLOCK RCSTR                     TIME =      3.10
      KODE = 2  NTRIAL =   0  T =   310.93  P =  0.4482E+07  V =   1.000      Q =  0.0000E+00

      UOS BLOCK RCSTR    MODEL: RCSTR                                             TIME =      3.10
      REACTOR DUTY = -0.13373E+07 VOLUME =   33.980     RES TIME =   1612.4    

 Report Writer entered                                                            Time =    204.56

 Results generated                                                                Time =    204.57

 Report Writer entered                                                            Time =    204.62

 Results generated                                                                Time =    204.63

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED
