


                                     +
                                   + + +
                                   + + +
                                   + + +
                             +     + + +     +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                           + + +   + + +   + + +
                     +     + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
           + + +   + + +   + + +   + + +   + + +   + + +   + + +
             +     + + +   + + +   + + +   + + +   + + +     +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                   + + +   + + +   + + +   + + +   + + +
                     +       +     + + +     +       +
                                   + + +
                                   + + +
                                   + + +
 ASPENTECH                         + + +
                                   + + +
 FLOWSHEET SIMULATION              + + +
 FOR THE PROCESS INDUSTRIES        + + +
                                     +


                                                                        TM
 AAAAA   SSSSS   PPPPP   EEEEE   NN    N   PPPPP   L       U   U   SSSSS
 A   A   S       P   P   E       N N   N   P   P   L       U   U   S    
 AAAAA   SSSSS   PPPPP   EEEEE   N   N N   PPPPP   L       U   U   SSSSS
 A   A       S   P       E       N    NN   P       L       U   U       S
 A   A   SSSSS   P       EEEEE   N     N   P       LLLLL   UUUUU   SSSSS

 ASPEN PLUS IS A TRADEMARK OF           HOTLINE:
 ASPEN TECHNOLOGY, INC.                 U.S.A. 888/996-7001
 TEN CANAL PARK                         EUROPE (32) 2/724-0100
 CAMBRIDGE, MASSACHUSETTS 02141                             
 617/949-1000

 PLATFORM: WIN32                                         NOVEMBER 27, 2016   
 VERSION: 11.1   Build 192                               SUNDAY      
 INSTALLATION: TEAM_EAT                                  4:46:35 P.M.        

 THIS COPY OF ASPEN PLUS LICENSED TO                                 


      ASPEN PLUS (R) IS A PROPRIETARY PRODUCT OF ASPEN TECHNOLOGY, INC.
      (ASPENTECH), AND MAY BE USED ONLY UNDER AGREEMENT WITH ASPENTECH.
      RESTRICTED RIGHTS LEGEND:  USE, REPRODUCTION, OR DISCLOSURE BY THE
      U.S. GOVERNMENT IS SUBJECT TO RESTRICTIONS SET FORTH IN 
      (i) FAR 52.227-14, Alt. III, (ii) FAR 52.227-19, (iii) DFARS 
      252.227-7013(c)(1)(ii), or (iv) THE ACCOMPANYING LICENSE AGREEMENT,
      AS APPLICABLE. FOR PURPOSES OF THE FAR, THIS SOFTWARE SHALL BE DEEMED
      TO BE "UNPUBLISHED" AND LICENSED WITH DISCLOSURE PROHIBITIONS.
      CONTRACTOR/SUBCONTRACTOR: ASPEN TECHNOLOGY, INC. TEN CANAL PARK,
      CAMBRIDGE, MA 02141.
 *** INPUT SUMMARY ***

 >>CURRENT RUN

   ORIGINAL RUN                           NOVEMBER 27, 2016   
   4:46:35 P.M.                           SUNDAY      
   INPUT FILE: _2136yqy.inm                                                                    
   RUN ID : _2136yqy
     1    ;
     2    ;Input file created by Aspen Plus Rel. 11.1 at 16:46:35 Sun Nov 27, 2016
     3    ;Directory D:\FaraDars.Org\T1173\FVCHE9506\FVCHE9506-S1\Files And Codes\SIM1  Runid simu1
     4    ;
     5
     6
     7
     8    TITLE 'simulation'
     9
    10    IN-UNITS MET
    11
    12    OUT-UNITS MET
    13
    14    DEF-STREAMS CONVEN ALL
    15
    16    ACCOUNT-INFO ACCOUNT=12 PROJECT-ID=123 PROJECT-NAME="ASA-1"  &
    17            USER-NAME="FLASH DRUM"
    18
    19    DESCRIPTION "
    20        General Simulation with English Units :
    21        F, psi, lb/hr, lbmol/hr, Btu/hr, cuft/hr.
    22
    23        Property Method: None
    24
    25        Flow basis for input: Mole
    26
    27        Stream report composition: Mole flow
    28        "
    29
    30    DATABANKS PURE11  / AQUEOUS  / SOLIDS  / INORGANIC  /  &
    31            NOASPENPCD
    32
    33    PROP-SOURCES PURE11  / AQUEOUS  / SOLIDS  / INORGANIC
    34
    35    COMPONENTS
    36        WT H2O /
    37        AC C3H6O-1 /
    38        MIBK C6H12O-2 /
    39        BUOH C4H10O-1 /
    40        NBAC C6H12O2-1 /
    41        ACT C2H4O2-1
    42
    43    FLOWSHEET
    44        BLOCK FLASH IN=FEED OUT=ACT WT
    45
    46    PROPERTIES NRTL
    47        PROPERTIES IDEAL / NRTL-HOC / PENG-ROB
    48
    49    PROP-DATA HOCETA-1
    50        IN-UNITS MET
    51        PROP-LIST HOCETA
    52        BPVAL WT WT 1.700000000
    53        BPVAL WT AC 1.000000000
    54        BPVAL WT MIBK 1.000000000
    55        BPVAL WT BUOH 1.550000000
    56        BPVAL WT NBAC 1.300000000
    57        BPVAL WT ACT 2.500000000
    58        BPVAL AC WT 1.000000000
    59        BPVAL AC AC .9000000000
    60        BPVAL AC MIBK .9000000000
    61        BPVAL AC BUOH 1.000000000
    62        BPVAL AC NBAC 1.100000000
    63        BPVAL AC ACT 1.800000000
    64        BPVAL MIBK WT 1.000000000
    65        BPVAL MIBK AC .9000000000
    66        BPVAL MIBK MIBK .9000000000
    67        BPVAL MIBK BUOH 1.000000000
    68        BPVAL MIBK NBAC 1.100000000
    69        BPVAL MIBK ACT 1.800000000
    70        BPVAL BUOH WT 1.550000000
    71        BPVAL BUOH AC 1.000000000
    72        BPVAL BUOH MIBK 1.000000000
    73        BPVAL BUOH BUOH 2.200000000
    74        BPVAL BUOH NBAC 1.300000000
    75        BPVAL BUOH ACT 2.500000000
    76        BPVAL NBAC WT 1.300000000
    77        BPVAL NBAC AC 1.100000000
    78        BPVAL NBAC MIBK 1.100000000
    79        BPVAL NBAC BUOH 1.300000000
    80        BPVAL NBAC NBAC .5300000000
    81        BPVAL NBAC ACT 2.000000000
    82        BPVAL ACT WT 2.500000000
    83        BPVAL ACT AC 1.800000000
    84        BPVAL ACT MIBK 1.800000000
    85        BPVAL ACT BUOH 2.500000000
    86        BPVAL ACT NBAC 2.000000000
    87        BPVAL ACT ACT 4.500000000
    88
    89    PROP-DATA NRTL-1
    90        IN-UNITS MET
    91        PROP-LIST NRTL
    92        BPVAL WT AC .0544000000 419.9716000 .3000000000 0.0 0.0  &
    93            0.0 293.1500000 368.2500000
    94        BPVAL AC WT 6.398100000 -1808.991000 .3000000000 0.0 0.0  &
    95            0.0 293.1500000 368.2500000
    96        BPVAL WT MIBK 9.162943000 -1248.744000 .2000000000 0.0 0.0  &
    97            0.0 273.1500000 389.1500000
    98        BPVAL MIBK WT -3.230481000 1208.877000 .2000000000 0.0 0.0  &
    99            0.0 273.1500000 389.1500000
   100        BPVAL AC MIBK -5.445200000 1833.522700 .3000000000 0.0 0.0  &
   101            0.0 298.1500000 383.2800000
   102        BPVAL MIBK AC 5.301300000 -1735.908200 .3000000000 0.0 0.0  &
   103            0.0 298.1500000 383.2800000
   104        BPVAL WT BUOH 13.11020000 -3338.953600 .3000000000 0.0 0.0  &
   105            0.0 292.3200000 390.7500000
   106        BPVAL BUOH WT -2.040500000 763.8692000 .3000000000 0.0 0.0  &
   107            0.0 292.3200000 390.7500000
   108        BPVAL AC BUOH -8.887500000 3077.281000 .3000000000 0.0 0.0  &
   109            0.0 331.2500000 388.1500000
   110        BPVAL BUOH AC 10.29790000 -3326.538100 .3000000000 0.0 0.0  &
   111            0.0 331.2500000 388.1500000
   112        BPVAL MIBK BUOH 0.0 -39.50760000 .3000000000 0.0 0.0 0.0  &
   113            386.7000000 390.8000000
   114        BPVAL BUOH MIBK 0.0 244.6096000 .3000000000 0.0 0.0 0.0  &
   115            386.7000000 390.8000000
   116        BPVAL WT NBAC 5.023900000 283.7672000 .3000000000 0.0 0.0  &
   117            0.0 317.7500000 399.2600000
   118        BPVAL NBAC WT -1.513200000 995.9705000 .3000000000 0.0 0.0  &
   119            0.0 317.7500000 399.2600000
   120        BPVAL AC NBAC 0.0 99.26540000 .3000000000 0.0 0.0 0.0  &
   121            331.2500000 380.4500000
   122        BPVAL NBAC AC 0.0 -12.90820000 .3000000000 0.0 0.0 0.0  &
   123            331.2500000 380.4500000
   124        BPVAL BUOH NBAC 1.760900000 -429.6393000 .3000000000 0.0  &
   125            0.0 0.0 323.8500000 399.3000000
   126        BPVAL NBAC BUOH -3.029600000 1122.138500 .3000000000 0.0  &
   127            0.0 0.0 323.8500000 399.3000000
   128
   129    STREAM FEED
   130        SUBSTREAM MIXED TEMP=105. <C> PRES=1. MOLE-FLOW=100.
   131        MOLE-FRAC WT 0.5 / ACT 0.5
   132
   133    BLOCK FLASH FLASH2
   134        PARAM TEMP=105. <C> PRES=1.
   135
   136    EO-CONV-OPTI
   137
   138    STREAM-REPOR MOLEFLOW MOLEFRAC MASSFRAC
   139
   140    PROPERTY-REP NOPARAM-PLUS
   141    ;
   142    ;
   143    ;
   144    ;
   145    ;
 *** INPUT TRANSLATOR MESSAGES ***


      INFORMATION                                              (ESBPLD.1)       
      BINARY PARAMETERS HOCETA (DATA SET 1) FOR MODEL ESHOC                     
      ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESHOC                         

      INFORMATION                                              (ESBPLD.1)       
      BINARY PARAMETERS PRKIJ (DATA SET 1) FOR MODEL ESPRSTD                    
      ARE RETRIEVED FROM SDF TABLE.  TABLE NAME = ESPRSTD                       
 
 

 PDF updated                                                                      TIME =      0.08

 *** CALCULATION TRACE ***

 SIMULATION                                                      

 *** FLOWSHEET ANALYSIS MESSAGES ***

 FLOWSHEET CONNECTIVITY BY STREAMS       

   STREAM     SOURCE     DEST           STREAM     SOURCE     DEST
   FEED       ----       FLASH          ACT        FLASH      ----    
   WT         FLASH      ----                                         

 FLOWSHEET CONNECTIVITY BY BLOCKS        

   BLOCK        INLETS                         OUTLETS
   FLASH        FEED                           ACT WT                      

      COMPUTATION ORDER FOR THE FLOWSHEET IS:
      FLASH 

Calculations begin                                                              time      0.12


 SIMULATION CALCULATIONS BEGIN                                                    TIME =      0.12

      ENTHALPY CALCULATION FOR INLET STREAM FEED OF BLOCK FLASH                   TIME =      0.12
      KODE = 2  NTRIAL =   1  T =   378.15  P =  0.1013E+06  V =  0.0000E+00  Q =  0.0000E+00

      UOS BLOCK FLASH    MODEL: FLASH2                                            TIME =      0.12
      KODE = 2  NTRIAL =   1  T =   378.15  P =  0.1013E+06  V =  0.0000E+00  Q =  0.0000E+00

 Report Writer entered                                                            Time =      0.21

 Results generated                                                                Time =      0.22

RUN SAVED



 NO ERRORS OR WARNINGS GENERATED
